[image: U:\UWTSD Logo.jpg]
Lab - Building an Ethernet Crossover Cable

Lab – Understanding Ethernet Cable Standards 
Topology
[image: ]
Addressing Table
	Device
	Interface
	IP Address
	Subnet Mask
	Default Gateway

	PC-A
	NIC
	192.168.10.1
	255.255.255.0
	N/A

	PC-B
	NIC
	192.168.10.2
	255.255.255.0
	N/A


Objectives
Part 1: Analyze Ethernet Cabling Standards and Pinouts
Part 2: Build an Ethernet Crossover Cable
Part 3: Test an Ethernet Crossover Cable
Background / Scenario
In this lab, you will build and terminate an Ethernet crossover cable and test it by connecting two PCs together and pinging between them. You will first analyze the Telecommunications Industry Association/Electronic Industries Association (TIA/EIA) 568-A and 568-B standards and how they apply to Ethernet cables. You will then construct an Ethernet crossover cable and test it. Finally, you will use the cable you just constructed to connect two PCs together and test it by pinging between them.
Note: With autosensing capabilities available on many devices, such as the Cisco 1941 Integrated Services Router (ISR) switch, you may see straight-through cables connecting like devices.
Required Resources
One length of cable, either Category 5 or 5e. Cable length should be 0.6 to 0.9m (2 to 3 ft.)
2 RJ-45 connectors
RJ-45 crimping tool
Wire cutter
Wire stripper
Ethernet cable tester (optional)
2 PCs (Windows 7 or 8)
Analyze Ethernet Cabling Standards and Pinouts
The TIA/EIA has specified unshielded twisted pair (UTP) cabling standards for use in LAN cabling environments. TIA/EIA 568-A and 568-B stipulates the commercial cabling standards for LAN installations; these are the standards most commonly used in LAN cabling for organizations and they determine which color wire is used on each pin.
With a crossover cable, the second and third pairs on the RJ-45 connector at one end of the cable are reversed at the other end, which reverses the send and receive pairs. The cable pinouts are the 568-A standard on one end and the 568-B standard on the other end. Crossover cables are normally used to connect hubs to hubs or switches to switches, but they can also be used to directly connect two hosts to create a simple network.
Reflection: 
Write a research report (Max word count 600) on Cat 5e and 6 Ethernet cable standards.  
Understanding Ethernet Cable
To understand the difference between Cat 5e and Cat 6 ethernet cabling it is important to compare the differences between the two cables and the standards that govern the termination of these cables and the types of environment they can be used in.

Cable Termination standards
Before looking at the different types of cabling available the types of termination need to be considered and for Cat5 and 6 the most common termination is via an RJ-45 connector using either T568A or T568B as described in the standards for this type of connection [1]. It is also important to be aware of where each of the standards is applied, for example although T568A may be the preferred cabling structure it is a requirement by law to use this formatting within federal contracts but T568B has a better compatibility with legacy telecoms carriers in the United States [2]. There is also the option for each end of the cable to be terminated differently to one another in order to allow connection of two like devices such as two PC’s without the use of a switch, this type of cable is referred to as a cross over cable [2].
Category 5e cabling
When looking at majority of networks around the world the most abundant cable used is category 5e given its price and availability [3]. Cat5e cabling is specified to operate at 100MHz, although some cabling that is sold is available up to 350MHz this is not supported within the Cat5e specification [4]. Cat5e also has a maximum speed supported of 1000Mbps which makes the cable suitable for gigabit networking although the maximum limit for using it at the gigabit speed is 50 metres rather than the specification of 100m [4]. There is also a ethernet standard as part of 802.3 IEEE which outlines what type of network that Cat5e cabling can support. Cat 5e supports up to 1000Base-T networks as specified in IEEE 802.3ab which was introduced in 1999 [5].
Category 6 Cabling
Cat6 cabling has been specified to operate at a higher frequency that previous cable standards and operates at 250MHz allowing for greater bandwidth, this increased operational frequency also allows for a greater capacity to operate at 1Gbps over a greater distance than cat 5e. The cable standard is designed for gigabit speed over the entire distance of 100m [6]. Cat 6 standard also allows for the cable to operate at speeds of 10Gbps but this is only possible at lengths of up to 55m as beyond this signal integrity suffers [6]. This increased speed means that Cat 6 cable is able to operate on networks based on the IEEE standard of 802.3an which accounts for 10GB-Base-T [5]. It is also worth noting that although the standard does not necessitate the use of any shielding within the cable a number of Cat 6 cables will use a shielding around either the individual twisted pairs or around within the jacket of the cable, this comes in the form of a foil layer to reduce cross talk and external interference [6].
Comparing the two cables
When comparing the two cables against one another it is important to understand the requirements of the business it is being installed into and any restraints present such as cost. Although Cat6 offers a greater redundancy going forward as it allows for higher transfer speeds and operability with newer hardware it does mean a greater capital investment when installing the cabling. Cat6 however does provide a lower amount of cross talk and is less susceptible to interference from external factors such as electrical cabling [6].
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Analyze diagrams and tables for the TIA/EIA 568-A standard Ethernet cable.
The following table and diagrams display the color scheme and pinouts, as well as the function of the four pairs of wires used for the 568-A standard. 
Note: In LAN installations using 100Base-T (100 Mb/s), only two pairs out of the four are used.
568-A 10/100/1000Base-TX Ethernet
	Pin Number
	Pair Number
	Wire Color
	10Base-T Signal
100Base-TX Signal
	1000Base-T Signal

	1
	2
	White/Green
	Transmit
	BI_DA+

	2
	2
	Green
	Transmit
	BI_DA-

	3
	3
	White/Orange
	Receive
	BI_DB+

	4
	1
	Blue
	Not Used
	BI_DC+

	5
	1
	White/Blue
	Not Used
	BI_DC-

	6
	3
	Orange
	Receive
	BI_DB-

	7
	4
	White/Brown
	Not Used
	BI_DD+

	8
	4
	Brown
	Not Used
	BI_DD-




The following diagrams display how the wire color and pinouts align with an RJ-45 jack for the 568-A standard.
[image: T-568A]
[image: RJ-45 Jack]
Analyze diagrams and tables for the TIA/EIA 568-B standard Ethernet cable.
The following table and diagram display the color scheme and pinouts for the 568-B standard.
568-B 10/100/1000-BaseTX Ethernet
	Pin Number
	Pair Number
	Wire Color
	10Base-T Signal
100Base-TX Signal
	1000Base-T Signal

	1
	2
	White/Orange
	Transmit
	BI_DA+

	2
	2
	Orange
	Transmit
	BI_DA-

	3
	3
	White/Green
	Receive
	BI_DB+

	4
	1
	Blue
	Not Used
	BI_DC+

	5
	1
	White/Blue
	Not Used
	BI_DC-

	6
	3
	Green
	Receive
	BI_DB-

	7
	4
	White/Brown
	Not Used
	BI_DD+

	8
	4
	Brown
	Not Used
	BI_DD-


[image: T568B_ColorPinout_AndRJ45Jack]


Build an Ethernet Crossover Cable
A crossover cable has the second and third pairs on the RJ-45 connector at one end, reversed at the other end (refer to the table in Part 1, Step 2). The cable pinouts are the 568-A standard on one end and the 568-B standard on the other end. The two following diagrams illustrate this concept.
[image: Cross_over_CableRJ45Connectors_1]
Build and terminate a TIA/EIA 568-A cable end.
Determine the cable length required. (Your instructor will let you know the cable length you should make.)
Note: If you were making a cable in a production environment, the general guideline is to add another 12 in. (30.48 cm) to the length.
Cut off a piece of cable to the desired length and using your wire stripper, remove 5.08 cm (2 in.) of the cable jacket from both ends.
Hold the four pairs of twisted cables tightly where the jacket was cut away. Reorganize the cable pairs into the order of the 568-A wiring standard. Refer to the diagrams, if necessary. Take as much care as possible to maintain the twists in the cable; this provides noise cancellation.
Flatten, straighten, and line up the wires using your thumb and forefinger.
Ensure that the cable wires are still in the correct order for the 568-A standard. Using your wire cutters, trim the four pairs in a straight line to within 1.25 to 1.9 cm (1/2 to 3/4 in.).
Place an RJ-45 connector on the end of your cable, with the prong on the underside pointing downward. Firmly insert the wires into the RJ-45 connector. All wires should be seen at the end of the connector in their proper positions. If the wires are not extending to the end of the connector, take the cable out, rearrange the wires as necessary, and reinsert the wires back into the RJ-45 connector.
If everything is correct, insert the RJ-45 connector with cable into the crimper. Crimp down hard enough to force the contacts on the RJ-45 connector through the insulation on the wires, thus completing the conducting path. See the following diagram for an example.
[image: crimp_Pic]
Build and terminate a TIA/EIA 568-B cable end.
Repeat steps 1a to 1g using the 568-B color wiring scheme for the other end.
Test an Ethernet Crossover Cable
Test the cable.
Many cable testers will test for length and mapping of wires. If the cable tester has a wire map feature, it verifies which pins on one end of the cable are connected to which pins on the other end.
If your instructor has a cable tester, test the crossover cable for functionality. If it fails, check with your instructor first as to whether you should re-cable the ends and re-test.
Connect two PCs together via NICs using your Ethernet crossover cable.
Working with a lab partner, set your PC to one of the IP addresses shown in the Addressing Table (see page 1). For example, if your PC is PC-A, your IP address should be set to 192.168.10.1 with a 24-bit subnet mask. You partner’s IP address should be 192.168.10.2. The default gateway address can be left empty.
Using the crossover cable you made, connect the two PCs together via their NICs.
On the PC-A command prompt, ping the PC-B IP address.
Note: The Windows firewall may have to be temporarily disabled for pings to be successful. If the firewall is disabled, make sure you re-enable it at the conclusion of this lab.
Repeat the process and ping from PC-B to PC-A.
Assuming IP addressing and firewall are not issues, your pings should be successful if the cables were properly made.
Reflection
Which part of making cables did you find the most difficult?
It was difficult ensuring each cable was correctly seated in the connector to ensure correct operation
Why do you have to learn how to make a cable if you can easily buy pre-made cables?
[bookmark: _GoBack]It is cheaper to build your own cable and if in a corporate environment you may need shorter cable runs than are commercially available and the shorter the cable allows for more efficient data transfer and also the heat exchange possible in large datacenters.
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