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Abstract 
Detailed in this report is the design of a microcontroller based weather and air quality measurement and logging system which is required to record data over a 14 day period. This data acquisition system is intended to be used by amateur weather forecasters to aid in their weather predictions. The system will be portable and adaptable for a variety of monitoring sites. 
The data that the weather and air quality measurement and logging system will be required to measure the following data over a 14-day period: 
· Temperature
· Humidity
· Wind speed
· Wind direction 
· Airborne particle count
· Sunlight brightness
· UV levels 
· GPS position 
· VOC level




















Introduction 
There are a variety of portable weather and air quality measurement and logging systems available to buy on the market that can record a variety of different weather parameters to aid amateur weather forecasters and to record air particles in different environments to record possible pollution issues and harmful particles in a certain environment. Below are a few examples of portable weather and air quality measurement and logging systems that are available on the market. 
Davis Vantage Pro2 Wireless Weather Station & WeatherLink Live Bundle 6122UK
Figure 1 – Davis Vantage Pro2
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The Davis Vantage Pro2 weather station has a rugged design which is designed to offer years of service. The Integrated sensor suite is solar powered. All electronic components are protected in a weather resistant case. All the outdoor electronic components are designed to resist the effects of the environmental conditions. This system is designed so that the user can live stream any data that is being collected. 
The Davis Vantage Pro2 weather station is capable of measuring: 
· Air quality 
· Barometric pressure
· Dew point 
· Humidity 
· Leaf wetness 
· Rainfall 
· Soil moisture 
· Soil temperature 
· Temperature 
· Water temperature 
· Wind direction 
· Wind speed [1]
The Davis Vantage Pro2 is capable of measuring a large variety of weather parameters as shown above. This system would be ideal for an amateur weather forecaster, but it does not measure some parameters required in the specification such as airborne particle count. 
The cost of this weather system is £989.99

ACCUR8 DWS7100 7-in1 Complete Solar-Powered Wi-Fi Weather station 
[image: Graphical user interface
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The solar-powered 7 in 1 outdoor sensor suite reliably transmits a variety of different weather parameters to the display console seen in the above image. 
This weather station is capable of measuring: 
· Wind speed 
· Wind direction 
· Humidity 
· Temperature 
· Rainfall 
· UV level 
· Light intensity [2]
This weather system would be a great tool for amateur weather forecasters but is incapable of measuring some parameters required such as airborne particle count. 
This weather system costs £179.95



Bresser 5 in 1 Complete Weather Station 

[image: A picture containing text, clock
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The Bresser 5 in 1 wireless weather station combines a compact design with in depth information about the weather. This weather system is powered by 3 AA batteries for the outdoor sensor suite and the display console and there is no capability for solar power. 
The Bresser 5 in 1 wireless weather station is capable of measuring: 
· Wind speed 
· Wind direction 
· Humidity 
· Temperature 
· Precipitation [3]
This is a more basic weather system which is not capable of measuring several required weather parameters such as sunlight brightness, UV levels and Airborne particle count. 
The cost of this weather system is £109.99







Spectrum WatchDog 3250 weather station 
[image: ]
The Spectrum WatchDog 3250 weather station is a more professional weather station than the previous models. This model boasts integrated solar power and a variety of connectivity methods including USB, Bluetooth and RS232 communications. This weather station has an internal data logger that holds 18 months of data and can be used in a variety of environmental conditions with an operating temperature range of -30°C to 55 °C
The Spectrum WatchDog 3250 weather station is capable of measuring the following: 
· Evapotranspiration 
· Humidity 
· Leaf Wetness 
· Quantum Light 
· Rainfall 
· Soil moisture 
· Solar radiation 
· Temperature 
· UV 
· Wind direction 
· Wind speed [4]
The cost of this weather system is £2945.83




Table 1 – Comparison of Portable Weather Stations 
	
	Davis Vantage Pro2
	ACCUR8 DWS7100
	Bresser 7002510
	Spectrum WatchDog 3250 

	Cost 
	£989.99
	£179.95
	£109.99
	£2945.83

	Temperature 
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	Humidity 
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	Wind speed 
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	Wind direction 
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	Sunlight brightness 
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	UV levels 
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	VOC level 
	[image: X]
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	GPS position 
	[image: X]
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After comparing all relevant parameters, the ACCUR8 DWS7100 is the best choice portable weather system for an amateur weather forecaster. This weather system is capable of measuring temperature, humidity, wind speed, wind direction, sunlight brightness and UV levels. The only parameters that this system does not factor is the VOC level and it does not track GPS position. This weather system is very reasonably priced at £179.95 and therefore would be ideal for an amateur weather forecaster.













Equipment 
Microcontroller Selection
Before selecting an appropriate Microcontroller that is capable of processing the incoming signals from the sensors required to build the portable weather system a list was first compiled to choose which functions were required on the microcontroller. 
The Microcontroller selected was the PIC18F24K50. This microcontroller has all the pins required for the 14 day weather and air quality measurement and logging system. 
[image: Diagram, schematic

Description automatically generated]Figure 1 – Microcontroller PIC18F24K50






[28]

Casing selection 
An appropriate case is required to house the electronic components and to protect against all environmental conditions. The portable weather system will be used outside in poor weather conditions so the case must be rated to at least IP66. The case must also be of sturdy design so that it can survive impact damage and protect the delicate electronic components inside. 
The case that has been selected for this portable weather system is the Peli 1200 Waterproof Plastic Equipment case as seen below: 
[image: ][29]
The Peli watertight equipment case is designed to protect materials inside and is supplied with internal foam support to keep articles safe and secure. The case is rated to IP67 so it will keep internal components dry and protected. Cost = £109.07
Non – volatile Memory Storage
	
	Logging rate
	Bytes 
	Bytes/s

	Temperature 
	60 min
	2 
	2000 bytes/s

	Humidity 
	60 min
	2
	2000 bytes/s

	Wind speed 
	60 min
	2
	2000 bytes/s 

	Wind direction 
	60 min
	1
	1 byte/s

	Airborne particle count
	12 hours 
	1
	1 byte/s 

	Sunlight brightness 
	60 min
	2
	2000 bytes/s

	VOC levels
	12 hours
	1
	1 byte/s

	UV levels
	· 
	1
	2000 bytes/s

	GPS position 
	60 mins
	2
	1 byte/s 



It can be seen in the above table that the system is required to record 10004 bytes per second. 
To calculate the total bytes per minute = 10004 x 60 = 600,240 bytes
Number of bytes per hour = 600,240 x 60 = 36,014,400 bytes 
Number of bytes per day = 36,014,400 x 24 = 864,345,600 bytes 
Number of bytes per week (7 days) = 6,050,419,200 bytes 
Number of bytes of the required 14 period = 6,050,419,200 x 2 = 12,100,838,400 (12.1 GB) 
Using these calculations, a 16GB SD card is required for the non-volatile storage. The SD card selected is the ATP 16 GB industrial SD card as shown below and costs £65.05. 
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Sensor Selection 

Temperature/humidity sensor
The portable weather system is required to measure a number of environmental conditions such as temperature and humidity. There are several sensors on the market that can measure both temperature and humidity. A comparison of some examples are shown below: 

	
	HygroVUE10 [5]
	EE181-L [6]
	Amphenol Advanced Sensors Temperature and Humidity sensor [7]
	TE Connectivity Temperature & Humidity Sensor [8]

	Image of sensor 
	[image: A close-up of a syringe
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	[image: A close-up of a stethoscope
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	Power supply 
	7 – 28 Vdc
	7-30 Vdc
	5 Vdc
	3-10 Vdc

	Temperature range 
	-40˚C - +70˚C
	-40˚C - +60˚C
	-20˚C - 70˚C
	-40˚C - 85˚C

	Temperature accuracy 
	+/- 0.2˚C
	+/- 0.2˚C
	+/-0.5˚C
	N/A

	Relative humidity range
	0 – 100% RH
	0 – 100% RH
	0 – 95% RH
	1 – 99% RH

	Relative humidity range 
	+/-1% RH
	+/-2.3% RH
	+/-2% RH
	+/-3 RH

	Number of pins
	4
	5
	4
	4

	Environment protection 
	IP67
	IP65 
	IP67
	N/A

	Cost 
	Unknown 
	Unknown
	£43.97
	£128.95



The sensor selected to measure the temperature and humidity is the Amphenol Advanced. This sensor is the most appropriate for the application required. It runs off low voltage, is accurate enough for the requirements of an amateur weather forecaster and is very reasonably priced at £43.97. 






Wind speed/direction sensor 
The portable weather measurement system is required to measure both wind speed and direction. Below is a comparison table of sensors that measure both wind speed and direction. 

	
	WSD-V Wind speed and direction sensor [9]
	WindSonic solid state wind speed and direction sensor
	Meteorological sensor wind speed and direction [11]
	05103-L Wind Monitor [12]

	Image of sensor 
	[image: ]
	[image: ]
	[image: ]
	[image: ]

	Power supply
	12V AC/DC
	5 – 30Vdc
	9Vdc – 26Vdc
	Voltage supplied by data logger

	Output 
	0-5Vdc
	RS232
	4 – 20 mA
	AC voltage (3 pulses per revolution)

	Wind speed Accuracy 
	5% or 1.5 m/s
	+/- 2%
	+/- 0.3 m/s
	+/- 0.3 m/s

	Maximum wind speed 
	Unknown 
	60 m/s
	60 m/s
	100 m/s

	Wind direction accuracy 
	+/- 5˚
	+/- 2%
	+/- 1%
	+/- 3°

	Number of pins 
	4
	RS232 connection
	6
	6 

	Cost 
	£552
	£812
	£1393.93
	Unknown 



The wind direction and speed sensor selected for the weather measurement sensor is the WSD-V wind speed and direction sensor. This is the most appropriate for the application required. The selected sensor is accurate and costs £552 which is the cheapest out of the sensors compared. 










Airborne particle count 
The portable weather measurement system is required to measure the amount of airborne particles in the environment. Below is a comparison of sensors that measure airborne particles. 
	
	Airnet ll channel air particle sensor [13]
	TERA sensor Next-PM [14]
	Sensirion SEN50-SDN-T [15]

	Image of sensor 
	[image: ]
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	Power supply 
	24Vdc
	5Vdc
	5Vdc

	Size range
	0.3 - 0.5 µm
	0.3-10 µm
	0.3 – 1 µm

	Output 
	24Vdv, 4-20mA
	5Vdv
	3.3V

	Number of pins 
	6
	3
	6

	Cost 
	Unknown
	£93.16
	£21.44



The airborne particle sensor selected for the weather measurement system is the TERA sensor Next-PM. Through comparison, this sensor is the most appropriate for the required application. It has the largest size range and costs £93.16

Sunlight brightness sensor 
The portable weather measurement system is required to measure sunlight brightness. Below is a comparison table for sensors that measure sunlight brightness/lux. 
	
	External light level sensor[16]
	ML-020S-0 Lux sensor [17]
	ML-020S-I Lux sensor[18]

	Image of sensor 
	[image: ]
	[image: ]
	[image: ]

	Supply voltage
	12V AC/DC
	0-30mV
	0-30mV

	Output 
	0-10V / 4-20mA
	0-20mV
	0-30mV

	Range 
	0 – 20000 Lux
	0-150Klux 
	0-30Klux 

	Number of pins
	3
	2
	2

	Cost 
	£40
	Unknown
	Unknown



The sunlight brightness sensor selected for the weather measurement system is the External Light Level Sensor. This sensor has the most robust design which will hold up to the environmental conditions and costs £40. 






UV sensor 
The portable weather measurement system is required to measure UV levels in the environment. Below is a comparison table of sensors capable of measuring UV levels. 
	
	Davis UV sensor[19]
	Renke UV sensor (wall mounted) [20]
	Renke UV sensor (aluminum shell)[21]

	Image of sensor 
	[image: ]
	[image: ]
	[image: ]

	Power supply 
	3V +/-10%
	0-30Vdc
	0-30Vdc

	Output 
	0-2.5V
	0-5V
	0-5V

	Range 
	300 – 1100 nm
	240-370nm
	290-390nm

	Number of pins
	4
	3
	3

	Cost 
	£530.58
	£51
	£67



The UV sensor selected for the portable weather system is the Renke UV sensor (aluminum shell) This sensor is designed to be used outdoors so it is appropriate for the portable weather system. The cost of this sensor is £67. 






VOC level sensor 
The next sensor to be selected is the VOC sensor. VOC stands for Volatile Organic Compound. Volatile Organic Compounds are often components of hydraulic fluids or petroleum products and are common ground water contaminants. 
	
	AQDTF Duct Air Quality VOC Sensor [22]
	Titon VOC sensor [23] 
	BAPI voc Duct and Harsh Environment Sensor [24]

	Image of sensor
	[image: ]
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	Power supply 
	20-28V AC/DC
	12-35Vdc
	12Vdc

	Output 
	0-5V
	0-10V
	0-5V

	Range 
	450-2000 ppm 
	400-2000ppm
	0-2000ppm

	Number of pins 
	3
	3
	3

	Cost 
	£310
	Unknown
	£284.61



The VOC level sensor selected for the portable weather system is the BAPI VOC Duct and Harsh Environment sensor. This sensor has the widest range and runs off a 12Vdc supply. The cost of this sensor is £284.61. 





GPS Position sensor 
The portable weather measurement system is required to track the position of the weather system using GPS. Below is a comparison table of appropriate GPS sensors. 
	
	GPS 16Xlvs [25]
	GPS160 NMEA 0183 [26]
	GPS 34xd GPS receiver [27]

	Image of sensor 
	[image: ]
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	Power supply 
	3.3 – 6Vdc
	12Vdc
	9-16Vdc

	Accuracy 
	10 metres 
	1 metre
	Precise 

	Number of pins
	Cat5
	3
	3

	Cost 
	$81.47
	£156
	£249.95



The GPS sensor to be used in this portable weather system is the GPS160 NMEA 0183. This sensor is very accurate and has an accuracy of 1 metre which will be more than sufficient for the portable weather system. The cost of this sensor is £156. 
Connector Selection
The sensors selected require both 3 pin and 4 pin connectors. 
The selected connectors must have good protection from environmental conditions and the material of the pins must be gold. The pins of the connectors must be gold as the material gives improved electrical connectivity as gold plating provides a smooth finish which allows consistent circuit connection and gold has very good conductive properties which ensures a strong electrical connection. Gold connectors also increase durability and provide improves corrosion protection which is especially important in this weather monitoring system as it will be outdoors for long periods. 
3 pin plug/socket
The connector selected for the 3 pin connectors is the ‘RS PRO cable mount connector’ as seen in the image below: 
[image: A close-up of some binoculars
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These connectors are gold plated which will ensure quality electrical connection. They are rated to IP68 so they are designed to be used in very harsh environmental conditions and have a current rating of 10 amps which is more than enough. The cost of this plug/socket is £26.53 and 5 of them are required. 

4 pin plug/socket
The connector selected for the 4 pin connector is also the ‘RS PRO Cable Mount Connector’ except this one has 4 pins instead of 3 and can be seen below: 
[image: A close-up of a binoculars

Description automatically generated with low confidence][32]
These connectors are also gold plated and rated to IP68 so they will be appropriate for use in the weather measurement system. The cost of this plug/socket is £24.67 and 2 of them are required. 
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