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ANSWER ALL QUESTIONS

1. A message is PCM coded by the system below:

[image: ]
(a) How many bits per second are actually sent in this coding schema?
[2 Marks]
(b) What is the bandwidth of the PCM data stream?
[2 Marks]
(c) If this PCM coded stream is encoded using a Manchester code, what is the new bandwidth of the PCM coded data stream and why?
[4 Marks]
(d) Explain why using a Manchester code is useful for transmitting digital data over a DC decoupled wire transmission line.
[6 Marks]
(e) Explain the benefits of employing HDB3 instead of Manchester code for this PCM data stream when transmitting over a DC decoupled wire transmission line.
[6 Marks]


2. 
(a) Explain the operation of cyclic redundancy checks (CRCs) and comment on their effect on the transmitted information. 
[5 Marks]

(b) A system proposes to transmit a data word 11001 using the CRC generator polynomial G(x) = x3 + x2 +1.

Using the frame to be transmitted, M(x), the generator or divisor, G(x), and the remainder, R(x), calculate the transmitted codeword, and prove that it would be correctly decoded at the receiver if it were using the same CRC generator G(x).
[10 Marks]

(c) Explain the uses of go-back-n and selective repeat in ARQ processes with logical link control (LLC) protocols.
[5 Marks]

3. The output from a receiver contains the following series of values when digitised with an 8-bit digitiser:

	n
	0
	1
	2
	3
	4
	5
	6
	7
	8
	9

	x
	62
	68
	65
	255
	66
	68
	97
	106
	101
	104



(a) What would the output be from passing this sequence through a moving average filter of window size 3 (3rd order moving average filter)?
[7 Marks]
(b) What would the output be from passing the same input stream through a median filter of window size 3?
[7 Marks]
(c) Explain the effect of  increasing the window size for windowed filters on
 
(i) Noise reduction
[2 Marks]
(ii) Delay (latency)
[2 Marks]
(iii) Detecting step transitions in the input data stream  (e.g. “1/0” or “0/1” symbol changes in digital data).
[2 Marks]
4. 
a) Draw a constellation diagram for a quadrature phase shift keying (QPSK) system and allocate binary codes to each phase. Using your allocation of codes indicate the phases used to transmit the following sequence of digits.


[6 Marks]

b) State 'Shannon's Noisy Channel Coding Theorem' and use your answer to calculate the required bandwidths necessary to achieve a 1 x 103 bits/sec data rate when the signal to noise ratio (S/N) is 1, 3, 15, 255 and 1023 respectively.

[4 Marks]

c) 
A set of transmitted data is to be encoded using a (7,4) Hamming code with the parity check matrix,  given by equation Q4c.

	Equation Q4c


Find the generator matrix,  to produce the coded data and calculate the codes produced by the sequences:



[10 Marks]
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