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· Is DHCP successful in Ha1 and Ha2? 
no
Should be successful. If not Troubleshoot!
· From Ha1, ping Ha2. Is it successful? 
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Should be successful. If not Troubleshoot!






· From Ha2, ping Ra1. Is it successful?
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· Connect 209.165.201.1 from Hc1 using SSH. Is it reachable? 
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Should be reachable. If not Troubleshoot!
· Connect 209.165.201.1 from Hc2 using SSH. Is it reachable? 
· 
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Should be reachable. If not Troubleshoot!
· Connect 209.165.201.1 from Ha1 using SSH. Is it reachable? 
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Should be reachable. If not Troubleshoot!
· Connect 209.165.201.1 from Ha2 using SSH. Is it reachable? 
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Should be reachable. If not Troubleshoot!
· Connect 209.165.201.1 from Hc1 using SSH. Is it reachable? 
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Should be reachable. If not Troubleshoot!
· Connect 209.165.201.1 from Hc2 using SSH. Is it reachable? 
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Should not reach. If not Troubleshoot!
· Connect 209.165.201.1 from Ha1 using SSH. Is it reachable? 
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Should not reach. If not Troubleshoot!
· Connect 209.165.201.1 from Ha2 using SSH. Is it reachable? 
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Activy Resus :47:49

You did not complete the activity. Please close this window and try again.
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Packet Tracer BC Command Line 1.0
C:\sping 152.163.20.4

Pinging 152.168.20.4 with 32 byves of data:

Request timed out.
Request timed out.
Request timed out.
Request timed out.

Ping scavistics for 192.168.20 4:
Packets: Sent = 4, Received = 0, Lost = 4 (100% loss),

il
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Packet Tracer BC Command Line 1.0
C:\>ping 152163 10.1

Pinging 152.168.10.1 with 32 byves of dava:

Request timed out.
Request timed out.
Request timed out.
Request timed out.

Ping stavistics for 192.168.10.
Packets: Sent = 3, Received

Tost = 4 (1008 loss),

e
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Packet Tracer PC Command Line 1.0
Covsssh -1 admin 205.165.201.1

s Connection vimed ouss zemote host not sespending
el
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C:\>ssh -1 admin 10.0.0.1

% Connection timed out; remote host mot responding




