	
	HAZARD IDENTIFICATION & RISK ASSESSMENT 
	

	
	
	06 May 2020

	
	
	Page 11 



	Project Title:
	Single two storey detached building with loft
	Person Completing Assessment:
	Dylan Matthews

	Risk Assessment Title:
	RA for Working at heights, Manuel handling and pouring concrete 
	Signature:
	D.matthews

	Date:
	06.5.2020
	
	

	
	Severity
	 KEY:

	
	1
	2
	3
	4
	LOW
	LOW (1 - 4) – May be acceptable: however, review task to see if risk can be reduced further

	Probability
	Negligible
	Minor
	Severe
	Extreme
	
	

	1
	Improbable
	1
	2
	3
	4
	MEDIUM
	MEDIUM (4 – 9) – Task should only proceed with appropriate consultation with specialist personnel. Where possible, the task should be refined to take account of the hazards involved or the risks should be reduced further prior to task commencement  

	2
	Remote
	2
	4
	6
	8
	
	

	3
	Possible
	3
	6
	9
	12
	HIGH
	HIGH (12 – 16) – Task must not proceed. It should be redefined or further control measures put in place to reduce risk. The controls should be re-assessed for adequacy prior to task commencement

	4
	Probable
	4
	8
	12
	16
	
	

	Hazard Identification, Risk Assessments and Determining Controls:
The process of developing any risk assessment should consider the following hierarchy:
	Risk Assessments should now consider the following issues:
· Routine and non-routine activities
· Activities of all persons with access to workplace including other contractors and visitors
· Human behaviours, capabilities and other human factors
· Possible hazards outside of the workplace that may impact on operations
· Legal obligations
· Infrastructure, equipment and materials
· Changes to an organisations activities or structure
· Changes to specification or methods of working

	1
	Identify Risk
	Identify the hazards, decide who might be harmed and how
	

	2
	Evaluate Risk
	Evaluate the probability and severity of the risk using above matrix
	

	3
	Eliminate Risk
	Always try and eliminate the risk by identifying if the operation needs to be carried out or whether it can be done in a different method. 
	

	4
	Reduce Risk
	Identify controls to mitigate risk i.e. engineering controls first then signage/warnings & administrative controls and PPE always as a last resort
	

	5
	Inform/consult people about the Risk
	Consult people likely to carry out the operations or obtain guidance if necessary then record the findings on this form & notify people about the risks by way of inductions etc.
	

	6
	Control the Risk
	Ensure that the required controls identified in stage 4 above are in place and effective
	

	7
	Review the Risk
	Review your assessment and update if necessary
	



	
	Identified Risk
	

	Residual Risk

	
Ref.
	
Hazard
	
Person at Risk
	
P
	
S
	
R
	
Response/Control Measure
	
P
	
S
	
R

	1
	Working at height 
	Staff
	3
	4
	12
	· All staff to use the designated walkways and crossing points.
· Safe working platforms at height
· Installed personal equipment such as roes
· No stacking materials near edges preventing falling objects
· Minimise gaps by closing up any small gaps in boarding 
· Avoid carrying materials up ladders
· Use toe boards and brick guards as safeguards


	1
	4
	4

	2
	






Manual Handling
	Working Party
	3
	3
	9
	· All ASL operatives have received manual handling training.
· It is not anticipated that any heavy items are going to be used.
· Awkward items, such as double glazed window panels, must also be handled by a minimum of two persons, and care should be taken to not place hands or fingers in any trapping points.
· It must be emphasised that any heavy items should always be moved by mechanical means where practicable.
· Operatives are to work to their own capabilities only, always ask for help where necessary and do not struggle.
· Prior to carrying items, operatives should check their transit route is clear of obstructions or anything which could pose a slip or trip hazard.

	1
	3
	3

	3
	








Pouring Concrete 
	Operatives
	3
	3
	9
	· All Personnel to be briefed on COSHH assessment before works commence.
· Correct task specific PPE to be worn at all times when handling substance.
· This includes gauntlets and eye protection
· If any concrete gets on skin or in a persons eyes then it must be rinsed immediately under the supervision of a first aider, if problems persist then then seek medical advice.
· You must read and understand the COSHH assessment, ask any questions if you are unsure of any elements

	1
	3
	3



