	Device
	Issue
	Action

	Factory Switch
	G 0/0/1 is disabled
	Use the no shutdown command on g0/0/1 to enable

	PC5
	Default Gateway not present on Device Network settings
	Enter the default gateway 192.168.5.129 to the NIC settings

	Branch-2 Switch
	S 0/1/0 has an incorrect ip addresses assigned prevent network connectivity
	Change IP address of S0/1/0 from 192.168.0.17 to 192.168.0.6 with command ip address 192.168.0.6 255.255.255.252

	Factory Switch
	OSPF Configuration no entry for the 192.168.4.0 network
	Add the 192.168.4.0 network with command router ospf 10 followed by Network 192.168.4.0 0.0.0.255

	Hub Router
	Nat Inside config not set on the Serial 0/1/0 port
	[bookmark: _GoBack]Configure the serial 0/1/0 port and add the ip nat inside command.



