Design and Connect a Simple Network
Task 1
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a. Ipconfig What is the IP address of PC-A? 
192.168.1.10
b. What is the subnet mask of the computer? 
255.255.255.0
c. Ping 192.168.1.11 (PC-B) Was the ping successful?
Yes
Click PCB (PC1)  Desktop  Command Prompt 
a. Ipconfig What is the IP address of PC-B? 
192.168.1.10
b. What is the subnet mask of the computer? 
255.255.255.0
c. Ping 192.168.1.10 (PC-A) Was the ping successful? 
Yes
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Task 2
1. Is your IP Address Automatically configured or Manually Configured? 
Automatic
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2. Were the ping results successful? 
Yes

3. Record your reflection
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Trace complete.

:\Users\taylo>

Command Prompt
Users\taylostracert wuw.google.com
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Tracing route to www.google.com [216.58.213.4]
ver a maximum of 36 hops:

192.168.128.1
no-dns-yet.as25178.net [169.246.19.181]
no-dns-yet.as25178.net [169.246.30.8]
72.14.195.66

108.176.246.129

172.253.65.269
1hr25525-in-f4.1€160.net [216.58.213.4]
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Packet Tracer BC Command Line 1.0
C:\>ping 152.165.1.11

Pinging 152.168.1.11 with 32 bytes of data:

Reply from 152.165.1.11 “ime=lms TTL-128
Reply from 152163 1.11 “ime=3ms TTL-128
Reply from 152163 1.11 “ime=loms TTL-128
Reply from 152165111 “ime<lms TTL-128

Ping stavisties for 152.165.1.11
Packets: Sent = 3, Received = 4, Lost = 0 (0% loss),
Bpprosimate round trip vimes in milli-seconds
Minimm = Oms, Maximm = 10ms, Average = dms
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General | Alternative Configuration
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TH You can get P settings assigned automatical f your network supports

this capabiity. Otherwise, you need to ask your network adminstrator
for the appropriate P settngs.

‘Sample for Manual Configuration. If “Obtain an IP address automatically” is selected, then your
PC/ Laptop is DHCP/ Automatic configured. Record the status above.
® Obtain an P address automatically

O Use the foloning I adaress:

Step 6: From your PC/ Laptop, use the Command Prompt to verify the PC settings and
connectivity. Right-click Start, select Command Prompt

Computer Management

Command Prompt
(O Obtain DN server address automaticaly

emmand Prompt (dmin)
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Command Prompt

Microsoft Windows [Version 16.6.18363.1082]
(c) 2619 Microsoft Corporation. All rights reserved.

:\Users\taylo>ipconfig /all

Windows TP Configuration

Host Name . . . . .. . .. ... : DESKTOP-T7P@DDU
Primary Dns Suffix . . . .. . .
Node Type . . . . . ... . ... Hybrid
1P Routing Enabled. . . . . . . . : No
WINS Proxy Enabled. . . . . . . . : No
Ethernet adapter Ethernet:
Connection-specific DNS Suffix .
Description . . . . . . . . ... : Realtek PCIe GbE Family Controller
Physical Address. . . . . . ... F4-30-B9-8D-E1-36
DHCP Enabled. . . . . . .. ... Yes
Autoconfiguration Enabled . . . . : Yes
Link-local IPv6 Address . . . . . Feg0: :c9c:8bce: ce09: esbe%16(Preferred)
Pva Address. . . . . . . ... . 192.168.129.87(Preferred)

Subnet Mask . . . . . .. .... : 255.255.240.0
02 October 2020 11:37:21
02 October 2020 16:07:21

Lease Expires . . . . . . .. ..

Default Gateway . . . . . . . . . : 192.168.128.1

DHCP Server . . . . . . .. ... 192.168.128.1

DHCPV6 TAID . . . . . . . . ... 183775417

DHCPV6 Client DUID. . . . . . . . : 60-61-00-01-27-67-67-00-F4-30-B9-8D-E1-36

DNS Servers . . . . . . . . . . . 109.246.13.15
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Command Prompt

:\Users\taylo>ping ww.google.com

Pinging wa.google.com [216.58.213.4] with 32 bytes of data:
Reply from 216.58.213.4: bytes=32 time=7ms TTL-120

Reply from 216.58.213.4: bytes=32 time=7ms
Reply from 216.58.213.4: bytes=32 time=7ms
Reply from 216.58.213.4: bytes=32 time=7ms

ping statistics for 216.58.213..
Packets: Sent = 4, Received = 4, Lost = @ (8% loss),

Approximate round trip times in milli-seconds:

Minimum = 7ms, Maximum = 7ms, Average = 7ms

:\Users\taylo>





