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Figure 1 : Adding a default forwarder[image: A screenshot of a computer

AI-generated content may be incorrect.]Figure 2 : creating NAT network because NAT network from vbox is not working
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Figure 3 : DHCP config
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Figure 4 : DHCP installation
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Figure 5 : DNS setup
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Figure 6 : all the features installed
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Figure 7 : DHCP setup on Debian
[image: A screenshot of a computer

AI-generated content may be incorrect.]
Figure 8 : IP WAN S-DC
[image: A screenshot of a computer

AI-generated content may be incorrect.]
Figure 9 : VPN setup
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Figure 10 : debian firewall config
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Figure 11 : router setup
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Figure 12 : scope for DHCP
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Figure 13 : website code
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Figure 14 : website setup
[image: A screenshot of a computer

AI-generated content may be incorrect.]
Figure 15 : website from ClientC1
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[root@c-server:/home/ewenn# sudo iptables -L INPUT -v

chain TNPUT (policy ACCEPT 0 packets, @ bytes)

pkts bytes target prot opt in out source destination
3 252 DROP 1k * 9.0.0.0/0 10.0.1.2

Jrootec-server: /home/euenn# sudo iptables -t nat -L POSTROUTING -v

chain POSTROUTING (policy ACCEPT @ packets, @ bytes)

pkts bytes target prot opt in out source destination
6 1472 MASQUERADE 6  -- x enpes3  9.9.0.0/0 9.0.0.0/0

rootac-server: /hame/euenn# suda susctl -p

et . ipva. ip_foruard = 1

et . ipvd.conf.all.proxy_arp = 1

rootac-server: /home/euenng date

Thu 13 Mar 19:52:35 GMT 2025

rootac-server: /home/euenng _

iemptype 8
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