R1

R1#show run
Building configuration...

Current configuration : 1219 bytes
!
version 15.1
no service timestamps log datetime msec
no service timestamps debug datetime msec
no service password-encryption
!
hostname R1
!
!
!
!
!
!
!
!
no ip cef
no ipv6 cef
!
!
!
!
license udi pid CISCO2911/K9 sn FTX1524EBU3-
!
!
!
!
!
!
!
!
!
!
!
spanning-tree mode pvst
!
!
!
!
!
!
interface GigabitEthernet0/0
 ip address 185.95.1.1 255.255.255.0
 duplex auto
 speed auto
!
interface GigabitEthernet0/1
 no ip address
 duplex auto
 speed auto
 shutdown
!
interface GigabitEthernet0/2
 no ip address
 duplex auto
 speed auto
 shutdown
!
interface Serial0/0/0
 no ip address
!
interface Serial0/0/1
 no ip address
 clock rate 2000000
!
interface GigabitEthernet0/1/0
 no ip address
 shutdown
!
interface FastEthernet0/2/0
 switchport mode access
!
interface FastEthernet0/2/1
 switchport mode access
!
interface FastEthernet0/2/2
 switchport mode access
!
interface FastEthernet0/2/3
 switchport mode access
!
interface Vlan1
 no ip address
 shutdown
!
router ospf 1
 log-adjacency-changes
!
router ospf 2
 router-id 1.1.1.1
 log-adjacency-changes
!
ip classless
!
ip flow-export version 9
!
!
!
banner motd ^CWelcome^C
!
!
!
!
!
line con 0
!
line aux 0
!
line 0/3/0 0/3/7
 login
!
line vty 0 4
 login
!
!
!
end


--

R1#show ip int brief 
Interface              IP-Address      OK? Method Status                Protocol 
GigabitEthernet0/0     185.95.1.1      YES manual up                    up 
GigabitEthernet0/1     unassigned      YES unset  administratively down down 
GigabitEthernet0/2     unassigned      YES unset  administratively down down 
Serial0/0/0            unassigned      YES unset  down                  down 
Serial0/0/1            unassigned      YES unset  down                  down 
GigabitEthernet0/1/0   unassigned      YES unset  administratively down down 
FastEthernet0/2/0      unassigned      YES unset  up                    down 
FastEthernet0/2/1      unassigned      YES unset  up                    down 
FastEthernet0/2/2      unassigned      YES unset  up                    down 
FastEthernet0/2/3      unassigned      YES unset  up                    down 
Vlan1                  unassigned      YES unset  administratively down down
R1#

--

R1#show ip route
R1#show ip route 
Codes: L - local, C - connected, S - static, R - RIP, M - mobile, B - BGP
       D - EIGRP, EX - EIGRP external, O - OSPF, IA - OSPF inter area
       N1 - OSPF NSSA external type 1, N2 - OSPF NSSA external type 2
       E1 - OSPF external type 1, E2 - OSPF external type 2, E - EGP
       i - IS-IS, L1 - IS-IS level-1, L2 - IS-IS level-2, ia - IS-IS inter area
       * - candidate default, U - per-user static route, o - ODR
       P - periodic downloaded static route

Gateway of last resort is not set

     185.95.0.0/16 is variably subnetted, 2 subnets, 2 masks
C       185.95.1.0/24 is directly connected, GigabitEthernet0/0
L       185.95.1.1/32 is directly connected, GigabitEthernet0/0


--

ip ospf neighbor 
%OSPF: Router process 1 is not running, please configure a router-id


show ip ospf database 
%OSPF: Router process 1 is not running, please configure a router-id



------------------------------------------------------------------------------------------------------



R3

R3#show run
Building configuration...

Current configuration : 1225 bytes
!
version 15.1
no service timestamps log datetime msec
no service timestamps debug datetime msec
no service password-encryption
!
hostname R3
!
!
!
!
!
!
!
!
no ip cef
no ipv6 cef
!
!
!
!
license udi pid CISCO2911/K9 sn FTX1524MNU2-
!
!
!
!
!
!
!
!
!
!
!
spanning-tree mode pvst
!
!
!
!
!
!
interface GigabitEthernet0/0
 ip address 185.95.3.1 255.255.255.0
 duplex auto
 speed auto
!
interface GigabitEthernet0/1
 no ip address
 duplex auto
 speed auto
 shutdown
!
interface GigabitEthernet0/2
 no ip address
 duplex auto
 speed auto
 shutdown
!
interface GigabitEthernet0/0/0
 no ip address
 shutdown
!
interface Serial0/1/0
 no ip address
 clock rate 2000000
 shutdown
!
interface Serial0/1/1
 no ip address
 clock rate 2000000
 shutdown
!
interface FastEthernet0/2/0
 switchport mode access
!
interface FastEthernet0/2/1
 switchport mode access
!
interface FastEthernet0/2/2
 switchport mode access
!
interface FastEthernet0/2/3
 switchport mode access
!
interface Vlan1
 no ip address
 shutdown
!
router ospf 2
 router-id 3.3.3.3
 log-adjacency-changes
!
ip classless
!
ip flow-export version 9
!
!
!
banner motd ^CWelcome Back^C
!
!
!
!
!
line con 0
!
line aux 0
!
line 0/3/0 0/3/7
 login
!
line vty 0 4
 login
!
!
!
end

--

R3#show ip int brief 
Interface              IP-Address      OK? Method Status                Protocol 
GigabitEthernet0/0     185.95.3.1      YES manual up                    up 
GigabitEthernet0/1     unassigned      YES unset  administratively down down 
GigabitEthernet0/2     unassigned      YES unset  administratively down down 
GigabitEthernet0/0/0   unassigned      YES unset  administratively down down 
Serial0/1/0            unassigned      YES unset  administratively down down 
Serial0/1/1            unassigned      YES unset  administratively down down 
FastEthernet0/2/0      unassigned      YES unset  up                    down 
FastEthernet0/2/1      unassigned      YES unset  up                    down 
FastEthernet0/2/2      unassigned      YES unset  up                    down 
FastEthernet0/2/3      unassigned      YES unset  up                    down 
Vlan1                  unassigned      YES unset  administratively down down

--

R3#show ip route 
Codes: L - local, C - connected, S - static, R - RIP, M - mobile, B - BGP
       D - EIGRP, EX - EIGRP external, O - OSPF, IA - OSPF inter area
       N1 - OSPF NSSA external type 1, N2 - OSPF NSSA external type 2
       E1 - OSPF external type 1, E2 - OSPF external type 2, E - EGP
       i - IS-IS, L1 - IS-IS level-1, L2 - IS-IS level-2, ia - IS-IS inter area
       * - candidate default, U - per-user static route, o - ODR
       P - periodic downloaded static route

Gateway of last resort is not set

     185.95.0.0/16 is variably subnetted, 2 subnets, 2 masks
C       185.95.3.0/24 is directly connected, GigabitEthernet0/0
L       185.95.3.1/32 is directly connected, GigabitEthernet0/0

--

R3#show ip ospf neighbor 

R3#show ip ospf neighbor 

R3#show ip ospf neighbor ?
  Ethernet         IEEE 802.3
  FastEthernet     FastEthernet IEEE 802.3
  GigabitEthernet  GigabitEthernet IEEE 802.3z
  Loopback         Loopback interface
  Serial           Serial
  detail           detail of all neighbors
  <cr>
R3#show ip ospf neighbor 

R3#show ip ospf neighbor 
R3#show ip ospf neighbor g
R3#show ip ospf neighbor gigabitEthernet 
% Incomplete command.
R3#show ip ospf neighbor gigabitEthernet ?
  <0-9>  GigabitEthernet interface number
R3#show ip ospf neighbor gigabitEthernet 1
                                          ^
% Invalid input detected at '^' marker.
	
R3#show ip ospf nei
R3#show ip ospf neighbor 

R3#show ip ospf database
R3#show ip ospf database 
R3#show ip ospf database ?
  asbr-summary  ASBR summary link states
  external      External link states
  network       Network link states
  router        Router link states
  summary       Network summary link states
  <cr>
R3#show ip ospf database 
R3#



-----------------------------------------------------------------------------------


R2#show run
Building configuration...

Current configuration : 1221 bytes
!
version 15.1
no service timestamps log datetime msec
no service timestamps debug datetime msec
no service password-encryption
!
hostname R2
!
!
!
!
!
!
!
!
no ip cef
no ipv6 cef
!
!
!
!
license udi pid CISCO2911/K9 sn FTX1524C4EO-
!
!
!
!
!
!
!
!
!
!
!
spanning-tree mode pvst
!
!
!
!
!
!
interface GigabitEthernet0/0
 ip address 185.95.2.1 255.255.255.0
 duplex auto
 speed auto
!
interface GigabitEthernet0/1
 no ip address
 duplex auto
 speed auto
 shutdown
!
interface GigabitEthernet0/2
 no ip address
 duplex auto
 speed auto
 shutdown
!
interface GigabitEthernet0/0/0
 no ip address
 shutdown
!
interface Serial0/1/0
 no ip address
 clock rate 2000000
 shutdown
!
interface Serial0/1/1
 no ip address
 clock rate 2000000
 shutdown
!
interface FastEthernet0/3/0
 switchport mode access
!
interface FastEthernet0/3/1
 switchport mode access
!
interface FastEthernet0/3/2
 switchport mode access
!
interface FastEthernet0/3/3
 switchport mode access
!
interface Vlan1
 no ip address
 shutdown
!
router ospf 2
 router-id 2.2.2.2
 log-adjacency-changes
!
ip classless
!
ip flow-export version 9
!
!
!
banner motd ^CWelcome2^C
!
!
!
!
!
line con 0
!
line aux 0
!
line 0/2/0 0/2/7
 login
!
line vty 0 4
 login
!
!
!
end

--

R2#show ip int brief 
Interface              IP-Address      OK? Method Status                Protocol 
GigabitEthernet0/0     185.95.2.1      YES manual up                    up 
GigabitEthernet0/1     unassigned      YES unset  administratively down down 
GigabitEthernet0/2     unassigned      YES unset  administratively down down 
GigabitEthernet0/0/0   unassigned      YES unset  administratively down down 
Serial0/1/0            unassigned      YES unset  administratively down down 
Serial0/1/1            unassigned      YES unset  administratively down down 
FastEthernet0/3/0      unassigned      YES unset  up                    down 
FastEthernet0/3/1      unassigned      YES unset  up                    down 
FastEthernet0/3/2      unassigned      YES unset  up                    down 
FastEthernet0/3/3      unassigned      YES unset  up                    down 
Vlan1                  unassigned      YES unset  administratively down down

--
R2#show ip route 
Codes: L - local, C - connected, S - static, R - RIP, M - mobile, B - BGP
       D - EIGRP, EX - EIGRP external, O - OSPF, IA - OSPF inter area
       N1 - OSPF NSSA external type 1, N2 - OSPF NSSA external type 2
       E1 - OSPF external type 1, E2 - OSPF external type 2, E - EGP
       i - IS-IS, L1 - IS-IS level-1, L2 - IS-IS level-2, ia - IS-IS inter area
       * - candidate default, U - per-user static route, o - ODR
       P - periodic downloaded static route

Gateway of last resort is not set

     185.95.0.0/16 is variably subnetted, 2 subnets, 2 masks
C       185.95.2.0/24 is directly connected, GigabitEthernet0/0
L       185.95.2.1/32 is directly connected, GigabitEthernet0/0


--

R2#show ip ospf 
 Routing Process "ospf 2" with ID 2.2.2.2
 Supports only single TOS(TOS0) routes
 Supports opaque LSA
 SPF schedule delay 5 secs, Hold time between two SPFs 10 secs
 Minimum LSA interval 5 secs. Minimum LSA arrival 1 secs
 Number of external LSA 0. Checksum Sum 0x000000
 Number of opaque AS LSA 0. Checksum Sum 0x000000
 Number of DCbitless external and opaque AS LSA 0
 Number of DoNotAge external and opaque AS LSA 0
 Number of areas in this router is 0. 0 normal 0 stub 0 nssa
 External flood list length 0


--
R2#show ip ospf databa
R2#show ip ospf database 
R2#
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