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c) 
Determinate structures are analysed just by the use of basic equilibrium equations. By this analysis, the unknown reactions are found for the further determination of stresses. Whereas indeterminate structures are not capable of being analysed by mere use of basic equilibrium equations. Along with the basic equilibrium equations, some extra conditions are required. Special methods like strain energy method, slope deflection method, moment distribution method, column analogy method, virtual work method, matrix methods, etc are used for the analysis of redundant structures.

e) 
· For statically determinate structures, r = 3n 
· If r > 3n, structure is statically indeterminate 
Where; 
n = the total number of the parts of structure. 
r = the total number of unknown reactive force and moment components

g)
Frame structures are the structures having the combination of beam, column and slab to resist the lateral and gravity loads. These structures are usually used to overcome the large moments developing due to the applied loading. Two basic classifications of frame structure would be rigid frame structure and braced frame structure.

h) 
Over rigid meaning the truss has too many members. Under rigid meaning the truss has too little members.

i) 
For a truss to be rigid, the following condition must exist
m = 2j – 3 
where m = Number of members
j = Number of joints
Non-rigid or imperfect truss does not obey this equation.

j) 
(i) – Warren truss    (ii) – Pratt truss     (iii) – Howe truss     (iv) – K-truss      (v) – Fink truss
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