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[bookmark: _GoBack]A Guide to Safety Precautions when TRAINED OFFICERS attend a Road Collision involving a Hybrid or Plug in Electrical vehicles.

1. Ask the driver/owner or witness if the vehicles involved in the collision are Electric Hybrid vehicles?
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2.	 “Turn the ignition OFF”.
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3.	Remove the Key from the vehicle and place it at least 5 meters away from the vehicle in a safe place, Don’t Lose the key!
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4.	If the vehicle has collision damage “THINK about YOUR SAFETY FIRST” before you return to the vehicle PUT YOUR RUBBER GUANTLETS ON!!
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5.	Do not push the vehicle or rotate the vehicles wheels until the service plug has been removed, remember you are dealing with 600Volts.
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6.	Stay safe and wait until a Trained Police officer or Trained recovery agent arrives at the scene.
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7.	Trained Police officers can disconnect the Negative terminal on the 12v Auxiliary Battery, use insulated tools.
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8.	REMOVE the Electric Service plug and put it in the Police vehicle for safe keeping.
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8.	Where to find the Electric Service Plug? Check the vehicles handbook if it’s inside the vehicle, if not use the Application named RESCUE CODE.
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9.	Type in the vehicle details into the application and it will automatically show you where to find the Electric Service Plug.
10.	REMEMBER TO WAIT 5 minutes before Moving or Working the vehicle. 
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11.	If in doubt ask for the Commercial Vehicle Unit officers to assist, namely PC 1521 YOUNG and PC 1230 DUNNING.
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