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LewisaL-C0: " ip a
1: 1o: <LOOPBACK,UP,LOMER_UP> mtu 65536 gdisc nogueue state UNKNOWN group default olen 1000
Link/loophack 00:00:00:00:00:00 brd 00:00:00:00:00:00
inet 127.0.0.1/8 scope host lo
valid_Lft forever preferred_lft forever
ineté /128 scope host noprefixroute
valid_Lft forever preferred_lft forever
o: enpos3: <BROADCAST,MULTICAST,UP,LOHER_UP> mtu 1560 gdisc fo_codel state U group default glen 1008
Link/ether 08:00:27:16:2:28 brd ff:ff:ff:if:fffi
altname enxo80027f62128
inet 192.168.2.1/24 brd 192.165.2.255 scape global enpes3
valid_Lft forever preferred_lft forever
ineté -~ oo o /64 scope link proto kernel 11
valid_Lft forever preferred_lft forever
f: enposs: <BROADCAST,MULTICAST,UP,LOER_UP> mtu 1560 gdisc fo_codel state U group default glen 1008
Link/ether 08:00:27:31:86:4 brd ff:ff:ff:if:fffi
altname enxo800273a6f4
inet 20.6.0.2/39 brd 20.0.0.3 scope global enpose
valid_Lft forever preferred_lft forever
ineté -~ oo - /64 scope link proto kernel 11
valid_Lft forever preferred_lft forever
42 enpos3: <BROADCAST,MULTICAST,UP,LOHER_UP> mtu 1560 gdisc fo_codel state U group default glen 1008
Link/ether 08:00:27:a0:07:45 brd ff:ff:ff:ffaffff
altname enxo80027ac0745
inet 10.0.4.15/24 brd 10.0.4.255 scope global dynamic noprefixroute enpess
valid_Lft 784d6sec preferred_lft 67646sec
inete oot oiooiooosooii/64 scope link
valid_Lft forever preferred_lft forever
J5: wga: <POINTOPOINT,NDARP,UP,LOWER_UP> mtu 1420 odisc nogueue state UNKNOWN group default glen 1060
Link/none
inet 10.0.0.1/24 scope global uge
valid_Lft forever preferred_lft forever
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lewisel-cD:™s ip route

default via 10.0.4.2 dev enpess proto dhcp src 10.9.4.15 metric 1004
10.0.0.0/24 dev uge proto kernel scope link src 10.0.0.1

10.0.4.0/24 dev enpos9 proto dhep scope Link src 10.9.4.15 metric 1004
0.0.0.0/50 dev enpose proto kernel scope link src 20.0.0.2

152,165, 1.0/24 dev ugo scope link

152.165.2.0/24 dev enps3 proto kernel scope link src 192.168.2.1
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opyright (C) Microsoft Corporation. All rights reserved.
jinstall the latest Powershell for new features and improvements! https://aka.ms/PSindous
ps C:\Users\Adninistrator> Get-Service RemoteAccess
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Running RemoteAccess Routing and Remote Access
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Administrator: Windows Po I

pS C:\Users\Adninistrator> Get-ItemProperty HKLM:\SYSTEM\CurrentControlSet\Services\Tcpip\Parameters\

IPEnableRouter

Microsoft.Powershell.Core\Registry: :HKEY_LOCAL_MACHINE\SYSTEM\CurrentControlSet\Services\Tcpip\Parameters\

Microsoft.Powershell.Core\Registry: :HKEY_LOCAL_MACHINE\SYSTEM\CurrentControlSet\Services\Tcpip
Parameters
HKLM

: Microsoft.Powershell.Core\Registry

ps C:\Users\Administrator> o

s
RS g0, [




image10.png
LewisL-CD: ™8 cat /proc/sys/net/invd/ip_foruard
a
LewisaL-co:~e




image11.png
P Windows Defender Firewall with Advanced Security -
Fle Acion View Help

e a2 E
& Windows Defender Frewall vt [ 1 ‘Actions
oo Name Gow Profile  Ensbled  Action || Inbound Rules
e Connection Securty Rules | @ Allow HITP A Ve Alow 1 || NewRue.
% Monitoring @ Allow HTTPS A Ve Alow 0 ey profie R
@ Allow HTTPS for RDS A Ve Alow 1
@ ICMPTraffic Al Yes Alow 1 || FiferbyState 4
@ WireGusrd UDP A Ve Mlow 1 || 7 Fiterby Group »
 Actve Dirctory Domain Controle - Ec... Actve Diectory DomainSer. Al Ves Alow 1 View R
 Active Directory Domain Controle - Ec... Actve Diectory DomainSer. Al Ves Alow 1
€9 Active Directory Domain Controller - LD... Active Directory Domain Ser... All Yes Alow b || G Refresh
9 Active Dirctory Domin Controler - LD... Active A Ve Mlow 1 ||l Bporit
9 Active Dirctory Domin Controler - LD... Active A Ve Mlow 0 |[@ Hep
© Active Directory Domin Controle - et A Ve Alow 1
9 Active Dirctory Domin Controle - SA. A Ve Alow 1
@ Active Directory Domin Controle - SA. A Ve Alow 1
 Actve Direcory Domin Controle - Se. A Ve Alow 1
@ Active Dirctory Domin Controle - Sec.. A Ve Alow 1
@ Actve Directory Domin Controler - ... A Ve Alow 1
1 Active Dirctory Domain Controler (RPC) CAL e Alow 1
@ Active Dirctory Domain Controler (RPC... CAL e Alow 1
 Actve Directory Web Services (TCP-In)  Actve Directory Web Senvices Al Ves Alow 1
@ Alloyn Router (TCP-In) Alloyn Router Alow 1
@ Alloyn Router (UDP-In) Alloyn Router Ves Alow 1
Border Gateway Protocol BGP-In) Border Gateway Protocol (B.. Al No Alow 1
BranchCache Content Retrieval (HTTP-in) No Alow 1
BranchCache Hosted Cache Server (HTTP... . No Alow 1
BranchCache Peer Discovery (WSD-in)  BranchCache - PeerDiscove.. Al No Alow 1
@ Castto Device functionlity (qWave-TCP... Castto Device functionsity Alow 1
© Castto Device functionlity (qWsve-UDP... Cstto Device functionsity Alow 1
© Castto Device SSDP Discovery (UDP-In)  Castto Device functionsity Alow 1
© Castto Device streaming server (HTTP-S... Castto Device functionsity Alow ¥
>

) ENG





image12.png
LewiseL-CD:~¢ sudn wg

[sudo] passuord for lewis:

interface: wzo
public key: GY@aUpR24M11rGHIBTkATvablTuNs30 JRUHGINDAYGE=
private key: (hidden)
Listening port: 51820

Jpeer: ud96LCrbN1BouNLVOBHNRE THY 1YB1LRSDSOLTVEUZKK=
endpaint: 20.0.0.1:51820
allowed ips: 10.6.0.0/24, 192.168.1.0/24
latest handshake: 43 seconds ago
transfer: 300.54 KiB received, 385.82 KiB sent
persistent keepalive: every 25 seconds
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$ systemctl status wg-ouick@uge
uwgd.service - WireGuard via wg-guick(8) for uge

loaded (/usr/lib/systemd/systen/ug-guicke.service; enabled; preset: enabled
active (exited) since Sat 2026-05-02 12:07:23 BST; 2h 24min ago
8686070491324a63965 72311078403

man: ug-quick (8)

man: ug (8)

https://u. wireguard.con/

https://uuw. wireguard. con/quickstart/

https:s/git.zx2cd. con/uireguard-tonls/about /src/man/ug-ouick .8
https:s/git.zx2cd. con/uireguard-tonls/about /src/man/ug .8

837 ExecStart=/usr/bin/ug-quick up wgs (code=exited, status=0/SUCCESS)
837 (code=exited, status=0/SUCCESS)

2.7

26ms

me journal files were not opened due to insufficient permissions.
% systemctl is-enabled ug-ouick@uzo

~%
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Deactivate

Peer
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3 Administrator: Command Prompt

icrosoft Windows [Version 10.6.26348.587] ~
(c) Microsoft Corporation. All rights reserved.

:\Users\Administrator>ping 16.6.0.1

pinging 16.0.6.1 with 32 bytes of data:

[Reply from 2 timecins TTL-64
Reply from 2 timecins TTL-64
Reply from 2 timecins TTL-64
[Reply from 2 timecins TTL-64

ping statistics for 16.0.6.1:
Packets: Sent = 4, Received = 4, Lost = © (8% loss),
ppproximate round trip times in milli-seconds:
Minimum = @ms, Maximum - ems, Average = 6ms

:\Users\Adninistrator>ping 192.168.2.1

pinging 192.168.2.1 with 32 bytes of data:
bytes=32 timecims TTL-64

[Reply from 192.168.2.1
[Reply from 192.168.2.1
[Reply from 192.168.2.1
[Reply from 192.168.2.1: byte:

ping statistics for 192.168.2.1
Packets: Sent = 4, Received = 4, Lost = © (8% loss),
ppproximate round trip times in milli-seconds:
Minimum = @ms, Maximum - ems, Average = 6ms

:\Users\Administrator>

e
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lewiseL-C0: "8 ping 10.0.8.2
PING 10.0.0.2 (10.6.0.2) 56(84) butes of data.

64 bytes from 10.0.0.2: icmp_sen=1 tt
64 butes from 10.0.0.2: icmp_sen=2 ti
64 butes from 10.0.0.2: icmp_sen=3 ti
¢ butes from 10.0.0.2: icmp_sen=¢ tt1=128 time=0.997 ms
64 butes from 10.0.0.2: icmp_sen=5 ti

--- 16.0.0.2 ping statistics ---

5 packets transmitted, 5 received, 6% packet loss, time 4672ms
It min/ave/max/mdev = .337/0.622/0.937/0.201 ms
lewiseL-c0: " ping 192.168.1.1

PING 192.168.1.1 (192.168.1.1) 56(84) butes of data

64 bytes from 192.168.1.1: icmp_seg=1 tt

¢ butes from 192.168.1.1: icmp_seq=2 tt1=127 time=0.950 ms
64 butes from 192.168.1.1: icmp_sed=3 tt

64 butes from 192.168.1.1: icmp_ser

64 butes from 192.168.1.1: icmp_sed=S tt

--- 152.166.1.1 ping statistics
5 packets transmitted, 5 received, 8% packet loss, time 4086ms
It min/avg/max/mdev = 0.544/1.132/1.690/0.478 ms
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Administrator: Windows

jindows PowerShell
opyright (C) Microsoft Corporation. All rights reserved

install the latest PowerShell for new features and improvements! https://aka.ms/PSindous

Ps c:\Users\administrator> nslookup lewis.acca
fserver:  Unknoun

address: ::1

Name:  lewis.acca

addresses: 20.0.0.1
192.168.1.1
10.0.0.2
10.0.4.15

PS C:\Users\Administrator> nslookup webs.lewis.acca
fserver:  Unknoun
Jaddress:

Name:  webs.lewis.acca
hddress: 192.168.1.1

Ps c:\Users\administrator> nslookup rds.lewis.acca

fserver:  Unknoun
Jaddress:
Name:  rds.lewis.acca

hddress:  192.168.1.1

Ps c:\Users\administrator> nslookup Clientl1.lewis.acca
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20.0.0.

lewiseL-c0:~$ nslookup uebs. lewis.acca 192.168.1.1
fserver 192.168.1.1
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ame:  uebs. lewis.acca
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B Administrator: Windows PowerShell ISE - X
Fie Edit View Tools Debug Add-ons Help
& H 4 0o » P & W w | & oot m.
[ User Creation Scriptpst X
1 SCsvPath "C:\Users\Administrator\Documents\users.csv"
2 sBaseoy o,
3 SDomainFQON = "lewis.acca”
i STemppud “TenpPassword20261 1"
s
6 Import-vodule ActiveDirectory
7
s
5 Gtry {
10 New-ADOrganizationalUnit -Name "Students” -Path "DC=lewis,DC-acca” -ProtectedFromiccidentalDeletion $False -Erroraction Stop
11 |3 cateh €3
12
e
13 Srous = Import-Csv -Path SCsvPath
pr}
16 Eforeach (sr in Srows) {
brd SFirst = Sr_First_nane.TrimQ)
18 $last = Srlast_name.TrinQ)
19 SF ([string]: :IsNul10rwhiteSpaca(SFirst) -or [string]::IsNullOrWhiteSpace(STast)) { continue }
20
21
22 Ssam = ("{0}.{1}" -F $First.Substring(0,1), Slast).ToLower()
25
2 $local = (Sr.email -split "e")[0]
2 Supn S5 2n@SDoma nFQDN”
26 $mail = "SlocalesDonainFQON"
27
28 if (-not (Get-ADUser -Filter "UserPrincipalName -eq 'Supn'" -ErrorAction SilentlyContinue)) {
29 New-ADUser -Name "SFirst Slast” '
30 “GivenName SFirst -Surname Slast °
51 “SamAccountNane Ssan -UserPrincipalNane Supn °
32 “path SGase0U -Enabled Strue -ChangePasswordAtLogon Strue *
33 -AccountPassword (ConvertTo-SecureString STempPwd -AsPlainText -Force) °
3 “Title Sr_job -Department Sr.department -Company Sr.company -City Sr.city °
35 “Enailaddrass Smatl
36 Write-Host "Created $(s$first) $($last) (Ssam)”
375 jelsef
38 Write-Host "Exists  $(Sfirst) $($last) (Ssam) -- skipped”
39 b
a0 [3
a1
42 writeHost "Done.”
Ln1 Col1 100%
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LewisaL-CD:~¢ suda realm list
[sudo] passuord for lewis:
Lewis.acca
type: kerberos
realn-name: LEWIS.ACCA
domain-name: lewis.acca
configured: kerberos-member
server-softuare: active-directary
client-softuare: sssd
required-package: sssd-tools
required-package: sssd
required-package: 1ibnss-sss
required-package: libpam-sss
required-package: adcli
required-package: samba-common-bin
login-formats: #Ualewis.acca
login-policy: allow-realm-logins
LewiseL-co:~s
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Network

lewis@ClientL1: ~
Bluetooth

root@ClientL1:/home/lewis# sudo realm list
lewis.acca
Displays | type: kerberos
realm-name: LEWIS.ACCA
domain-name: lewis.acca
configured: kerberos-member
server-software: active-directory
Power client-software: sssd
required-package: sssd-tools
Multitaskin required-package: sssd
required-package: libnss-sss
required-package: Llibpam-sss
Appearancé  required-package: adcli
required-package: samba-common-bin
Tlogin-formats: %U@lewis.acca
Apps Togin-policy: allow-realm-logins
root@Clientl1:/home/lewis# [
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lewis@l -CD:~$ sudo cat /etc/default/isc-dhcp-relay

j# Defaults for isc-dhcp-relay initscript

J# sourced by setc/init.dsisc-ohep-relay

J# installed at setc/defaultsisc-dhcp-relay by the maintainer scripts

a
J» This is a POSIX shell fragment
d

J# Hhat servers should the DHCP relay foruard requests to?
JSERVERS="20.0.0.1"

J# 0n what interfaces should the DHCP relay (dhrelay) serve DHCP requests?
enpos3 enposs”

INTERFACESVE=

J# Additional options that are passed to the DHCP relay daemon?
P TIONS=""
lewiseL-c0: " systemctl status isc-dhcp-relay

o isc-dhcp-relay.service - LSB: DHCP relay
Loaded: loaded (/etc/init.d/isc-dhep-relay; generated
Active: active (running) since Sat 2026-05-02 12:07:23 BST; 3h 18min ago

Invocation: b27804653e3fd6albesfe78b2dI41121
Dacs: man:systend-sysv-generator (8
Process: 830 ExecStart=/etc/init.d/isc-dhcp-relay start (codesexited, statu:
Tasks: 1 (limit: 2301)
Memory: 2.5M (peak: 3.1M)
CPU: 14ms
Ceroup: /systen.slice/isc-dhcp-relay. service
658 /usr/shin/dhcrelay - 20.0.0.1

/SUCCESS)

Jiarning: some journal files were not opened due to insufficient permissions
lewisel-co: "5 _
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ay 15:29

lewis@ClientL1: ~ Qfl = [

root@ClientL1:/home/lewis# sudo /sbin/dhclient -v enpos3
Internet Systems Consortium DHCP Client 4.4.3-P1
Copyright 2004-2022 Internet Systems Consortium.

AU rights reserved.

For info, please visit https://www.isc.org/software/dhcp/

Listening on LPF/enp@s3/08: 6l
Sending on  LPF/enp@s3/08: 0l
sending on  Socket/fallback
DHCPREQUEST for 192.168.2.10 on enp®s3 to 255.255.255.255 port 67
DHCPACK of 192.168.2.10 from 192.168.2.1
Error: ipvd: Address already assigned
bound to 192.168.2.10 -- renewal in 318816 seconds.
root@ClientL1:/home/lewis# ip a
1: lo: <LOOPBACK,UP,LOWER UP> mtu 65536 qdisc noqueue state UNKNOWN group default qlen 1000
link/loopback 00:00:00:00:00:00 brd 00:00:00:00:00:00
inet 127.0.0.1/8 scope host lo
valid_1ft forever preferred ft forever
inet6 ::1/128 scope host noprefixroute
valid_Lft forever preferred 1ft forever
2: enpos3: <BROADCAST,MULTICAST,UP,LOWER UP> mtu 1500 qdisc fq_codel state UP group default glen 1000
link/ether 08:00:27:ab:cf:7d brd ff:f:Ff:ff:ff:f
altname enx@80027abcf7d
inet 192.168.2.10/24 brd 192.168.2.255 scope global dynamic noprefixroute enp@s3
valid_lft 679606sec preferred 1ft 679606sec
inet6 fe80::a00:27ff:feab:cf7d/64 scope link noprefixroute
valid_1ft forever preferred 1ft forever
root@Clientl1:/home/lewis# [

b:cf:7d
b:cf:7d
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lewis@ClientL1: ~ Qfl = [

root@ClientL1:/home/lewis# ip route

default via 192.168.2.1 dev enpos3

default via 192.168.2.1 dev enp0s3 proto dhcp src 192.168.2.10 metric 100
192.168.2.0/24 dev enp0s3 proto kernel scope link src 192.168.2.10 metric 100
root@ClientL1:/home/lewis# sudo cat /etc/resolv.conf

domain lewis.acca

search lewis.acca

nameserver 192.168.1.1

root@ClientL1:/home/lewis#
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lewiseL-c0: "8 ping 192.168.1.1

PING 192.168.1.1 (192.168.1.1) 56(84) butes of data

64 butes from 192.168.1.1: icmp_seg=1 tt1=127 time=0.633 ms
b4 butes from 192.168. icmp_seg=2 tt
b4 butes from 192.168. icmp_seq=3 tt
b4 butes from 192.168. icmp_seq=4 tt
¢ butes from 192.168.1.1: icmp_seq=S tt1=127 time=0.546 ms

--- 192.166.1.1 ping statistics ---
5 packets transmitted, 5 received, 6% packet loss, time 4033ms
rtt min/avg/max/mdev = 6.546/0.825/1.377/6.290 ns
"ClewiseL-C0: "% ping webs. lewis.acca

IPING webs. lewis.acca (192.166.1.1) 56(84) bytes of data.

64 butes from rds.lewis.acca (192.168.1.1): icmp_se
¢ butes from rds.lewis.acca (192.168.1.1): icmp_se
4 butes from rds.lewis acca (192.168.1.1): icmp seq=3 tt1=127 tine=1.63 ms
¢ butes from rds. lewis.acca (192.168.1.1): t11=127 tine=1.77 ms
¢ butes from rds.lewis.acca (192.168.1.1)

|--- webs. lewis.acca ping statistics ---

5 packets transmitted, 5 received, 6% packet loss, time 4027ms
It min/avg/max/mdev = 0.422/1.123/1.765/0.543 ms
"ClewiseL-C0: "8 ping rds. lewis.acca

PING rds. lewis.acca (192.168.1.1) 56(84) butes of data

¢ butes from files.lewis.acca (192.168.1.1): icmp_se
¢ butes from files.lewis.acca (192.168.1.1): icmp_se
¢ butes from files.lewis.acca (192.168.1.1): icmp_se
¢ butes from files.lewis.acca (192.168.1.1): icmp_se

54 butes from files.leuis.acca (192.168.1.1)¢ lcmp_seq=5 1=127 tine=0.542
°C

|--- rds.lewis.acca ping statistics ---

5 packets transmitted, 5 received, 6% packet loss, time 4048ms

it min/ave/max/mdev = .423/0.598/0.650/0.145 ns

lewiseL-cD: "8 ping Clientst

PING Clientst.lewis.acca (192.168.1.10) 56(84) butes of data.

¢ butes from Clientsi.lewis.acca (192.168.1.16): icmp_seq=1 tt1=127 time=0.957 ms
¢ butes from Clientsi.lewis.acca (192.168.1.16): icmp_seq=2 tt1=127 time=0.910 ms
64 butes from Clientsi.lewis.acca (192.168.1.10): .865 ms
4 butes from ClientSi.lewis.acca (192.168.1.18): icmp_seg=¢ tt1=127 time=1.16 ms
¢ butes from Clientsi.lewis.acca (192.168.1.16): icmp_seq=5 tt1=127 time=0.739 ms

°C

--- clientst.lewis.acca ping statistics ---

5 packets transmitted, 5 received, 6% packet loss, time 4024ms
It min/avg/max/mdev = .739/0.926/1.159/0.137 ms

lewisaL-co:
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icrosoft Windows [Version 10.6.26348.587]
(c) Microsoft Corporation. All rights reserved

:\Users\Adninistrator>ping 192.168.2.1

pinging 192.168.2.1 with 32 bytes of data
192.168.2.1
192.168.2.1
192.168.2.1: bytes=32 time<ims
192.168.2.1: bytes=32 time<ims

ping statistics for 192.168.2.1:

Packets: Sent = 4, Received = 4, Lost = @ (8% loss)
ppproximate round trip times in milli-seconds:

Minimum = @ms, Maximum - ems, Average = 6ms

:\Users\Administrator>ping ClientL1

pinging Clientl1.lewis.acca [192.168.2.10] with 32 bytes of data
192.168.2.10: bytes=32 time<ims TTL=63
192.168.2.10: bytes=32 time-Ims TTL=63
192.168.2.10: bytes=32 time TTL-63
192.168.2.10: bytes=32 time TTL-63

ping statistics for 192.168.2.1

Packets: Sent = 4, Received = 4, Lost = @ (8% loss)
ppproximate round trip times in milli-seconds:

Minimum = @ms, Maximum = ims, Average = 6ms

:\Users\Administrator>

A @) NG

15:32
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-1 Advanced Security Setings for SwanseaFils (E) o

Name: E\

Ouner  SYSTEM @ Change

Permissions | Auditing  Effective Access.

For additional information, double-click a permission entry. To modify a permission entry, select the entry and click Edit (f available).

Permission enties:
Tpe  Principsl Access Inheited from Applesto
82 Allow  Administrators (lewis\Adr Full control None “This folder, subfolders and files
82 Allow  SYSTEM Full control None “This folder, subfolders and files
2 Allow  CREATOR OWNER Ful control None Subfolders an filesonly
82 Allow  Users (lewis\Users) Read & execute None “This folder, subfolders and files
82 Allow  Users (lewi\Users) Creste folders/ sppen.. None This folder and subfolders
82 Allow  Users (lewi\Users) Crestefiles /wite dsta  None Subfolders only
2 Allow  Everyone Resd & execute None Thisfolderonly
Add Remove View
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o]
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82 Allow  Administrators (lewis\Adr Ful control None “This folder, subfolders and files
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S8 Allow  Authenticated Users Read & execute None “This folder, subfolders and files

Add Remove View

Enable inheritance.

[]Replace al child object permission entres with inheritable permission entries from this object

ok [ cancel | [ Aol





image44.png
RecydleBin
B0 E | Svansebies

Home  Share  View

€ o1 s Nework » SDClevisacca > Swanseafiles

Quick access

Test
Desktop =

Downloads
< Documents
&) Pictures

Music
B videos

OneDrive
This PC

¥ Network

item

©
=
3
g
z
@
5
8
I
o

anseaFiles

ument

oke

1559
& D) 050 B




image45.png
&
File Action View Help

e a@XEz Bm §E

£ ons
v § sbc
~ [ Forward Lookup Zones
& _msdeslewisacca
- lewisacca
1 Reverse Lookup Zones
(5] Trust Points
[ Conditional Forwarders

Name
msdes

Type Data

Timestamp

Dishes

)

oudp
Elpomainonszond
Sorestonszones
=

Elsame s parent
[Elsame as parent
[Elsame as parent
[Elsame as parent
[Elsame as parent
[Elsame as parent
Elctentt
Elctentst
Elres

o

Elas

Elsde

El-de

El-de

El-de

lwebs

webs Properties

Host () Secuty.

Host (uses parent domain  ef blank):

Fully qualfied domain name (FADN):

[webs.ews acca

1P address:

[192:168.1.1

Usdate associated porter (PTR) record

Aoply

FRARAAA

=

I
"

&) we |,





image46.png
'€ Internet Information Services (1IS) Manager - X
@75 [@) 5DC » Sites » webslewisacca » @@
Fle View Help
- bslewis.acca H
‘webs.lewis.acca Home
@iz |8 e B Explore
T sortPage o
LT ey | - 6o - EyshowAl | Goupby: Area e
22 Application Pocls ASPNET =
- s N i
@ Default Web Site =] U 2 [ Basic setings
M- NET NET NETEmor | NET  NETProfle NETRoles NETTust Ve A
.15 aspot.chent Authorizet. Compiltion  Pages  Globalztion Leves Vios e
] system_web. P 3 —
40019 2 & ® & Wanage Website B
NETUsers  Application Connection MachineKey Pagesand  Providers Session State 2 Restart
SEkings Stings Contels >
® Sop
Browse Website
31 Browae b lewiaccaon

Compression _Default
Document

i al¥

[t %

T M P Address

Redirect  Respon... snd Doma.

P

i, = o=

Output  Request  SSLSettings

Caching  Fitering

3
P
e

¢

ISAP! Filters

Logging  MIME Types

192.168.1.1:80 (htp)
Browse webs.lewis.acca on
B 152.160.1.1:443 (rtps)

Advanced Settings.
Configure.
Failed Request Tracing

Limits
HSTS.

Help

Ready
H P Type here to search

o

&) we |,




image47.png
v @ webskewisaces x
G & Notseaure webs.lewis.accs/

Welcome to Swansea Website

+





image48.png
File Action View Help

e a@XEz Bm §E

£ ons
v § sbc
~ [ Forward Lookup Zones
& _msdeslewisacca
v [ lewisacca
1 msdes
] stes
O tep
1 _udp
(] DomainDnsZone|
(5] ForestDnsZones
=
v [ Reverse Lookup Zones
1 1168.192n-addrarp|
(] 2168.192n-addrarp|
[ Trust Points
[ Conditional Forwarders

Name
msdes

Type Data

Timestamp

Dishes

)

oudp
Elpomainonszond
Sorestonszones
=

Elsame s parent
[Elsame as parent
[Elsame as parent
[Elsame as parent
[Elsame as parent
[Elsame as parent
Elctentt
Elctentst
Elres

o

s

Els-de

El-de

El-de

El-de

Elwebs

rds Properties

Host () Secuty.

Host (uses parent domain  ef blank):

Fully qualfied domain name (FADN):

[rastewis acea

1P address:

[192:168.1.1

Update associated painter (PTR)record

Aoply

FRARAAA

=

16:0:

& D) NG g L





image49.png
PS C:\Users\Administrator> Get-Service TermService

tatus  Name DisplayName

Running Termservice Remote Desktop Services
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r: Command Prompt
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Connection-specific DNS Suffix
Description .

Physical Address.

DHCP Enabled. S
Autoconfiguration Enabled .
Link-local IPv6 Address .
1Pv4 Address.

Subnet Mask .

Default Gateway .

DHCPYV6 TATD . .

DHCPYV6 Client DUID.

DNS Servers .

NetBIOS over Tcpip.
[ethernet adapter S-DC NAT:

Connection-specific DNS Suffix
Description .

Physical Address.

DHCP Enabled. . . . . . . .
Autoconfiguration Enabled .
Link-local IPv6 Address .
1Pv4 Address.

Subnet Mask .

Lease Obtained.

Lease Expires .

Default Gateway .

DHCP Server .

DHCPYV6 TAID . .

DHCPYV6 Client DUID.

DNS Servers .

NetBIOS over Tcpip.

:\Users\Administrator>

192.168.1.1

: Enabled

Intel(R) PRO/1066 MT Desktop Adapter #2
08-00-27-47-87-7E

+:3850:815:5236: d3e2%3 (Preferred)
20.6.0.1(Preferred)
255.255.255.252

319201431
00-61-00-01-31-1D-82-40-08-00-27-95-F3-39
a

127.6.0.1
: Enabled

soac.local

Intel(R) PRO/1066 MT Desktop Adapter #3
08-06-27-81-78-C5

Yes

99F : ebdb : 6ca0: 710C%4 (Preferred)
10.6.4.15(Preferred)
255.255.255.6
02 May 2026 13:04:24
03 May 2626 13:04:23
10.6.2.2
10.6.4.2
386400205
06-01-00-01-31-1D-82-40-68-60-27-95-F3-39
1
127.0.6.1

: Enabled

A @) NG

1414
02/05/2026

™)
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dministr rmand Prompt
\Users\Administrator>route print

.WireGuard Tunnel

.08 06 27 95 £3 39 ......Intel(R) PRO/1006 MT Desktop Adapter

.08 06 27 47 87 7e ......Intel(R) PRO/1060 MT Desktop Adapter #2

.08 06 27 81 78 5 ......Intel(R) PRO/1000 MT Desktop Adapter #3
.Software Loopback Interface 1

Active Routes
jetuork Destination Netmask Gateway Interface Metric
0.0.0.0 0.0.6.0 10.6.4.2
10.6.6.0  255.255.255.8 on-link .0.0. 5
10.6.6.2 255.255.255.255 on-link
10.6.6.255 255.255.255.255 on-link
10.6.4. 255.255.255.6 on-link
255.255.255.255 on-link
10.6.4. 255.255.255.255 on-link
20.6.6.0 255.255.255.252 on-link
20.6.6.1 255.255.255.255 on-link
20.6.6.3 255.255.255.255 on-link
127.0.6. 255.0.6.0 on-link
127.0.6.1 255.255.255.255 on-link
127.255.255. 255.255.255.255 on-link
192.168.1. 255.255.255.6 on-link
192.168.1.1 255.255.255.255 on-link 192.168.
192.168.1. 255.255.255.255 on-link 192.168.
192.168.2. 255.255.255.6 on-link 10.0.
192.168.2. 255.255.255.6 10.6.6.1 10.0.
192.168.2.1 255.255.255.255 20.0.0.2 20.0.
192.168.2. 255.255.255.255 on-link 10.0.
224.0.6. 240.0.6.0 on-link 127.0.
224.0.6. 246.0.6.0 on-link 192.168.1.
224.0.6. 246.0.6.0 on-link 20.6.0.
224.0.6. 240.0.6.0 on-link 10.6.4.1:
255.255.255. 255.255.255.255 on-link 127.0.6.1
255.255.255. 255.255.255.255 on-link 192.168.1.1
255.255.255. 255.255.255.255 on-link 20.6.6.1
255.255.255. 255.255.255.255 on-link 10.6.4.15
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Administrator: Command Prompt

192.168.2.255 255.255.255.255 On-Link 10.0.0.2 261
224.0.6.0 240.0.6.0 on-Link 127.6.6.1 331
224.0.0.0 240.0.0.0 on-Link 192.168.1.1 281
224.0.0.0 240.0.0.0 on-Link 20.0.0.1 281
224.0.6.0 240.0.0.0 on-Link 10.0.4.15 281

255.255.255.255  255.255.255.255 on-Link 127.6.6.1 331

255.255.255.255  255.255.255.255 on-Link 192.168.1.1 281

255.255.255.255  255.255.255.255 on-Link 20.0.0.1 281

255.255.255.255  255.255.255.255 on-Link 10.0.4.15 281

Jpersistent Routes:

Network Address Netmask Gateway Address Metric
192.168.2.0  255.255.255.0 10.0.0.1 1
192.168.2.1 255.255.255.255 20.0.0.2 1

If Metric Network Destination Gateway
1 331 ::1/128 on-link
9 281 fege::/64 on-link
3 281 fese::/64 on-link
4 281 fege::/64 on-link
33 261 fese::/64 on-link
3 281 fese::3850:815F:5236:d3¢2/128
on-link
4 281 fege::899f:ebdb:6ca0:710c/128
on-link
33 261 fege::bd69:ddea:b34a:81bs/128
on-link
© 281 fege::d817:718d:2ebe:4f7c/128
on-link
1 331 ffee::/8 on-link
9 281 ffee::/8 on-link
3 281 Ffee::/8 on-link
4 281 ffee::/8 on-link
33 261 ffee::/8 on-link

persistent Routes
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