UWTSD Level 6 - Lab - Configure VLANs and Trunking 
Topology 
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Addressing Table 
	Device 
	Interface 
	IP Address 
	Subnet Mask 
	Default Gateway 

	S1 
	VLAN 1 
	192.168.10.11 
	255.255.255.0 
	N/A 

	S2 
	VLAN 1 
	192.168.10.12 
	255.255.255.0 
	N/A 

	PC-A 
	NIC 
	192.168.10.3 
	255.255.255.0 
	192.168.10.1 

	PC-B 
	NIC 
	192.168.10.4 
	255.255.255.0 
	192.168.10.1 


Objectives 
Part 1: Build the Network and Configure Basic Device Settings 
Part 2: Create VLANs and Assign Switch Ports 
Part 3: Maintain VLAN Port Assignments and the VLAN Database 
Part 4: Configure an 802.1Q Trunk between the Switches Part 5: Delete the VLAN Database 
Background / Scenario 
Modern switches use virtual local-area networks (VLANs) to improve network performance by separating large Layer 2 broadcast domains into smaller ones. VLANs can also be used as a security measure by controlling which hosts can communicate. In general, VLANs make it easier to design a network to support the goals of an organisation. 
VLAN trunks are used to span VLANs across multiple devices. Trunks allow the traffic from multiple VLANS to travel over a single link, while keeping the VLAN identification and segmentation intact. 
In this lab, you will create VLANs on both switches in the topology, assign VLANs to switch access ports, verify that VLANs are working as expected, and then create a VLAN trunk between the two switches to allow hosts in the same VLAN to communicate through the trunk, regardless of which switch the host is actually attached to. 
Cisco IOS version, the commands available and the output produced might vary from what is shown in the labs. Refer to the Router Interface Summary Table at the end of the lab for the correct interface identifiers. 
Note: Ensure that the routers and switches have been erased and have no startup configurations. If you are unsure contact your instructor. 
Required Resources 
· 2 Switches 
· 2 PCs (Windows with a terminal emulation program, such as Tera Term or Putty) 
· Console cables to configure the Cisco IOS devices via the console ports 
· Ethernet cables as shown in the topology 
Instructions 
Part 1: Build the Network and Configure Basic Device Settings 
In Part 1, you will set up the network topology and configure basic settings on the PC hosts and switches. 
Step 1: Cable the network as shown in the topology. 
Attach the devices as shown in the topology diagram, and cable as necessary. 
Step 2: Configure basic settings for each switch. 
a. Console into the switch and enable privileged EXEC mode. 
Open configuration window 
b. Enter configuration mode. 
c. Assign a device name to the switch. 
d. Disable DNS lookup to prevent the router from attempting to translate incorrectly entered commands as though they were host names. 
e. Configure the IP address listed in the Addressing Table for VLAN 1 on the switch. 
f. Shut down all interfaces that will not be used. 
g. Set the clock on the switch. 
h. Save the running configuration to the startup configuration file. 
Close configuration window 
Step 3: Configure PC hosts. 
Refer to the Addressing Table for PC host address information. 
Step 4: Test connectivity. 
Verify that the PC hosts can ping one another. 
Note: It may be necessary to disable the PCs firewall to ping between PCs. 
Questions: 
Can PC-A ping PC-B? 
Type your answers here. 
Can PC-A ping S1? 

Can PC-B ping S2? 
Type your answers here. 
Open configuration window 
Can S1 ping S2? 
Type your answers here. 
If you answered no to any of the above questions, why were the pings unsuccessful? 
Type your answers here. 
Close configuration window 
Part 2: Create VLANs and Assign Switch Ports 
In Part 2, you will create Management, Operations, CarPark, and Native VLANs on both switches. You will then assign the VLANs to the appropriate interface. The show vlan command is used to verify your configuration settings. 
Step 1: Create VLANs on the switches. 
Open configuration window 
a. Create the VLANs on S1. 
S1(config)# vlan 10 
S1(config-vlan)# name Operations 
S1(config-vlan)# vlan 20 
S1(config-vlan)# name CarPark 
S1(config-vlan)# vlan 99 
S1(config-vlan)# name Management 
S1(config-vlan)# vlan 1000 
S1(config-vlan)# name Native 
S1(config-vlan)# end 
b. Create the same VLANs on S2. 
c. Issue the show vlan brief command to view the list of VLANs on S1. 
S1# show vlan brief 
 
VLAN Name                             Status    Ports 
---- -------------------------------- --------- ------------------------------- 
1    default                          active    Fa0/1, Fa0/2, Fa0/3, Fa0/4 
                                                Fa0/5, Fa0/6, Fa0/7, Fa0/8 
                                                Fa0/9, Fa0/10, Fa0/11, Fa0/12 
                                                Fa0/13, Fa0/14, Fa0/15, Fa0/16 
                                                Fa0/17, Fa0/18, Fa0/19, Fa0/20 
                                                Fa0/21, Fa0/22, Fa0/23, Fa0/24 
                                                Gi0/1, Gi0/2 
10   Operations                       active 
20   CarPark                      active 
99   Management                       active 
1000 Native                           active 
1002 fddi-default                     act/unsup 
1003 token-ring-default               act/unsup 
1004 fddinet-default                  act/unsup 
1005 trnet-default                    act/unsup 
Questions: 
What is the default VLAN? 
Type your answers here. 
What ports are assigned to the default VLAN? 
Type your answers here. 
Step 2: Assign VLANs to the correct switch interfaces. 
a. Assign VLANs to the interfaces on S1. 
1) Assign PC-A to the Operation VLAN. 
S1(config)# interface f0/6 
S1(config-if)# switchport mode access S1(config-if)# switchport access vlan 10 
2) Move the switch IP address VLAN 99. 
S1(config)# interface vlan 1 
S1(config-if)# no ip address 
S1(config-if)# interface vlan 99 
S1(config-if)# ip address 192.168.1.11 255.255.255.0 
S1(config-if)# end 
b. Issue the show vlan brief command and verify that the VLANs are assigned to the correct interfaces. c. Issue the show ip interface brief command. 
Question: 
What is the status of VLAN 99? Explain. 
Type your answers here. 
d. Assign PC-B to the Operations VLAN on S2. 
e. Remove the IP address for VLAN 1 on S2. 
f. Configure an IP address for VLAN 99 on S2 according to the Addressing Table. 
g. Use the show vlan brief command to verify that the VLANs are assigned to the correct interfaces. 
Questions: 
Is S1 able to ping S2? Explain. 
Type your answers here. 
Close configuration window 
Is PC-A able to ping PC-B? Explain. 
Type your answers here. 
Part 3: Maintain VLAN Port Assignments and the VLAN Database 
In Part 3, you will change VLAN assignments to ports and remove VLANs from the VLAN database. 
Step 1: Assign a VLAN to multiple interfaces. 
Open configuration window 
a. On S1, assign interfaces F0/11 – 24 to VLAN99. 
S1(config)# interface range f0/11-24 
S1(config-if-range)# switchport mode access 
S1(config-if-range)# switchport access vlan 99 
S1(config-if-range)# end 
b. Issue the show vlan brief command to verify VLAN assignments. 
c. Reassign F0/11 and F0/21 to VLAN 10. 
d. Verify that VLAN assignments are correct. 
Step 2: Remove a VLAN assignment from an interface. 
a. Use the no switchport access vlan command to remove the VLAN 99 assignment to F0/24. 
S1(config)# interface f0/24 
S1(config-if)# no switchport access vlan 
S1(config-if)# end 
b. Verify that the VLAN change was made. 
Question: 
Which VLAN is F0/24 now associated with? 
Type your answers here. 
Step 3: Remove a VLAN ID from the VLAN database. 
a. Add VLAN 30 to interface F0/24 without issuing the global VLAN command. 
S1(config)# interface f0/24 
S1(config-if)# switchport access vlan 30 
% Access VLAN does not exist. Creating vlan 30 
Note: Current switch technology no longer requires that the vlan command be issued to add a VLAN to the database. By assigning an unknown VLAN to a port, the VLAN will be created and added to the VLAN database. 
b. Verify that the new VLAN is displayed in the VLAN table. 
Question: 
What is the default name of VLAN 30? 
Type your answers here. 
c. Use the no vlan 30 command to remove VLAN 30 from the VLAN database. 
S1(config)# no vlan 30 
S1(config)# end 
d. Issue the show vlan brief command. F0/24 was assigned to VLAN 30. 
Question: 
After deleting VLAN 30 from the VLAN database, what VLAN is port F0/24 assigned to? What happens to the traffic destined to the host attached to F0/24? 
Type your answers here. 
e. Issue the no switchport access vlan command on interface F0/24. 
f. Issue the show vlan brief command to determine the VLAN assignment for F0/24. 
Questions: 
To which VLAN is F0/24 assigned? 
Type your answers here. 
Note: Before removing a VLAN from the database, it is recommended that you reassign all the ports assigned to that VLAN. 
Why should you reassign a port to another VLAN before removing the VLAN from the VLAN database? 
Type your answers here. 
Close configuration window 
Part 4: Configure an 802.1Q Trunk Between the Switches 
In Part 4, you will configure interface F0/1 to use the Dynamic Trunking Protocol (DTP) to allow it to negotiate the trunk mode. After this has been accomplished and verified, you will disable DTP on interface F0/1 and manually configure it as a trunk. 
Step 1: Use DTP to initiate trunking on F0/1. 
The default DTP mode of a 2960 switch port is dynamic auto. This allows the interface to convert the link to a trunk if the neighboring interface is set to trunk or dynamic desirable mode. 
Open configuration window 
a. Set F0/1 on S1 to negotiate trunk mode. 
S1(config)# interface f0/1 
S1(config-if)# switchport mode dynamic desirable 
Sep 19 02:51:47.257: %LINEPROTO-5-UPDOWN: Line protocol on Interface FastEthernet0/1, changed state to up 
Sep 19 02:51:47.291: %LINEPROTO-5-UPDOWN: Line protocol on Interface Vlan99, changed state to up 
You should also receive link status messages on S2. 
S2# 
Sep 19 02:42:19.424: %LINK-3-UPDOWN: Interface FastEthernet0/1, changed state to up 
Sep 19 02:42:21.454: %LINEPROTO-5-UPDOWN: Line protocol on Interface Vlan99, changed state to up 
Sep 19 02:42:22.419: %LINEPROTO-5-UPDOWN: Line protocol on Interface FastEthernet0/1, changed state to up 
b. Issue the show vlan brief command on S1 and S2. Interface F0/1 is no longer assigned to VLAN 1. Trunked interfaces are not listed in the VLAN table. 
c. Issue the show interfaces trunk command to view trunked interfaces. Notice that the mode on S1 is set to desirable, and the mode on S2 is set to auto. 
S1# show interfaces trunk 
 
S2# show interfaces trunk 
Note: By default, all VLANs are allowed on a trunk. The switchport trunk command allows you to control what VLANs have access to the trunk. For this lab, keep the default settings which allows all VLANs to traverse F0/1. 
Close configuration window 
d. Verify that VLAN traffic is traveling over trunk interface F0/1. 
Questions: 
Can S1 ping S2? 
Type your answers here. 
Can PC-A ping PC-B? 
Type your answers here. 
Can PC-A ping S1? 
Type your answers here. 
Can PC-B ping S2? 
Type your answers here. 
If you answered no to any of the above questions, explain below. 
Type your answers here. 
Step 2: Manually configure trunk interface F0/1. 
The switchport mode trunk command is used to manually configure a port as a trunk. This command should be issued on both ends of the link. 
a. Change the switchport mode on interface F0/1 to force trunking. Make sure to do this on both switches. 
Open configuration window 
S1(config)# interface f0/1 
S1(config-if)# switchport mode trunk 
b. Issue the show interfaces trunk command to view the trunk mode. Notice that the mode changed from desirable to on. 
S2# show interfaces trunk 
c. Modify the trunk configuration on both switches by changing the native VLAN from VLAN 1 to VLAN 1000. 
S1(config)# interface f0/1 
S1(config-if)# switchport trunk native vlan 1000 
d. Issue the show interfaces trunk command to view the trunk. Notice the Native VLAN information is updated. 
S2# show interfaces trunk 
Questions: 
Why might you want to manually configure an interface to trunk mode instead of using DTP? 
Type your answers here. 
Why might you want to change the native VLAN on a trunk? 
Type your answers here. 
Close configuration window 











Can PC-A ping S1? 
Type your answers here. 
Can PC-B ping S2? 
Type your answers here. 
If you answered no to any of the above questions, explain below. 
Type your answers here. 
Step 2: Manually configure trunk interface F0/1. 
The switchport mode trunk command is used to manually configure a port as a trunk. This command should be issued on both ends of the link. 
a. Change the switchport mode on interface F0/1 to force trunking. Make sure to do this on both switches. 
Open configuration window 
S1(config)# interface f0/1 
S1(config-if)# switchport mode trunk 
b. Issue the show interfaces trunk command to view the trunk mode. Notice that the mode changed from desirable to on. 
S2# show interfaces trunk 
c. Modify the trunk configuration on both switches by changing the native VLAN from VLAN 1 to VLAN 1000. 
S1(config)# interface f0/1 
S1(config-if)# switchport trunk native vlan 1000 
d. Issue the show interfaces trunk command to view the trunk. Notice the Native VLAN information is updated. 
S2# show interfaces trunk 
Questions: 
Why might you want to manually configure an interface to trunk mode instead of using DTP? 
Type your answers here. 
Why might you want to change the native VLAN on a trunk? 

Part 5: Delete the VLAN Database 
In Part 5, you will delete the VLAN Database from the switch. It is necessary to do this when initialising a switch back to its default settings. 
Step 1: Determine if the VLAN database exists. 
Open configuration window 
Issue the show flash command to determine if a vlan.dat file exists in flash. 
S1# show flash: 
Note: If there is a vlan.dat file located in flash, then the VLAN database does not contain its default settings. 
Step 2: Delete the VLAN database. 
a. Issue the delete vlan.dat command to delete the vlan.dat file from flash and reset the VLAN database back to its default settings. You will be prompted twice to confirm that you want to delete the vlan.dat file. Press Enter both times. 
S1# delete vlan.dat 
Delete filename [vlan.dat]?  
Delete flash:/vlan.dat? [confirm] 
b. Issue the show flash command to verify that the vlan.dat file has been deleted. 
S1# show flash: 
Question: 
c.	 INITIALISE THE SWITCHES 

To initialise each switch back to its default settings, clear the configuration from each switch with the command:
Erase start
At the prompt: 
Erasing the nvram filesystem will remove all configuration files! Continue? [confirm]
Press the Enter/Return Key to confirm. 

The following message confirms all is reset: 
[OK]
Erase of nvram: complete
%SYS-7-NV_BLOCK_INIT: Initialized the geometry of nvram

Type Do this for all switches.

Reflection Questions 
1. What is needed to allow hosts on VLAN 10 to communicate to hosts on VLAN 99? 
Type your answers here. 
2. What are some primary benefits that an organisation can receive through effective use of VLANs? 
Type your answers here. 
End of Document 

Type your answers here. 
Close configuration window 
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