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Replacing the Drum Unit - IRAVD C33XX-C35XX
6RCR-0L6
When the drum unit is near the end of life, a message will show in the bottom of the screen requesting the part be replaced. Press the icon on the bottom right corner of the screen and follow the instructions to replace the drum unit. 
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How to replace the Drum Unit



	IMPORTANT

	Keep the drum units away from light sources (like direct sunlight).
Keeping the drum unit in a room with sudden changes in temperature causes droplets (condensation) to form 
inside the part.
Do not remove the protective orange cover until receiving instructions to do so on the following procedure.

	NOTE

	To see the model number of the drum unit check Spare Parts.
The message to replace the drum unit shown in the bottom part of the screen changes according to your 
entitlement.
Press <Close> when finished replacing the drum unit.
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Changing drum unit procedure
When doing the following procedure, the screen also shows the instructions to replace the drum unit, which are useful to make sure you are doing it correctly.

1
Open the front panel of the main unit.
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2
Open the door of the drum unit.
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3
Pull the drum unit out.
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Important:
Remove the drum unit supporting it with your hands, as shown in the picture. Do not tilt it. It might spill the toner within.
4
Remove the new drum unit from the box.
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5
Install the new drum unit.
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6
Remove the protective lid.
First, push the sliding part on the right side of the orange protective cover towards the back part of the main unit until you can’t push anymore, then remove the protective cover.
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7
Close the drum unit door.



8
Close the front panel of the main unit.
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