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	Contract Name:
	Single two story detached building with loft

	Method Statement Title:
	Blockwork 

	Activity Start Date on Site:
	06/05/2020

	
	Signature:
	D.matthews

	Method Statement 

Prepared by: 
	Dylan Matthews
	Date:
	25/04/2020


	Title:
	Two Storey detached building with loft blockwork method

	
	

	Risk Assessment
	 See Risk Assessment  Hazards and Control Measures as Attached. 

	Scope of Works
	This Method Statement defines the sequence and describes the control procedures to be followed for Architectural Finishes Blockworks. The purpose of this Method Statement is to establish the rules to be applied during all the types of masonry block works

	Plant & Equipment
	•
110v transformer and leads.

•
Small tools.

•
Mobile scaffolding and Steps.

•
Trowels. Dumpy Levels

•
Hammers and chisels

•
Disc Cutter.

•
Tin Snips

	Methodology
	Blockwork Methodology  
The sequence of the works shall carry out to the approved programme of works, which are to be issued on site.  Check with the Client that work can commence and that all unauthorised persons are off site/ out of building.  Ensure that the work area is adequately identified and that suitable signage is posted and visible.

Isolation of Services.

Ensure that isolation of all the services within the location of the proposed working area is completed prior to work commencing.  This work will be carried out by suitably trained, competent and certificated persons.

Storage of Materials

The bricks and blocks required for the works will be transported from their storage area to the area of the work by mechanical means where practical or operatives will use a barrow to transport the materials to the working area. Blocks for the liftshaft are stored on pallets and equally distributed across the three floors. They are stored next to the lift shaft work area. The bricks for the plinth are stored in the storage area and are to be brought over to the work area using the telehander as work progresses.

Preparing the Mortar.

The mortar used within the construction process will be mixed outside the building and will transported from the mixing area to the working area by mechanical means or by barrow and will be set down adjacent to the working area.  The mortar will come in tubs or barrow for easy transportation around site.

Laying the Bricks and Blocks.

The blocks will then be laid using trowels, plumb lines and dumpy levels. For the blockwork plinth, a layer of 100mm insulation is to be installed between the concrete slab and new brickwork. The blockwork and associated block work will be built up to the required level or halted for the installation of the scaffolding, to provide a working platform for the remaining courses to be laid.

Regular checks are to be made for line, level and plumb with the ASL site engineer.



	First Aid  &  PPE
	PPE
Mandatory 

· Safety Helmet EN397

· High Visibility Jacket or Vest 

· Safety Footwear 

· Gloves 

All works shall comply with safety procedure or instruction set out in project safety plan and municipality rules and regulations.

Basic PPE to be worn by all staff and laborers.

Trained operator and banksman would be engaged to control or operate heavy equipment machine.

Provide sufficient lighting whenever night casting.
 

	Environment
	Spill kits will be readily available during works so any spillages can be contained and dealt with.
Any materials used on site which have been identified within their product data sheet to have the potential to harm the environment will be stored in accordance with the procedures outlined within the relevant data sheet and COSHH Assessment.

COSHH assessments will be undertaken for the relevant materials and will accompany this Method Statement.  Where required spill kits will be made available for use on site and any drains with the potential to be contaminated will be covered and protected.



	Emergency  Procedures
	· All personnel to sign in/out when leaving site.

· Assembly point at site access gate

· Nearest A&E Hospital: 
Morriston Hospital 
· Report all accidents/incidents to site supervisor immediately so it can be recorded.

· In the event of a spillage contain the area using a spill Kit and report to the site supervisor immediately.

· Spill kits are sited in site compound.



