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	Site Specific Activity and Control Measures        
                                     (This section must be completed)

	Method
	Storage , Mixing & Use by Hand tools

	
	Location
	General Site

	
	Duration
	Various stages during contract duration

	
	Control
	Assessment included in RA/MP’s briefing

	Exposure Limits
	OEL 5mg/m3 8hr TWA


	Physical Properties
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	Contains calcium silicates, aluminates and sulphates, small quantities of alkali, lime and chlorides, trace quantities of chromium compounds, may contain pulverised fuel ash or granulated blast furnace slag

	Hazard
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	Risk of serious damage to eyes
Contact with wet cement or mortar may cause irritation, dermatitis or burns

	
	
	Contact with dry cement powder and sweat or eye fluids may  cause irritation, dermatitis or burns
Possible skin sensitisation from chromates in cement. 
Prolonged inhalation (dust) can lead to long term lung damage

	Work Procedures/PPE
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	Ensure adequate ventilation
Avoid creation of airborne dust. Keep skin covered, wear impervious heavy duty gloves (BS EN 374, 388), rubber boots, overalls, eye protection (BS EN166 F).
Maintain high standard of personnel hygiene
Restrict public access during mixing, application and until set.

	First Aid/Fire
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	Inhalation: remove to fresh air and rest, seek medical attention if irritation persists
Ingestion: do not induce vomiting, drink plenty of water, seek medical attention
Eye Contact: irrigate with plenty of water, seek medical attention
Skin Contact: wash with plenty of soap and water immediately, remove contaminated clothing, seek medical attention if irritation persists
Fire: non-combustible

	Storage/Disposal
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	Storage: in a cool dry place

Disposal: in accordance with legislative and company requirements

	Environmental
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	Keep away from drains, watercourses etc.
Do not allow airborne pollution/ground contamination/leaching into water supplies/boreholes etc.
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