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Lab - Building an Ethernet Crossover Cable
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Lab – Understanding Ethernet Cable Standards 
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Addressing Table
	Device
	Interface
	IP Address
	Subnet Mask
	Default Gateway

	PC-A
	NIC
	192.168.10.1
	255.255.255.0
	N/A

	PC-B
	NIC
	192.168.10.2
	255.255.255.0
	N/A


Objectives
Part 1: Analyze Ethernet Cabling Standards and Pinouts
Part 2: Build an Ethernet Crossover Cable
Part 3: Test an Ethernet Crossover Cable
Background / Scenario
In this lab, you will build and terminate an Ethernet crossover cable and test it by connecting two PCs together and pinging between them. You will first analyze the Telecommunications Industry Association/Electronic Industries Association (TIA/EIA) 568-A and 568-B standards and how they apply to Ethernet cables. You will then construct an Ethernet crossover cable and test it. Finally, you will use the cable you just constructed to connect two PCs together and test it by pinging between them.
Note: With autosensing capabilities available on many devices, such as the Cisco 1941 Integrated Services Router (ISR) switch, you may see straight-through cables connecting like devices.
Required Resources
One length of cable, either Category 5 or 5e. Cable length should be 0.6 to 0.9m (2 to 3 ft.)
2 RJ-45 connectors
RJ-45 crimping tool
Wire cutter
Wire stripper
Ethernet cable tester (optional)
2 PCs (Windows 7 or 8)
Analyze Ethernet Cabling Standards and Pinouts
The TIA/EIA has specified unshielded twisted pair (UTP) cabling standards for use in LAN cabling environments. TIA/EIA 568-A and 568-B stipulates the commercial cabling standards for LAN installations; these are the standards most commonly used in LAN cabling for organizations and they determine which color wire is used on each pin.
With a crossover cable, the second and third pairs on the RJ-45 connector at one end of the cable are reversed at the other end, which reverses the send and receive pairs. The cable pinouts are the 568-A standard on one end and the 568-B standard on the other end. Crossover cables are normally used to connect hubs to hubs or switches to switches, but they can also be used to directly connect two hosts to create a simple network.
Reflection: 
Write a research report (Max word count 600) on Cat 5e and 6 Ethernet cable standards.  
This research report will discuss the main comparisons between the CAT 5E cable and CAT 6 cable. This will be accomplished through including the cable support which CAT 5E and CAT 6 cables as well as the speed that these cables run at. This report will also compare such cables through addressing the Signal to Noise ratio which both of these cables are operated at.
	It is considered that the most noticeable comparison is the maximum bandwidth of each cable. For instance, the CAT 5e cable carries a bandwidth of up to 100MHz, whereas the CAT 6 doubles the CAT 5e cable bandwidth, with the CAT 6 having a maximum bandwidth of 200-250 MHz.[2] This difference in bandwidth is further discussed by Jack Field who quotes “A spline (or Longitudinal separator) being incorporated into the CAT 6 design”.[1] Through using this information, it suggests that the spline of these cables, has allowed them to become rigid, and thus transfer more MHz.[2] Therefore meaning that this could be a possible reason to why CAT 6 has an improved Bandwidth. [2]
	Alternatively, another comparison between CAT 5E and CAT6 Cables is the level of support that they offer Ethernet.[1] This is clearly exemplified through the fact that CAT 5e can support 10BASE-T (Ethernet), Full Duplex 100BASE-TX (Fast Ethernet) and 1000BASE-T (also known as Gigabit Ethernet).[3] On the other hand, CAT 6 cables support up to the 10GBASE-T (10-Gigabit Ethernet). Due to what the cables can support the CAT 5e is rated at 1Gbps up to 55m and the CAT 6 is rated at 10Gbps up to 55m.[3]
	In addition to this, there is also different Signal to Noise ratio between CAT 5E and Cat 6 cables. [1] This is supported through the Signal to Noise ratio was 12db (or 16 times) better than the results than a 5e cable, when it is compared over a wide frequency radio. [1] It is also suggested that the CAT 6 had a lower cross talk, and thus helps for it to be major difference when comparing these cables. 
It should also be suggested that there are some similarities, between CAT 5E and CAT 6 cables. [2] This is clear through them both having backwards compatibility, meaning both of the cables are compatible with CAT 5 and CAT 3. [2] It should also be considered that CAT 6 is also backwards compatible with CAT 5e. Furthermore, both CAT 5e and CAT 6 use 4 twisted pairs in each cable that incorporate copper wires.[2]
	In conclusion, it is clear that the CAT 6 cable is a big improvement on the CAT 5e cables. This is most prominent through the fact that it can support a much larger bandwidth than the previous CAT 5e Cable.[2] Moreover, the CAT 6 cables is also able to support higher LAN ethernets cables compared to the CAT 5e cable.[1]  Despite such differences, which have been outlined within my research report, there is also some similarities, between the two cables, such as them both being able to support backwards compatibility. [2] It should also be noted that they are able to support higher LAN ethernets. [3] This research report has highlighted the main differences and similarities between the two cables, however it can be hoped that with further research the comparisons between CAT 5e and CAT 6 cables can continue to expand. 
Analyze diagrams and tables for the TIA/EIA 568-A standard Ethernet cable.
The following table and diagrams display the color scheme and pinouts, as well as the function of the four pairs of wires used for the 568-A standard. 
Note: In LAN installations using 100Base-T (100 Mb/s), only two pairs out of the four are used.
568-A 10/100/1000Base-TX Ethernet
	Pin Number
	Pair Number
	Wire Color
	10Base-T Signal
100Base-TX Signal
	1000Base-T Signal

	1
	2
	White/Green
	Transmit
	BI_DA+

	2
	2
	Green
	Transmit
	BI_DA-

	3
	3
	White/Orange
	Receive
	BI_DB+

	4
	1
	Blue
	Not Used
	BI_DC+

	5
	1
	White/Blue
	Not Used
	BI_DC-

	6
	3
	Orange
	Receive
	BI_DB-

	7
	4
	White/Brown
	Not Used
	BI_DD+

	8
	4
	Brown
	Not Used
	BI_DD-




The following diagrams display how the wire color and pinouts align with an RJ-45 jack for the 568-A standard.
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Analyze diagrams and tables for the TIA/EIA 568-B standard Ethernet cable.
The following table and diagram display the color scheme and pinouts for the 568-B standard.
568-B 10/100/1000-BaseTX Ethernet
	Pin Number
	Pair Number
	Wire Color
	10Base-T Signal
100Base-TX Signal
	1000Base-T Signal

	1
	2
	White/Orange
	Transmit
	BI_DA+

	2
	2
	Orange
	Transmit
	BI_DA-

	3
	3
	White/Green
	Receive
	BI_DB+

	4
	1
	Blue
	Not Used
	BI_DC+

	5
	1
	White/Blue
	Not Used
	BI_DC-

	6
	3
	Green
	Receive
	BI_DB-

	7
	4
	White/Brown
	Not Used
	BI_DD+

	8
	4
	Brown
	Not Used
	BI_DD-


[image: T568B_ColorPinout_AndRJ45Jack]


Build an Ethernet Crossover Cable
A crossover cable has the second and third pairs on the RJ-45 connector at one end, reversed at the other end (refer to the table in Part 1, Step 2). The cable pinouts are the 568-A standard on one end and the 568-B standard on the other end. The two following diagrams illustrate this concept.
[image: Cross_over_CableRJ45Connectors_1]
Build and terminate a TIA/EIA 568-A cable end.
Determine the cable length required. (Your instructor will let you know the cable length you should make.)
Note: If you were making a cable in a production environment, the general guideline is to add another 12 in. (30.48 cm) to the length.
Cut off a piece of cable to the desired length and using your wire stripper, remove 5.08 cm (2 in.) of the cable jacket from both ends.
Hold the four pairs of twisted cables tightly where the jacket was cut away. Reorganize the cable pairs into the order of the 568-A wiring standard. Refer to the diagrams, if necessary. Take as much care as possible to maintain the twists in the cable; this provides noise cancellation.
Flatten, straighten, and line up the wires using your thumb and forefinger.
Ensure that the cable wires are still in the correct order for the 568-A standard. Using your wire cutters, trim the four pairs in a straight line to within 1.25 to 1.9 cm (1/2 to 3/4 in.).
Place an RJ-45 connector on the end of your cable, with the prong on the underside pointing downward. Firmly insert the wires into the RJ-45 connector. All wires should be seen at the end of the connector in their proper positions. If the wires are not extending to the end of the connector, take the cable out, rearrange the wires as necessary, and reinsert the wires back into the RJ-45 connector.
If everything is correct, insert the RJ-45 connector with cable into the crimper. Crimp down hard enough to force the contacts on the RJ-45 connector through the insulation on the wires, thus completing the conducting path. See the following diagram for an example.
[image: crimp_Pic]
Build and terminate a TIA/EIA 568-B cable end.
Repeat steps 1a to 1g using the 568-B color wiring scheme for the other end.
Test an Ethernet Crossover Cable
Test the cable.
Many cable testers will test for length and mapping of wires. If the cable tester has a wire map feature, it verifies which pins on one end of the cable are connected to which pins on the other end.
If your instructor has a cable tester, test the crossover cable for functionality. If it fails, check with your instructor first as to whether you should re-cable the ends and re-test.
Connect two PCs together via NICs using your Ethernet crossover cable.
Working with a lab partner, set your PC to one of the IP addresses shown in the Addressing Table (see page 1). For example, if your PC is PC-A, your IP address should be set to 192.168.10.1 with a 24-bit subnet mask. You partner’s IP address should be 192.168.10.2. The default gateway address can be left empty.
Using the crossover cable you made, connect the two PCs together via their NICs.
On the PC-A command prompt, ping the PC-B IP address.
Note: The Windows firewall may have to be temporarily disabled for pings to be successful. If the firewall is disabled, make sure you re-enable it at the conclusion of this lab.
Repeat the process and ping from PC-B to PC-A.
Assuming IP addressing and firewall are not issues, your pings should be successful if the cables were properly made.
Reflection
Which part of making cables did you find the most difficult?
Making sure that the wires were in the correct order when pushing them into the plug
Why do you have to learn how to make a cable if you can easily buy pre-made cables?
There could be a standard or specialist cable which you may need that isn’t available.
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