	Activity to be Assessed
	Assessment Number
	

	Construction of Block and Block Wall
	10003
	

	Persons undertaking or affected by the activity
	

	
	

	
	Y
	Employees
	Y
	Contractor
	Y
	Public
	Y
	Service User
	

	
	

	
	Y
	Other: Principal Designer and Principle Contractor 
	

	Identified Hazards and Associated Risks
	Likelihood
	Severity
	Risk Level
	

	1
	Slips, trips and falls.
	4
	3
	12
	

	2
	Unsafe manual handling of tools and materials. 
	3
	3
	9
	

	3
	Falls from height.
	3
	5
	15
	

	4
	Working with hazardous materials.
	5
	3
	15
	

	5
	Unsafe use of hand held power tools
	4
	4
	16
	

	Existing Control Measures / Additional Control Measures Required
	

	1
	Slips, trips and falls from height can be avoided installing scaffolding to prevent people falling from the edge. Edge protection must be fit to the eaves of the roof, once constructed. A secure double guardrail and toeboard must be fit around the edge. Scaffolding walkways must be kept clear at all times. On the ground, tools, blocks and wheelbarrows must not obstruct walkways and the ground must be kept as clear as possible. Workers must regularly check for anything in their path that could cause a slip, trip or fall and remove that hazard of safe to do so. If it is not safe to do so, they should should stop work immediately, notify their colleagues and notify the site manager. Work will only then commence once the hazard has been dealt with.
	

	2
	To prevent unsafe manual handling of tools and materials the Manual Handling Operations Regulations 1992 must be followed. Workers must not carry unstable or unbalanced loads. Workers must not overreach or overexert when handling tools or materials. Workers must not exceed the maximum manual handling load of 25kg.
	

	3
	To prevent objects and people from falling from height, guardrails and toeboards must be used in the scaffolding. All tools and materials on the scaffolding should be secured where possible to prevent them falling on people below. Debris nets or catch platforms can be installed to help catch falling objects or people. To prevent unsafe access and egress, ladders should be used and fixed to the scaffold at the appropriate opening. Stair towers and fixed or mobile scaffold towers should be used. All openings should have a gate to prevent them from staying open when not in use. Where scaffolding is not available, then mobile access equipment should be used in strict accordance with the Lifting Operations and Lifting Equipment Regulations 1998 (LOLER) and a separate risk assessment for this must be carried out.
	

	4
	When working with hazardous materials workers must follow The Control of Substances Hazardous to Health Regulations 2002. This includes some dusts, such as concrete dust, especially in high concentrations. Also included are substances with WEL's (Workplace Exposure Limits). Masks should be worn when working with harmful dusts. Gloves must be worn when working with liquids that are an irritant or corrosive, specifically materials used for the making of cement. Correct PPE must be worn at all times. Choose products which are CE marked in accordance with the Personal Protective Equipment Regulations 2002.
	

	5
	Power tools, such as grinders and disc cutters, used for more than an hour a day by workers should be used with regular breaks to prevent Hand Arm Vibration (HAV). All equipment should be regularly checked and maintained following the Provision and Use of Work Equipment Regulations 1998. All correct PPE should be worn, including safety glasses or goggles, in accordance with the Personal Protective Equipment Regulations 2002.
	

	Reassessment of Activity Hazards 
	Likelihood
	Severity
	Risk Level
	

	1
	Slips, trips and falls.
	1
	2
	2
	

	2
	Unsafe manual handling of tools and materials. 
	1
	2
	2
	

	3
	Falls from height.
	2
	3
	6
	

	4
	Working with hazardous materials.
	5
	2
	10
	

	5
	Unsafe use of hand held power tools
	4
	4
	16
	

	Name  Lee Thomas

Position  Principle Designer
	Signed L. Thomas


	   Date of Completion: 19.04.2020
	

	Reviews
	Key
	
	

	Review Date: 
	Likelihood
	Severity
	Severity of Injury
	5
	5Y
	10R
	15
	20
	25

	Reviewed by: 
	1   very     unlikely

2   unlikely

3   likely

4   very likely

5   certainty
	1   nuisance

2   minor

3   medical treatment

4   major

5   fatal
	
	4
	4
	8
	12
	16
	20

	Review Date :
	
	
	
	3
	3
	6G
	9
	12
	15

	Reviewed by:
	
	
	
	2
	2
	4
	6Y
	8
	10Y

	Review Date :
	
	
	
	1
	1
	2
	3
	4
	5G

	Reviewed by:
	
	
	
	0
	1
	2
	3
	4
	5

	Review Date :
	
	
	
	Likelihood of Injury
	

	Reviewed by:
	
	
	
	Low Risk
	
	Medium Risk
	
	High Risk
	


