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Ping from R1 to R3 and ISP on both IPv4 and IPv6
Ping From PA3 IPv4 and IPv6 successful to the routers but not ISP (removing the ACL from R1 allows ping) not enough time to troubleshoot
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Ran out of time for the rest. I don’t think 2 hours is long enough for everything.
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