       ^
% Invalid input detected at '^' marker.

r1#enable secret cisco123
          ^
% Invalid input detected at '^' marker.

r1#config t
Enter configuration commands, one per line.  End with CNTL/Z.
r1(config)#ip domain-name swre-lab.com
                    ^
% Invalid input detected at '^' marker.

r1(config)#ip domain name swre-lab.com
r1(config)#enable secret cisco123
r1(config)#line console 0
r1(config-line)#password cisco123
r1(config-line)#login
r1(config-line)#exit
r1(config)#username cisco privilege 15 secret cisco123
r1(config)#
s1>
s1>
s1>en
s1#ip domain name swre-lab.com
       ^
% Invalid input detected at '^' marker.

s1#config t
Enter configuration commands, one per line.  End with CNTL/Z.
s1(config)#ip domain name swre-lab.com
s1(config)#enable secret cisco123
s1(config)#line console 0
s1(config-line)#password cisco123
s1(config-line)#login
s1(config-line)#exit
s1(config)#username cisco privilege 15 secret cisco123
s1(config)#
s2>
s2>
s2>
s2>
s2>en
s2#config t
Enter configuration commands, one per line.  End with CNTL/Z.
s2(config)#ip domain name swre-lab.com
s2(config)#enable secret cisco123
s2(config)#line console 0
s2(config-line)#password cisco123
s2(config-line)#login
s2(config-line)#exit
s2(config)#username cisco privilege 15 secret cisco123
s2(config)#line vty 0 4
s2(config-line)#login local
s2(config-line)#transport input ssh
s2(config-line)#exit
s2(config)#crypto key generate rsa
The name for the keys will be: s2.swre-lab.com
Choose the size of the key modulus in the range of 360 to 4096 for your
  General Purpose Keys. Choosing a key modulus greater than 512 may take
  a few minutes.

How many bits in the modulus [512]: 1024
% Generating 1024 bit RSA keys, keys will be non-exportable...
[OK] (elapsed time was 3 seconds)

s2(config)#
*Aug 22 11:25:57.313: %SSH-5-ENABLED: SSH 1.99 has been enabled
s2(config)#
r1(config)#line vty 0 4
r1(config-line)#login local
r1(config-line)#transport input ssh
r1(config-line)#exit
r1(config)#crypto key generate rsa
The name for the keys will be: r1.swre-lab.com
Choose the size of the key modulus in the range of 512 to 4096 for your
  General Purpose Keys. Choosing a key modulus greater than 512 may take
  a few minutes.

How many bits in the modulus [2048]: 1024
% Generating 1024 bit RSA keys, keys will be non-exportable...
[OK] (elapsed time was 1 seconds)

r1(config)#
*Aug 21 10:52:09.039: %CRYPTO_ENGINE-5-KEY_ADDITION: A key named r1.swre-lab.com has been generated or imported by crypto-engine
r1(config)#
s1(config)#
s1(config)#
s1(config)#line vty 0 4
s1(config-line)#login local
s1(config-line)#transport input ssh
s1(config-line)#exit
s1(config)#crypto key generate rsa
The name for the keys will be: s1.swre-lab.com
Choose the size of the key modulus in the range of 360 to 4096 for your
  General Purpose Keys. Choosing a key modulus greater than 512 may take
  a few minutes.

How many bits in the modulus [512]: 1024
% Generating 1024 bit RSA keys, keys will be non-exportable...
[OK] (elapsed time was 2 seconds)

s1(config)#
*Aug 22 11:53:07.836: %SSH-5-ENABLED: SSH 1.99 has been enabled
s1(config)#
s1(config)#vlan 7
s1(config-vlan)#name vlan 7
s1(config-vlan)#exit
s1(config)#vlan 8
s1(config-vlan)#name vlan 8
s1(config-vlan)#exit
s1(config)#vlan 10
s1(config-vlan)#name vlan 10
s1(config-vlan)#exit
s1(config)#vlan 11
s1(config-vlan)#name vlan 11
s1(config-vlan)#
s2(config)#
s2(config)#
s2(config)#
s2(config)#vlan 7
s2(config-vlan)#name vlan 7
s2(config-vlan)#exit
s2(config)#vlan 8
s2(config-vlan)#name vlan 8
s2(config-vlan)#exit
s2(config)#vlan 10
s2(config-vlan)#name vlan 10
s2(config-vlan)#exit
s2(config)#vlan 11
s2(config-vlan)#name vlan 11
s2(config-vlan)#exit
s2(config)#interface f0/1
                      ^
% Invalid input detected at '^' marker.

s2(config)#interface fast ethernet 0/1
                      ^
% Invalid input detected at '^' marker.

s2(config)#interface fastethernet 0/1
                      ^
% Invalid input detected at '^' marker.

s2(config)#interface fethernet 0/1
                      ^
% Invalid input detected at '^' marker.

s2(config)#interface fethernet0/1
                      ^
% Invalid input detected at '^' marker.

s2(config)#interface fastethernet0/1
                      ^
% Invalid input detected at '^' marker.

s2(config)#interfa
*Aug 22 11:39:11.370: %LINEPROTO-5-UPDOWN: Line protocol on Interface GigabitEthernet1/0/18, changed state to downce
*Aug 22 11:39:12.371: %LINK-3-UPDOWN: Interface GigabitEthernet1/0/18, changed state to down
*Aug 22 11:39:15.212: %LINK-3-UPDOWN: Interface GigabitEthernet1/0/18, changed state to up
*Aug 22 11:39:16.212: %LINEPROTO-5-UPDOWN: Line protocol on Interface GigabitEthernet1/0/18, changed state to up
% Incomplete command.

s2(config)#interface fastethernet0/1
                      ^
% Invalid input detected at '^' marker.

s2(config)#interface F0/1
                      ^
% Invalid input detected at '^' marker.

s2(config)#interface f0/1
                      ^
% Invalid input detected at '^' marker.

s2(config)#interface range F0/1-2
                           ^
% Invalid input detected at '^' marker.

s2(config)#channel-group 1 mode active
            ^
% Invalid input detected at '^' marker.

s2(config)#interface port-chanel 1
                              ^
% Invalid input detected at '^' marker.

s2(config)#switchmode port trunk..
                 ^
% Invalid input detected at '^' marker.

s2(config)#switchport mode trunk..~
                 ^
% Invalid input detected at '^' marker.

s2(config)#s1s1
            ^
% Invalid input detected at '^' marker.

s2(config)#

































s2 con0 is now available





Press RETURN to get started.



*Aug 22 11:55:40.140: %SYS-5-CONFIG_I: Configured from console by console

User Access Verification

Password:
Password:
s2>en
Password:
s2#config t
Enter configuration commands, one per line.  End with CNTL/Z.
s2(config)#int
s2(config)#interface
s2(config)#interface f
s2(config)#interface f
s2(config)#interface f
s2(config)#interface f
s2(config)#interface range fastethernet0/1-2
                           ^
% Invalid input detected at '^' marker.

s2(config)#interface range fastethernet0/1-2 ?
% Unrecognized command
s2(config)#interface range fastethernet0/1-2 ?
% Unrecognized command
s2(config)#interface range fastethernet?
% Unrecognized command
s2(config)#interface range F0/1-2
                           ^
% Invalid input detected at '^' marker.

s2(config)#interface range F0/1-2?
% Unrecognized command
s2(config)#interface range ?
  GigabitEthernet  GigabitEthernet IEEE 802.3z
  Loopback         Loopback interface
  Port-channel     Ethernet Channel of interfaces
  Tunnel           Tunnel interface
  Vlan             Catalyst Vlans
  macro            macro keyword

s2(config)#interface range
% Incomplete command.

s2(config)#interface range gigabitethernet0/1-2
                                          ^
% Invalid input detected at '^' marker.

s2(config)#interface range gigabitethernet 0/1-2
                                           ^
% Invalid input detected at '^' marker.

s2(config)#interface range gigabitethernet ?
  <1-8>  GigabitEthernet interface number

s2(config)#interface range gigabitethernet1-2
                                           ^
% Invalid input detected at '^' marker.

s2(config)#interface range gigabitethernet0/1-2
                                          ^
% Invalid input detected at '^' marker.

s2(config)#interface range gigabitethernet 0/1-2
                                           ^
% Invalid input detected at '^' marker.

s2(config)#interface gigabitethernet 0/1
                                     ^
% Invalid input detected at '^' marker.

s2(config)#interface gigabitethernet 0/0/6
                                     ^
% Invalid input detected at '^' marker.

s2(config)#interface gigabitethernet0/0/6
                                    ^
% Invalid input detected at '^' marker.

s2(config)#interface gigabitethernet0/6/0
                                    ^
% Invalid input detected at '^' marker.

s2(config)#interface gigabitethernet 0/6/0
                                     ^
% Invalid input detected at '^' marker.

s2(config)#interface gigabitethernet 0/6
                                     ^
% Invalid input detected at '^' marker.

s2(config)#interface gigabitethernet 0/6
                                     ^
% Invalid input detected at '^' marker.

s2(config)#end
s2#
*Aug 22 12:05:10.385: %SYS-5-CONFIG_I: Configured from console by console
s2#show ip interface brief
Interface              IP-Address      OK? Method Status                Protocol
Vlan1                  unassigned      YES unset  up                    up
GigabitEthernet1/0/1   unassigned      YES unset  up                    up
GigabitEthernet1/0/2   unassigned      YES unset  up                    up
GigabitEthernet1/0/3   unassigned      YES unset  down                  down
GigabitEthernet1/0/4   unassigned      YES unset  down                  down
GigabitEthernet1/0/5   unassigned      YES unset  down                  down
GigabitEthernet1/0/6   unassigned      YES unset  down                  down
GigabitEthernet1/0/7   unassigned      YES unset  down                  down
GigabitEthernet1/0/8   unassigned      YES unset  down                  down
GigabitEthernet1/0/9   unassigned      YES unset  down                  down
GigabitEthernet1/0/10  unassigned      YES unset  down                  down
GigabitEthernet1/0/11  unassigned      YES unset  down                  down
GigabitEthernet1/0/12  unassigned      YES unset  down                  down
GigabitEthernet1/0/13  unassigned      YES unset  down                  down
GigabitEthernet1/0/14  unassigned      YES unset  down                  down
GigabitEthernet1/0/15  unassigned      YES unset  down                  down
GigabitEthernet1/0/16  unassigned      YES unset  down                  down
GigabitEthernet1/0/17  unassigned      YES unset  down                  down
GigabitEthernet1/0/18  unassigned      YES unset  up                    up
GigabitEthernet1/0/19  unassigned      YES unset  down                  down
GigabitEthernet1/0/20  unassigned      YES unset  down                  down
GigabitEthernet1/0/21  unassigned      YES unset  down                  down
GigabitEthernet1/0/22  unassigned      YES unset  down                  down
GigabitEthernet1/0/23  unassigned      YES unset  down                  down
GigabitEthernet1/0/24  unassigned      YES unset  down                  down
GigabitEthernet1/0/25  unassigned      YES unset  down                  down

s2#config
Configuring from terminal, memory, or network [terminal]?
Enter configuration commands, one per line.  End with CNTL/Z.
s2(config)#interface gigabitethernet 1/0/6
s2(config-if)#channel-group 1 mode active
Creating a port-channel interface Port-channel 1

s2(config-if)#interface port-channel 1
s2(config-if)#switchport mode trunk
s2(config-if)#no channel-group 1 mode active
                  ^
% Invalid input detected at '^' marker.

s2(config-if)#no switchport mode trunk
s2(config-if)#exit
s2(config)#interface gigabitethernet 1/0/18
s2(config-if)#channel-group 1 mode active
s2(config-if)#
*Aug 22 12:11:29.514: %LINEPROTO-5-UPDOWN: Line protocol on Interface GigabitEthernet1/0/18, changed state to down
s2(config-if)#
*Aug 22 12:11:36.520: %EC-5-L3DONTBNDL2: Gi1/0/18 suspended: LACP currently not enabled on the remote port.
s2(config-if)#interface port-channel 1
s2(config-if)#switchport mode trunk
s2(config-if)#

User Access Verification

Password:
Password:
Password:
% Bad passwords


































s1 con0 is now available





Press RETURN to get started.




User Access Verification

Password:
s1>en
Password:
s1#config t
Enter configuration commands, one per line.  End with CNTL/Z.
s1(config)#interface range gigabitethernet 1/0/1-2
s1(config-if-range)#channel-group 1 mode active
Creating a port-channel interface Port-channel 1

s1(config-if-range)#
*Aug 22 12:37:48.247: %LINEPROTO-5-UPDOWN: Line protocol on Interface GigabitEthernet1/0/1, changed state to down
*Aug 22 12:37:48.307: %LINEPROTO-5-UPDOWN: Line protocol on Interface GigabitEthernet1/0/2, changed state to down
*Aug 22 12:37:55.135: %EC-5-L3DONTBNDL2: Gi1/0/2 suspended: LACP currently not enabled on the remote port.
*Aug 22 12:37:56.163: %EC-5-L3DONTBNDL2: Gi1/0/1 suspended: LACP currently not enabled on the remote port.
s1(config-if-range)#interface port-channel 1
s1(config-if)#switchport mode trunk
s1(config-if)#
s2(config-if)#
s2(config-if)#exit
s2(config)#interface gigab
*Aug 22 12:16:27.015: %LINEPROTO-5-UPDOWN: Line protocol on Interface Vlan1, changed state to upitethernet
% Incomplete command.

s2(config)#
s2(config)#interface range gigabitethernet 1/0/1-2
s2(config-if-range)#channel-group 1 mode active
s2(config-if-range)#
*Aug 22 12:17:33.396: %EC-5-CANNOT_BUNDLE2: Gi1/0/1 is not compatible with Gi1/0/18 and will be suspended (speed of Gi1/0/1 is 1000M, Gi1/0/18 is 100M)
*Aug 22 12:17:33.463: %EC-5-CANNOT_BUNDLE2: Gi1/0/2 is not compatible with Gi1/0/18 and will be suspended (speed of Gi1/0/2 is 1000M, Gi1/0/18 is 100M)
*Aug 22 12:17:33.478: %LINEPROTO-5-UPDOWN: Line protocol on Interface Vlan1, changed state to down
*Aug 22 12:17:34.389: %LINEPROTO-5-UPDOWN: Line protocol on Interface GigabitEthernet1/0/1, changed state to down
*Aug 22 12:17:34.456: %LINEPROTO-5-UPDOWN: Line protocol on Interface GigabitEthernet1/0/2, changed state to down
s2(config-if-range)#interface port-channel 1
s2(config-if)#switchport mode trunk
s2(config-if)#exit
s2(config)#interface gigabitethernet 1/0/6
s2(config-if)#no channel-group 1 mode active
s2(config-if)#no switchport mode trunk
s2(config-if)#
s2(config-if)#exit
s2(config)#interface gigabitethernet 1/0/6
s2(config-if)#switchport mode access
s2(config-if)#switchport access vlan7
                                    ^
% Invalid input detected at '^' marker.

s2(config-if)#switchport access vlan 7
s2(config-if)#
s1(config-if)#exit
s1(config)#interface gigabitethernet 1/0/6
s1(config-if)#switchport mode access
s1(config-if)#switchport access vlan 7
s1(config-if)#interface gigab
% Incomplete command.

s2(config)#
s2(config)#
s2(config)#interface gigabitethernet 1/0/6
s2(config-if)#switchport mode access
s2(config-if)#no switchport access vlan 7
s2(config-if)#exit
s2(config)#interface gigabitethernet 1/0/18
s2(config-if)#switchport mode access
s2(config-if)#
*Aug 22 12:24:28.940: %EC-5-COMPATIBLE: Gi1/0/1 is compatible with port-channel members
*Aug 22 12:24:28.941: %EC-5-COMPATIBLE: Gi1/0/2 is compatible with port-channel members
*Aug 22 12:24:28.942: %EC-5-CANNOT_BUNDLE2: Gi1/0/18 is not compatible with Po1 and will be suspended (dtp mode of Gi1/0/18 is off, Po1 is on)
*Aug 22 12:24:28.944: %EC-5-CANNOT_BUNDLE2: Gi1/0/18 is not compatible with Po1 and will be suspended (dtp mode of Gi1/0/18 is off, Po1 is on)
*Aug 22 12:24:28.944: %EC-5-CANNOT_BUNDLE2: Gi1/0/18 is not compatible with Po1 and will be suspended (dtp mode of Gi1/0/18 is off, Po1 is on)
*Aug 22 12:24:30.866: %LINEPROTO-5-UPDOWN: Line protocol on Interface Vlan1, changed state to up
*Aug 22 12:24:31.847: %LINEPROTO-5-UPDOWN: Line protocol on Interface GigabitEthernet1/0/1, changed state to up
*Aug 22 12:24:32.840: %LINK-3-UPDOWN: Interface Port-channel1, changed state to up
*Aug 22 12:24:33.840: %LINEPROTO-5-UPDOWN: Line protocol on Interface Port-channel1, changed state to up
*Aug 22 12:24:35.840: %LINEPROTO-5-UPDOWN: Line protocol on Interface GigabitEthernet1/0/2, changed state to up
s2(config-if)#switchport access vlan 8
s2(config-if)#e
*Aug 22 12:24:53.553: %EC-5-CANNOT_BUNDLE2: Gi1/0/18 is not compatible with Gi1/0/1 and will be suspended (dtp mode of Gi1/0/18 is off, Gi1/0/1 is on)xit
s2(config)#
s2(config)#interface gigabitethernet 1/0/6
s1(config-if)#switchport port-security
s1(config-if)#switchport max 3
                          ^
% Invalid input detected at '^' marker.

s1(config-if)#switchport maximum 3
                          ^
% Invalid input detected at '^' marker.

s1(config-if)#switchport max?
% Unrecognized command
s1(config-if)#switchport ?
  access         Set access mode characteristics of the interface
  autostate      Include or exclude this port from vlan link up calculation
  block          Disable forwarding of unknown uni/multi cast addresses
  host           Set port host
  mode           Set trunking mode of the interface
  nonegotiate    Device will not engage in negotiation protocol on this
                 interface
  port-security  Security related command
  priority       Set appliance 802.1p priority
  private-vlan   Set the private VLAN configuration
  protected      Configure an interface to be a protected port
  trunk          Set trunking characteristics of the interface
  voice          Voice appliance attributes
  <cr>

s1(config-if)#switchport
s1(config-if)#maximum 3
                ^
% Invalid input detected at '^' marker.

s1(config-if)#max 3
                ^
% Invalid input detected at '^' marker.

s1(config-if)#switchport m 3
                           ^
% Invalid input detected at '^' marker.

s1(config-if)#exit
s1(config)#show ip config
             ^
% Invalid input detected at '^' marker.

s1(config)#end
s1#sho
*Aug 22 12:54:24.610: %SYS-5-CONFIG_I: Configured from console by consolew ip interface brief
Interface              IP-Address      OK? Method Status                Protocol
Vlan1                  unassigned      YES unset  administratively down down
GigabitEthernet1/0/1   unassigned      YES unset  up                    up
GigabitEthernet1/0/2   unassigned      YES unset  up                    up
GigabitEthernet1/0/3   unassigned      YES unset  down                  down
GigabitEthernet1/0/4   unassigned      YES unset  down                  down
GigabitEthernet1/0/5   unassigned      YES unset  down                  down
GigabitEthernet1/0/6   unassigned      YES unset  up                    up
GigabitEthernet1/0/7   unassigned      YES unset  down                  down
GigabitEthernet1/0/8   unassigned      YES unset  down                  down
GigabitEthernet1/0/9   unassigned      YES unset  down                  down
GigabitEthernet1/0/10  unassigned      YES unset  down                  down
GigabitEthernet1/0/11  unassigned      YES unset  down                  down
GigabitEthernet1/0/12  unassigned      YES unset  down                  down
GigabitEthernet1/0/13  unassigned      YES unset  down                  down
GigabitEthernet1/0/14  unassigned      YES unset  down                  down
GigabitEthernet1/0/15  unassigned      YES unset  down                  down
GigabitEthernet1/0/16  unassigned      YES unset  down                  down
GigabitEthernet1/0/17  unassigned      YES unset  down                  down
GigabitEthernet1/0/18  unassigned      YES unset  down                  down
GigabitEthernet1/0/19  unassigned      YES unset  down                  down
GigabitEthernet1/0/20  unassigned      YES unset  down                  down
GigabitEthernet1/0/21  unassigned      YES unset  down                  down
GigabitEthernet1/0/22  unassigned      YES unset  down                  down
GigabitEthernet1/0/23  unassigned      YES unset  down                  down
GigabitEthernet1/0/24  unassigned      YES unset  down                  down
GigabitEthernet1/0/25  unassigned      YES unset  down                  down
GigabitEthernet1/0/26  unassigned      YES unset  down                  down
GigabitEthernet1/0/27  unassigned      YES unset  down                  down
GigabitEthernet1/0/28  unassigned      YES unset  down                  down
Port-channel1          unassigned      YES unset  up                    up
s1#
s1#
s1#config t
Enter configuration commands, one per line.  End with CNTL/Z.
s1(config)#interface range gigabitethernet 1/0/3-5, 1/0/7-28
                                                    ^
% Invalid input detected at '^' marker.

s1(config)#interface range gigabitethernet 1/0/3-5
s1(config-if-range)#switchport access vlan 10
s1(config-if-range)#shutdown
s1(config-if-range)#switchport access vlan 10
*Aug 22 12:57:26.552: %LINK-5-CHANGED: Interface GigabitEthernet1/0/3, changed state to administratively down
*Aug 22 12:57:26.554: %LINK-5-CHANGED: Interface GigabitEthernet1/0/4, changed state to administratively down
*Aug 22 12:57:26.556: %LINK-5-CHANGED: Interface GigabitEthernet1/0/5, changed stateinterface range gigabitethernet 1/0/3-5
s1(config-if-range)#
s1(config-if-range)#interface range gigabitethernet 1/0/7-28
s1(config-if-range)#switchport access vlan 10
s1(config-if-range)#shutdown
s1(config-if-range)#
*Aug 22 12:58:09.590: %LINK-5-CHANGED: Interface GigabitEthernet1/0/7, changed state to administratively down
*Aug 22 12:58:09.592: %LINK-5-CHANGED: Interface GigabitEthernet1/0/8, changed state to administratively down
*Aug 22 12:58:09.594: %LINK-5-CHANGED: Interface GigabitEthernet1/0/9, changed state to administratively down
*Aug 22 12:58:09.595: %LINK-5-CHANGED: Interface GigabitEthernet1/0/10, changed state to administratively down
*Aug 22 12:58:09.597: %LINK-5-CHANGED: Interface GigabitEthernet1/0/11, changed state to administratively down
*Aug 22 12:58:09.599: %LINK-5-CHANGED: Interface GigabitEthernet1/0/12, changed state to administratively down
*Aug 22 12:58:09.600: %LINK-5-CHANGED: Interface GigabitEthernet1/0/13, changed state to administratively down
*Aug 22 12:58:09.602: %LINK-5-CHANGED: Interface GigabitEthernet1/0/14, changed state to administratively down
*Aug 22 12:58:09.603: %LINK-5-CHANGED: Interface GigabitEthernet1/0/15, changed state to administratively down
*Aug 22 12:58:09.605: %LINK-5-CHANGED: Interface GigabitEthernet1/0/16, changed state to administratively down
*Aug 22 12:58:09.607: %LINK-5-CHANGED: Interface GigabitEthernet1/0/17, changed state to administratively down
*Aug 22 12:58:09.608: %LINK-5-CHANGED: Interface GigabitEthernet1/0/18, changed state to administratively down
*Aug 22 12:58:09.610: %LINK-5-CHANGED: Interface GigabitEthernet1/0/19, changed state to administratively down
*Aug 22 12:58:09.611: %LINK-5-CHANGED: Interface GigabitEthernet1/0/20, changed state to administratively down
*Aug 22 12:58:09.613: %LINK-5-CHANGED: Interface GigabitEthernet1/0/21, changed state to administratively down
*Aug 22 12:58:09.615: %LINK-5-CHANGED: Interface GigabitEthernet1/0/22, changed state to administratively down
*Aug 22 12:58:09.616: %LINK-5-CHANGED: Interface GigabitEthernet1/0/23, changed state to administratively down
*Aug 22 12:58:09.618: %LINK-5-CHANGED: Interface GigabitEthernet1/0/24, changed state to administratively down
*Aug 22 12:58:09.619: %LINK-5-CHANGED: Interface GigabitEthernet1/0/25, changed state to administratively down
*Aug 22 12:58:09.621: %LINK-5-CHANGED: Interface GigabitEthernet1/0/26, changed state to administratively down
*Aug 22 12:58:09.622: %LINK-5-CHANGED: Interface GigabitEthernet1/0/27, changed state to administratively down
*Aug 22 12:58:09.624: %LINK-5-CHANGED: Interface GigabitEthernet1/0/28, changed state to administratively down
s1(config-if-range)#
s1(config-if-range)#

User Access Verification

Password:
Password:
s2>en
Password:
s2#config t
Enter configuration commands, one per line.  End with CNTL/Z.
s2(config)#interface range gigabitethernet 1/0/3-17
s2(config-if-range)#switchport mode access
s2(config-if-range)#switchport access vlan 10
s2(config-if-range)#shutdown
s2(config-if-range)#
*Aug 22 12:36:53.020: %LINK-5-CHANGED: Interface GigabitEthernet1/0/3, changed state to administratively down
*Aug 22 12:36:53.022: %LINK-5-CHANGED: Interface GigabitEthernet1/0/4, changed state to administratively down
*Aug 22 12:36:53.024: %LINK-5-CHANGED: Interface GigabitEthernet1/0/5, changed state to administratively down
*Aug 22 12:36:53.025: %LINK-5-CHANGED: Interface GigabitEthernet1/0/6, changed state to administratively down
*Aug 22 12:36:53.027: %LINK-5-CHANGED: Interface GigabitEthernet1/0/7, changed state to administratively down
*Aug 22 12:36:53.028: %LINK-5-CHANGED: Interface GigabitEthernet1/0/8, changed state to administratively down
*Aug 22 12:36:53.030: %LINK-5-CHANGED: Interface GigabitEthernet1/0/9, changed state to administratively down
*Aug 22 12:36:53.032: %LINK-5-CHANGED: Interface GigabitEthernet1/0/10, changed state to administratively down
*Aug 22 12:36:53.033: %LINK-5-CHANGED: Interface GigabitEthernet1/0/11, changed state to administratively down
*Aug 22 12:36:53.035: %LINK-5-CHANGED: Interface GigabitEthernet1/0/12, changed state to administratively down
*Aug 22 12:36:53.036: %LINK-5-CHANGED: Interface GigabitEthernet1/0/13, changed state to administratively down
*Aug 22 12:36:53.038: %LINK-5-CHANGED: Interface GigabitEthernet1/0/14, changed state to administratively down
*Aug 22 12:36:53.039: %LINK-5-CHANGED: Interface GigabitEthernet1/0/15, changed state to administratively down
*Aug 22 12:36:53.041: %LINK-5-CHANGED: Interface GigabitEthernet1/0/16, changed state to administratively down
*Aug 22 12:36:53.043: %LINK-5-CHANGED: Interface GigabitEthernet1/0/17, changed state to administratively down
s2(config-if-range)#exit
s2(config)#interface range gigabitethernet 1/0/19-29
                                                   ^
% Invalid input detected at '^' marker.

s2(config)#interface range gigabitethernet 1/0/19-28
s2(config-if-range)#switchport mode access
s2(config-if-range)#switchport access vlan 10
s2(config-if-range)#shutdown
s2(config-if-range)#
*Aug 22 12:38:42.668: %LINK-5-CHANGED: Interface GigabitEthernet1/0/19, changed state to administratively down
*Aug 22 12:38:42.670: %LINK-5-CHANGED: Interface GigabitEthernet1/0/20, changed state to administratively down
*Aug 22 12:38:42.672: %LINK-5-CHANGED: Interface GigabitEthernet1/0/21, changed state to administratively down
*Aug 22 12:38:42.673: %LINK-5-CHANGED: Interface GigabitEthernet1/0/22, changed state to administratively down
*Aug 22 12:38:42.675: %LINK-5-CHANGED: Interface GigabitEthernet1/0/23, changed state to administratively down
*Aug 22 12:38:42.677: %LINK-5-CHANGED: Interface GigabitEthernet1/0/24, changed state to administratively down
*Aug 22 12:38:42.678: %LINK-5-CHANGED: Interface GigabitEthernet1/0/25, changed state to administratively down
*Aug 22 12:38:42.680: %LINK-5-CHANGED: Interface GigabitEthernet1/0/26, changed state to administratively down
*Aug 22 12:38:42.681: %LINK-5-CHANGED: Interface GigabitEthernet1/0/27, changed state to administratively down
*Aug 22 12:38:42.682: %LINK-5-CHANGED: Interface GigabitEthernet1/0/28, changed state to administratively down

User Access Verification

Password:
r1>en
Password:
r1#config t
Enter configuration commands, one per line.  End with CNTL/Z.
r1(config)#interface g 1/0/7
                       ^
% Invalid input detected at '^' marker.

r1(config)#interface gigabitethernet 1/0/7
                                     ^
% Invalid input detected at '^' marker.

r1(config)#interface 0/0/1
                     ^
% Invalid input detected at '^' marker.

r1(config)#interface g0/0/1
r1(config-if)#exit
r1(config)#interface g0/0/1
r1(config-if)#exit
r1(config)#interface g0/0/1.7
r1(config-subif)#encapsulation dot1q 1.7
                                      ^
% Invalid input detected at '^' marker.

r1(config-subif)#encapsulation dot1q 1,7
                                      ^
% Invalid input detected at '^' marker.

r1(config-subif)#encapsulation dot1q 1.7
                                      ^
% Invalid input detected at '^' marker.

r1(config-subif)#encapsulation dot1q 7
r1(config-subif)#ip address 192.168.20.1 255.255.255.0
r1(config-subif)#exit
r1(config)#interface g0/0/1.8
r1(config-subif)#encapsulation dot1q 8
r1(config-subif)#ip address 192.168.30.1 255.255.255.0
r1(config-subif)#interface g0/0/1.9
r1(config-subif)#encapsulation dot1q 9
r1(config-subif)#ip address 192.168.40.1 255.255.255.0
r1(config-subif)#exit
r1(config)#interface loopback 0
r1(config-if)#
*Aug 21 12:12:18.022: %LINEPROTO-5-UPDOWN: Line protocol on Interface Loopback0, changed state to up
r1(config-if)#ip address 209.165.201.1 255.255.255.0
r1(config-if)#exit
r1(config)#

User Access Verification

Password:
Password:
s1>en
Password:
s1#config t
Enter configuration commands, one per line.  End with CNTL/Z.
s1(config)#interface vlan 9
s1(config-if)#
*Aug 22 13:13:47.918: %LINEPROTO-5-UPDOWN: Line protocol on Interface Vlan9, changed state to downip address 192.168.40.2 255.255.255.0
s1(config-if)#no shut
s1(config-if)#

User Access Verification

Password:
Password:
Password:
s2>en
Password:
s2#
s2#config t
Enter configuration commands, one per line.  End with CNTL/Z.
s2(config)#interface vlan 9
s2(config-if)#i
*Aug 22 12:51:56.982: %LINEPROTO-5-UPDOWN: Line protocol on Interface Vlan9, changed state to downp address 192.168.40.3 255.255.255.0
s2(config-if)#no shutdown
s2(config-if)#exit
s2(config)#end
s2#
*Aug 22 12:53:17.334: %SYS-5-CONFIG_I: Configured from console by console
s2#
s2#show run
Building configuration...

Current configuration : 3639 bytes
!
! Last configuration change at 12:53:17 UTC Thu Aug 22 2024
!
version 15.2
no service pad
service timestamps debug datetime msec
service timestamps log datetime msec
no service password-encryption
!
hostname s2
!
boot-start-marker
boot-end-marker
!
enable secret 9 $9$p8BXnchizbAuS3$XySIzCW3gpR.v93A1f9WcO5WjPE3jH1OvcVRR3p41q6
!
username cisco privilege 15 secret 9 $9$eNKzI5zhj4ODi8$F67/k6d9ctN3BiEsIAnKeqLOFfxv1DZTEcVarEXh7WU
no aaa new-model
switch 1 provision c1000-24t-4g-l
system mtu routing 1500
!
!
ip domain-name swre-lab.com
!
!
!
!
!
!
!
!
spanning-tree mode rapid-pvst
spanning-tree extend system-id
!
vlan internal allocation policy ascending
!
!
!
!
!
!
interface Port-channel1
 switchport mode trunk
!
interface GigabitEthernet1/0/1
 switchport mode trunk
 channel-group 1 mode active
!
interface GigabitEthernet1/0/2
 switchport mode trunk
 channel-group 1 mode active
!
interface GigabitEthernet1/0/3
 switchport access vlan 10
 switchport mode access
 shutdown
!
interface GigabitEthernet1/0/4
 switchport access vlan 10
 switchport mode access
 shutdown
!
interface GigabitEthernet1/0/5
 switchport access vlan 10
 switchport mode access
 shutdown
!
interface GigabitEthernet1/0/6
 switchport access vlan 10
 switchport mode access
 shutdown
!
interface GigabitEthernet1/0/7
 switchport access vlan 10
 switchport mode access
 shutdown
!
interface GigabitEthernet1/0/8
 switchport access vlan 10
 switchport mode access
 shutdown
!
interface GigabitEthernet1/0/9
 switchport access vlan 10
 switchport mode access
 shutdown
!
interface GigabitEthernet1/0/10
 switchport access vlan 10
 switchport mode access
 shutdown
!
interface GigabitEthernet1/0/11
 switchport access vlan 10
 switchport mode access
 shutdown
!
interface GigabitEthernet1/0/12
 switchport access vlan 10
 switchport mode access
 shutdown
!
interface GigabitEthernet1/0/13
 switchport access vlan 10
 switchport mode access
 shutdown
!
interface GigabitEthernet1/0/14
 switchport access vlan 10
 switchport mode access
 shutdown
!
interface GigabitEthernet1/0/15
 switchport access vlan 10
 switchport mode access
 shutdown
!
interface GigabitEthernet1/0/16
 switchport access vlan 10
 switchport mode access
 shutdown
!
interface GigabitEthernet1/0/17
 switchport access vlan 10
 switchport mode access
 shutdown
!
interface GigabitEthernet1/0/18
 switchport access vlan 8
 switchport mode access
 channel-group 1 mode active
!
interface GigabitEthernet1/0/19
 switchport access vlan 10
 switchport mode access
 shutdown
!
interface GigabitEthernet1/0/20
 switchport access vlan 10
 switchport mode access
 shutdown
!
interface GigabitEthernet1/0/21
 switchport access vlan 10
 switchport mode access
 shutdown
!
interface GigabitEthernet1/0/22
 switchport access vlan 10
 switchport mode access
 shutdown
!
interface GigabitEthernet1/0/23
 switchport access vlan 10
 switchport mode access
 shutdown
!
interface GigabitEthernet1/0/24
 switchport access vlan 10
 switchport mode access
 shutdown
!
interface GigabitEthernet1/0/25
 switchport access vlan 10
 switchport mode access
 shutdown
!
interface GigabitEthernet1/0/26
 switchport access vlan 10
 switchport mode access
 shutdown
!
interface GigabitEthernet1/0/27
 switchport access vlan 10
 switchport mode access
 shutdown
!
interface GigabitEthernet1/0/28
 switchport access vlan 10
 switchport mode access
 shutdown
!
interface Vlan1
 no ip address
!
interface Vlan9
 ip address 192.168.40.3 255.255.255.0
!
ip http server
ip http secure-server
!
!
!
!
line con 0
 password cisco123
 login
line vty 0 4
 login local
 transport input ssh
line vty 5 15
 login
 transport input none
!
end
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s2#en
s2#show ip interface brief
Interface              IP-Address      OK? Method Status                Protocol
Vlan1                  unassigned      YES unset  up                    up
Vlan9                  192.168.40.3    YES manual down                  down
GigabitEthernet1/0/1   unassigned      YES unset  up                    up
GigabitEthernet1/0/2   unassigned      YES unset  up                    up
GigabitEthernet1/0/3   unassigned      YES unset  administratively down down
GigabitEthernet1/0/4   unassigned      YES unset  administratively down down
GigabitEthernet1/0/5   unassigned      YES unset  administratively down down
GigabitEthernet1/0/6   unassigned      YES unset  administratively down down
GigabitEthernet1/0/7   unassigned      YES unset  administratively down down
GigabitEthernet1/0/8   unassigned      YES unset  administratively down down
GigabitEthernet1/0/9   unassigned      YES unset  administratively down down
GigabitEthernet1/0/10  unassigned      YES unset  administratively down down
GigabitEthernet1/0/11  unassigned      YES unset  administratively down down
GigabitEthernet1/0/12  unassigned      YES unset  administratively down down
GigabitEthernet1/0/13  unassigned      YES unset  administratively down down
GigabitEthernet1/0/14  unassigned      YES unset  administratively down down
GigabitEthernet1/0/15  unassigned      YES unset  administratively down down
GigabitEthernet1/0/16  unassigned      YES unset  administratively down down
GigabitEthernet1/0/17  unassigned      YES unset  administratively down down
GigabitEthernet1/0/18  unassigned      YES unset  up                    down
GigabitEthernet1/0/19  unassigned      YES unset  administratively down down
GigabitEthernet1/0/20  unassigned      YES unset  administratively down down
GigabitEthernet1/0/21  unassigned      YES unset  administratively down down
GigabitEthernet1/0/22  unassigned      YES unset  administratively down down
GigabitEthernet1/0/23  unassigned      YES unset  administratively down down
GigabitEthernet1/0/24  unassigned      YES unset  administratively down down
GigabitEthernet1/0/25  unassigned      YES unset  administratively down down
GigabitEthernet1/0/26  unassigned      YES unset  administratively down down
GigabitEthernet1/0/27  unassigned      YES unset  administratively down down
GigabitEthernet1/0/28  unassigned      YES unset  administratively down down
Port-channel1          unassigned      YES unset  up                    up
s2#
s2#
s2#
s2#
s2#
s2#
s2#show vlan

VLAN Name                             Status    Ports
---- -------------------------------- --------- -------------------------------
1    default                          active
7    vlan 7                           active
8    vlan 8                           active    Gi1/0/18
10   vlan 10                          active    Gi1/0/3, Gi1/0/4, Gi1/0/5
                                                Gi1/0/6, Gi1/0/7, Gi1/0/8
                                                Gi1/0/9, Gi1/0/10, Gi1/0/11
                                                Gi1/0/12, Gi1/0/13, Gi1/0/14
                                                Gi1/0/15, Gi1/0/16, Gi1/0/17
                                                Gi1/0/19, Gi1/0/20, Gi1/0/21
                                                Gi1/0/22, Gi1/0/23, Gi1/0/24
                                                Gi1/0/25, Gi1/0/26, Gi1/0/27
                                                Gi1/0/28
11   vlan 11                          active
20   CarPark                          active
99   Management                       active
1000 Native                           active
1002 fddi-default                     act/unsup
1003 token-ring-default               act/unsup
1004 fddinet-default                  act/unsup
1005 trnet-default                    act/unsup

VLAN Type  SAID       MTU   Parent RingNo BridgeNo Stp  BrdgMode Trans1 Trans2
---- ----- ---------- ----- ------ ------ -------- ---- -------- ------ ------
1    enet  100001     1500  -      -      -        -    -        0      0
7    enet  100007     1500  -      -      -        -    -        0      0
8    enet  100008     1500  -      -      -        -    -        0      0
10   enet  100010     1500  -      -      -        -    -        0      0
11   enet  100011     1500  -      -      -        -    -        0      0
20   enet  100020     1500  -      -      -        -    -        0      0
99   enet  100099     1500  -      -      -        -    -        0      0
1000 enet  101000     1500  -      -      -        -    -        0      0
1002 fddi  101002     1500  -      -      -        -    -        0      0
1003 tr    101003     1500  -      -      -        -    -        0      0
1004 fdnet 101004     1500  -      -      -        ieee -        0      0
1005 trnet 101005     1500  -      -      -        ibm  -        0      0

Primary Secondary Type              Ports
------- --------- ----------------- ------------------------------------------
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s2#

User Access Verification

Password:
r1>en
Password:
r1#show run
Building configuration...

Current configuration : 6558 bytes
!
! Last configuration change at 12:23:02 UTC Wed Aug 21 2024
!
version 17.9
service timestamps debug datetime msec
service timestamps log datetime msec
! Call-home is enabled by Smart-Licensing.
service call-home
platform qfp utilization monitor load 80
platform punt-keepalive disable-kernel-core
!
hostname r1
!
boot-start-marker
boot-end-marker
!
!
no aaa new-model
!
!
!
!
!
!
!
no ip domain lookup
ip domain name swre-lab.com
!
!
!
login on-success log
!
!
!
!
!
!
!
subscriber templating
vtp version 1
multilink bundle-name authenticated
!
!
!
crypto pki trustpoint TP-self-signed-2610773630
 enrollment selfsigned
 subject-name cn=IOS-Self-Signed-Certificate-2610773630
 revocation-check none
 rsakeypair TP-self-signed-2610773630
!
crypto pki trustpoint SLA-TrustPoint
 enrollment pkcs12
 revocation-check crl
!
!
crypto pki certificate chain TP-self-signed-2610773630
 certificate self-signed 01
  30820330 30820218 A0030201 02020101 300D0609 2A864886 F70D0101 05050030
  31312F30 2D060355 04031326 494F532D 53656C66 2D536967 6E65642D 43657274
  69666963 6174652D 32363130 37373336 3330301E 170D3234 30383231 30373535
  35315A17 0D333430 38323130 37353535 315A3031 312F302D 06035504 03132649
  4F532D53 656C662D 5369676E 65642D43 65727469 66696361 74652D32 36313037
  37333633 30308201 22300D06 092A8648 86F70D01 01010500 0382010F 00308201
  0A028201 0100EF4C DE35DE17 7ADA818B A94B5ED9 FF3858D2 3BD2A789 4BEC493B
  94BD9D00 CEFBE998 B7E2B01D 56365AF9 CBD44A72 7C35280F 3E327CF6 781A5431
  1FD47BE6 23E19AB5 C34A2A52 17BD46E2 082A728C 536B29CB 0D004964 993A01FB
  8FD05369 242FE615 79746D0B 38B2D276 2F1CD650 C69C1703 FFE26DC8 9FF9F56C
  020EF3C8 7CFB7FBF BCC8962C A95B1494 86756D68 CC696C1A 8EFE5D2D 15715DFB
  B7258632 EC79C5F6 8823C2F8 DD70A41C 0C866E9E F61BE01C 2D2E01F5 30D0755D
  56FC3994 49A7B270 9266C7E2 A66610F2 D532A373 166C030D D2D1CD60 354C9357
  879F7014 211E895F 526E829F 9CB6045B A132D1E2 78A098CA 22AB230C E4601852
  011F7EF7 8C150203 010001A3 53305130 0F060355 1D130101 FF040530 030101FF
  301F0603 551D2304 18301680 144369CE 20019740 53C73C84 87CCD560 8C2C332B
  86301D06 03551D0E 04160414 4369CE20 01974053 C73C8487 CCD5608C 2C332B86
  300D0609 2A864886 F70D0101 05050003 82010100 AFF831DB E552829B CE7123B9
  DB285914 6652B163 83598BF4 B677B227 B429CB14 13C4CF79 E7182813 7943798B
  9E3DF01C 0465D2C4 80C2C34B BA25AF59 DE4E6AB7 4312A53D 06CB13DA ED1256F7
  8AE306D6 339C696C 52019970 1D36A76E 3625A37F A15CC530 EC2E3ECC 65DCF46A
  AF5F8BF1 792DCABB CF6BA504 67642ABA 9E3EEB13 9BE0A0BD 9F33CBAB AC3AFA78
  5E4CBED6 D44AE0B8 8B894FAE 122181C9 B8BC79DA 1E47CBC7 2AFF71EF 2EC3D84B
  F6B2C1F7 9292E239 B3CF9A19 05A57B33 FB0F4727 99BF559E DDAC23FF 3CDEB6FE
  8F3970D9 4BEDA973 1B26D94B D6F3BF0B 81C4FBB5 CF44A2AD EABD89E8 8231C54F
  F1AFA7F0 AB931071 C96561AC 59D0A4E8 ACFD8DF6
        quit
crypto pki certificate chain SLA-TrustPoint
 certificate ca 01
  30820321 30820209 A0030201 02020101 300D0609 2A864886 F70D0101 0B050030
  32310E30 0C060355 040A1305 43697363 6F312030 1E060355 04031317 43697363
  6F204C69 63656E73 696E6720 526F6F74 20434130 1E170D31 33303533 30313934
  3834375A 170D3338 30353330 31393438 34375A30 32310E30 0C060355 040A1305
  43697363 6F312030 1E060355 04031317 43697363 6F204C69 63656E73 696E6720
  526F6F74 20434130 82012230 0D06092A 864886F7 0D010101 05000382 010F0030
  82010A02 82010100 A6BCBD96 131E05F7 145EA72C 2CD686E6 17222EA1 F1EFF64D
  CBB4C798 212AA147 C655D8D7 9471380D 8711441E 1AAF071A 9CAE6388 8A38E520
  1C394D78 462EF239 C659F715 B98C0A59 5BBB5CBD 0CFEBEA3 700A8BF7 D8F256EE
  4AA4E80D DB6FD1C9 60B1FD18 FFC69C96 6FA68957 A2617DE7 104FDC5F EA2956AC
  7390A3EB 2B5436AD C847A2C5 DAB553EB 69A9A535 58E9F3E3 C0BD23CF 58BD7188
  68E69491 20F320E7 948E71D7 AE3BCC84 F10684C7 4BC8E00F 539BA42B 42C68BB7
  C7479096 B4CB2D62 EA2F505D C7B062A4 6811D95B E8250FC4 5D5D5FB8 8F27D191
  C55F0D76 61F9A4CD 3D992327 A8BB03BD 4E6D7069 7CBADF8B DF5F4368 95135E44
  DFC7C6CF 04DD7FD1 02030100 01A34230 40300E06 03551D0F 0101FF04 04030201
  06300F06 03551D13 0101FF04 05300301 01FF301D 0603551D 0E041604 1449DC85
  4B3D31E5 1B3E6A17 606AF333 3D3B4C73 E8300D06 092A8648 86F70D01 010B0500
  03820101 00507F24 D3932A66 86025D9F E838AE5C 6D4DF6B0 49631C78 240DA905
  604EDCDE FF4FED2B 77FC460E CD636FDB DD44681E 3A5673AB 9093D3B1 6C9E3D8B
  D98987BF E40CBD9E 1AECA0C2 2189BB5C 8FA85686 CD98B646 5575B146 8DFC66A8
  467A3DF4 4D565700 6ADF0F0D CF835015 3C04FF7C 21E878AC 11BA9CD2 55A9232C
  7CA7B7E6 C1AF74F6 152E99B7 B1FCF9BB E973DE7F 5BDDEB86 C71E3B49 1765308B
  5FB0DA06 B92AFE7F 494E8A9E 07B85737 F3A58BE1 1A48A229 C37C1E69 39F08678
  80DDCD16 D6BACECA EEBC7CF9 8428787B 35202CDC 60E4616A B623CDBD 230E3AFB
  418616A9 4093E049 4D10AB75 27E86F73 932E35B5 8862FDAE 0275156F 719BB2F0
  D697DF7F 28
        quit
!
!
license udi pid C8200L-1N-4T sn FCZ2818R0MC
memory free low-watermark processor 62972
!
diagnostic bootup level minimal
!
spanning-tree extend system-id
!
enable secret 9 $9$pGjpF3U3LKrdo.$LjjHWyxpWAvzRkUEjf.dYylZSK9qF5Ka0UbsdC54qY2
!
username cisco privilege 15 secret 9 $9$cWOEbiH7rhmumU$aUpDvqXcnc3tYG7KbFHisC5HD.eQz7fHiXy9EZPAJSo
!
redundancy
 mode none
!
!
!
!
!
!
!
!
interface Loopback0
 ip address 209.165.201.1 255.255.255.0
!
interface GigabitEthernet0/0/0
 no ip address
 shutdown
 negotiation auto
!
interface GigabitEthernet0/0/1
 no ip address
 shutdown
 negotiation auto
!
interface GigabitEthernet0/0/1.7
 encapsulation dot1Q 7
 ip address 192.168.20.1 255.255.255.0
!
interface GigabitEthernet0/0/1.8
 encapsulation dot1Q 8
 ip address 192.168.30.1 255.255.255.0
!
interface GigabitEthernet0/0/1.9
 encapsulation dot1Q 9
 ip address 192.168.40.1 255.255.255.0
!
interface GigabitEthernet0/0/2
 no ip address
 shutdown
 negotiation auto
!
interface GigabitEthernet0/0/3
 no ip address
 shutdown
 negotiation auto
!
interface Serial0/1/0
 no ip address
 shutdown
!
interface Serial0/1/1
 no ip address
 shutdown
!
ip http server
ip http authentication local
ip http secure-server
ip forward-protocol nd
!
!
!
!
!
!
control-plane
!
!
line con 0
 password cisco123
 login
 stopbits 1
line aux 0
line vty 0 4
 login local
 transport input ssh
line vty 5 14
 login
 transport input ssh
!
call-home
 ! If contact email address in call-home is configured as sch-smart-licensing@cisco.com
 ! the email address configured in Cisco Smart License Portal will be used as contact email address to send SCH notifications.
 contact-email-addr sch-smart-licensing@cisco.com
 profile "CiscoTAC-1"
  active
  destination transport-method http
!
!
!
!
!
!
end
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r1#
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r1#
r1#
r1#
r1#
r1#
r1#
r1#
r1#
r1#
r1#
r1#
r1#show ip interface brief
Interface              IP-Address      OK? Method Status                Protocol
GigabitEthernet0/0/0   unassigned      YES unset  administratively down down
GigabitEthernet0/0/1   unassigned      YES unset  administratively down down
GigabitEthernet0/0/1.7 192.168.20.1    YES manual administratively down down
GigabitEthernet0/0/1.8 192.168.30.1    YES manual administratively down down
GigabitEthernet0/0/1.9 192.168.40.1    YES manual administratively down down
GigabitEthernet0/0/2   unassigned      YES unset  administratively down down
GigabitEthernet0/0/3   unassigned      YES unset  administratively down down
Serial0/1/0            unassigned      YES unset  administratively down down
Serial0/1/1            unassigned      YES unset  administratively down down
Loopback0              209.165.201.1   YES manual up                    up
r1#
r1#show vlan

VLAN Name                             Status    Ports
---- -------------------------------- --------- -------------------------------
1    default                          active
1002 fddi-default                     act/unsup
1003 token-ring-default               act/unsup
1004 fddinet-default                  act/unsup
1005 trnet-default                    act/unsup

VLAN Type  SAID       MTU   Parent RingNo BridgeNo Stp  BrdgMode Trans1 Trans2
---- ----- ---------- ----- ------ ------ -------- ---- -------- ------ ------
1    enet  100001     1500  -      -      -        -    -        0      0
1002 fddi  101002     1500  -      -      -        -    -        0      0
1003 tr    101003     1500  -      -      -        -    -        0      0
1004 fdnet 101004     1500  -      -      -        ieee -        0      0
1005 trnet 101005     1500  -      -      -        ibm  -        0      0

Primary Secondary Type              Ports
------- --------- ----------------- ------------------------------------------

r1#
r1#
r1#
r1#
r1#

User Access Verification

Password:
Password:
Password:
s1>en
Password:
s1#show run
Building configuration...

Current configuration : 3046 bytes
!
! Last configuration change at 13:24:22 UTC Thu Aug 22 2024
!
version 15.2
no service pad
service timestamps debug datetime msec
service timestamps log datetime msec
no service password-encryption
!
hostname s1
!
boot-start-marker
boot-end-marker
!
enable secret 9 $9$Lqd0MlW1vSiXO3$81/W.IqxYMTLjO5DI3/UEOqLwQU56dNrC4Ualp5sQt6
!
username cisco privilege 15 secret 9 $9$whu3.VziyFOZiL$dS/fcYv23HspjySsOnRSwFSY/J/98AOGhvCOUS8GNTU
no aaa new-model
switch 1 provision c1000-24t-4g-l
system mtu routing 1500
!
!
ip domain-name swre-lab.com
!
!
!
!
!
!
!
!
spanning-tree mode rapid-pvst
spanning-tree extend system-id
!
vlan internal allocation policy ascending
!
!
!
!
!
!
interface Port-channel1
 switchport mode trunk
!
interface GigabitEthernet1/0/1
 switchport mode trunk
 channel-group 1 mode active
!
interface GigabitEthernet1/0/2
 switchport mode trunk
 channel-group 1 mode active
!
interface GigabitEthernet1/0/3
 switchport access vlan 10
 shutdown
!
interface GigabitEthernet1/0/4
 switchport access vlan 10
 shutdown
!
interface GigabitEthernet1/0/5
 switchport access vlan 10
 shutdown
!
interface GigabitEthernet1/0/6
 switchport access vlan 7
 switchport mode access
 switchport port-security
!
interface GigabitEthernet1/0/7
 switchport access vlan 10
 shutdown
!
interface GigabitEthernet1/0/8
 switchport access vlan 10
 shutdown
!
interface GigabitEthernet1/0/9
 switchport access vlan 10
 shutdown
!
interface GigabitEthernet1/0/10
 switchport access vlan 10
 shutdown
!
interface GigabitEthernet1/0/11
 switchport access vlan 10
 shutdown
!
interface GigabitEthernet1/0/12
 switchport access vlan 10
 shutdown
!
interface GigabitEthernet1/0/13
 switchport access vlan 10
 shutdown
!
interface GigabitEthernet1/0/14
 switchport access vlan 10
 shutdown
!
interface GigabitEthernet1/0/15
 switchport access vlan 10
 shutdown
!
interface GigabitEthernet1/0/16
 switchport access vlan 10
 shutdown
!
interface GigabitEthernet1/0/17
 switchport access vlan 10
 shutdown
!
interface GigabitEthernet1/0/18
 switchport access vlan 10
 shutdown
!
interface GigabitEthernet1/0/19
 switchport access vlan 10
 shutdown
!
interface GigabitEthernet1/0/20
 switchport access vlan 10
 shutdown
!
interface GigabitEthernet1/0/21
 switchport access vlan 10
 shutdown
!
interface GigabitEthernet1/0/22
 switchport access vlan 10
 shutdown
!
interface GigabitEthernet1/0/23
 switchport access vlan 10
 shutdown
!
interface GigabitEthernet1/0/24
 switchport access vlan 10
 shutdown
!
interface GigabitEthernet1/0/25
 switchport access vlan 10
 shutdown
!
interface GigabitEthernet1/0/26
 switchport access vlan 10
 shutdown
!
interface GigabitEthernet1/0/27
 switchport access vlan 10
 shutdown
!
interface GigabitEthernet1/0/28
 switchport access vlan 10
 shutdown
!
interface Vlan1
 no ip address
 shutdown
!
interface Vlan9
 ip address 192.168.40.2 255.255.255.0
!
ip http server
ip http secure-server
!
!
!
!
line con 0
 password cisco123
 login
line vty 0 4
 login local
 transport input ssh
line vty 5 15
 login
 transport input none
!
end
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s1#show ip interface brief
Interface              IP-Address      OK? Method Status                Protocol
Vlan1                  unassigned      YES unset  administratively down down
Vlan9                  192.168.40.2    YES manual down                  down
GigabitEthernet1/0/1   unassigned      YES unset  up                    up
GigabitEthernet1/0/2   unassigned      YES unset  up                    up
GigabitEthernet1/0/3   unassigned      YES unset  administratively down down
GigabitEthernet1/0/4   unassigned      YES unset  administratively down down
GigabitEthernet1/0/5   unassigned      YES unset  administratively down down
GigabitEthernet1/0/6   unassigned      YES unset  up                    up
GigabitEthernet1/0/7   unassigned      YES unset  administratively down down
GigabitEthernet1/0/8   unassigned      YES unset  administratively down down
GigabitEthernet1/0/9   unassigned      YES unset  administratively down down
GigabitEthernet1/0/10  unassigned      YES unset  administratively down down
GigabitEthernet1/0/11  unassigned      YES unset  administratively down down
GigabitEthernet1/0/12  unassigned      YES unset  administratively down down
GigabitEthernet1/0/13  unassigned      YES unset  administratively down down
GigabitEthernet1/0/14  unassigned      YES unset  administratively down down
GigabitEthernet1/0/15  unassigned      YES unset  administratively down down
GigabitEthernet1/0/16  unassigned      YES unset  administratively down down
GigabitEthernet1/0/17  unassigned      YES unset  administratively down down
GigabitEthernet1/0/18  unassigned      YES unset  administratively down down
GigabitEthernet1/0/19  unassigned      YES unset  administratively down down
GigabitEthernet1/0/20  unassigned      YES unset  administratively down down
GigabitEthernet1/0/21  unassigned      YES unset  administratively down down
GigabitEthernet1/0/22  unassigned      YES unset  administratively down down
GigabitEthernet1/0/23  unassigned      YES unset  administratively down down
GigabitEthernet1/0/24  unassigned      YES unset  administratively down down
GigabitEthernet1/0/25  unassigned      YES unset  administratively down down
GigabitEthernet1/0/26  unassigned      YES unset  administratively down down
GigabitEthernet1/0/27  unassigned      YES unset  administratively down down
GigabitEthernet1/0/28  unassigned      YES unset  administratively down down
Port-channel1          unassigned      YES unset  up                    up
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s1#show vlan

VLAN Name                             Status    Ports
---- -------------------------------- --------- -------------------------------
1    default                          active
7    vlan 7                           active    Gi1/0/6
8    vlan 8                           active
10   vlan 10                          active    Gi1/0/3, Gi1/0/4, Gi1/0/5
                                                Gi1/0/7, Gi1/0/8, Gi1/0/9
                                                Gi1/0/10, Gi1/0/11, Gi1/0/12
                                                Gi1/0/13, Gi1/0/14, Gi1/0/15
                                                Gi1/0/16, Gi1/0/17, Gi1/0/18
                                                Gi1/0/19, Gi1/0/20, Gi1/0/21
                                                Gi1/0/22, Gi1/0/23, Gi1/0/24
                                                Gi1/0/25, Gi1/0/26, Gi1/0/27
                                                Gi1/0/28
11   vlan 11                          active
1002 fddi-default                     act/unsup
1003 token-ring-default               act/unsup
1004 fddinet-default                  act/unsup
1005 trnet-default                    act/unsup

VLAN Type  SAID       MTU   Parent RingNo BridgeNo Stp  BrdgMode Trans1 Trans2
---- ----- ---------- ----- ------ ------ -------- ---- -------- ------ ------
1    enet  100001     1500  -      -      -        -    -        0      0
7    enet  100007     1500  -      -      -        -    -        0      0
8    enet  100008     1500  -      -      -        -    -        0      0
10   enet  100010     1500  -      -      -        -    -        0      0
11   enet  100011     1500  -      -      -        -    -        0      0
1002 fddi  101002     1500  -      -      -        -    -        0      0
1003 tr    101003     1500  -      -      -        -    -        0      0
1004 fdnet 101004     1500  -      -      -        ieee -        0      0
1005 trnet 101005     1500  -      -      -        ibm  -        0      0

Primary Secondary Type              Ports
------- --------- ----------------- ------------------------------------------
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