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	Device
	Interface
	IP Address 
	Subnet Mask
	Default Gateway
	DNS

	PC-A
	NIC
	192.168.1.1
	255.255.255.0
	192.168.1.0
	192.168.1.100

	PC-B
	NIC
	192.168.1.2
	255.255.255.0
	192.168.1.0
	192.168.1.100

	PC-C
	NIC
	192.168.1.3
	255.255.255.0
	192.168.1.0
	192.168.1.100

	Tablet-1
	Wireless
	192.168.1.5
	255.255.255.0
	192.168.1.0
	192.168.1.100

	WR1
	NIC/Wireless
	192.168.1.4
	255.255.255.0
	192.168.1.0
	192.168.1.100

	L1
	Wireless
	192.168.1.6
	255.255.255.0
	192.168.1.0
	192.168.1.100

	Server-1
	NIC
	192.168.1.100
	255.255.255.0
	192.168.1.0
	192.168.1.100
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In order to verify the network is working correctly and as intended, one of the first steps is too ping devices across the network.
PC-B To PC-A
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PC-C To PC-A
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Tablet-1 To PC-A
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L1 To PC-A
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Programming  Attributes

Packet Tracer BC Command Line 1.0
C:\>ping 152.165.1.1

Pinging 152.168.1.1 with 32 byres of data:

Reply from 152168 “ime=3lms TTL-128
Reply from 152168 “ime=l3ms TTL-128
Reply from 152168 e
Reply from 152168 “ime=llms TTL-128

Ping scavisvics for 152.165.1.1
Packets: Sent = 3, Received = 4, Lost = 0 (0% loss),
Bpproximate round trip vimes in milli-seconds
Minimum = oms, Maximm = 3lms, Average = lsms

e
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0p  Programming  Attributes

fcommana Prompt

Packet Tracer BC Command Line 1.0
e\

C:\>ping 152.165.1.1
Pinging 152.168.1.1 with 32 byres of data:

Reply from 152168 bytes=32 vime=3oms TTL=123
Reply from 152168 bytes=32 cime=l3ms TTL=123
Reply from 152168 bytes=32 cime=loms TTL=125
Reply from 152168 bytes=32 cime=l2ms TTE=125

Ping scavisvics for 152.165.1.1
Packets: Sent = 3, Received = 4, Lost = 0 (0% loss),

Bpproximate round trip times in milli-seconds

Minimm = 10ms, Maximm = 30ms, Average = léms

e
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0p  Programming  Atribute

fcommana Prompt

Packet Tracer BC Command Line 1.0
C:\>ping 152.165.1.1

Pinging 152.168.1.1 with 32 byres of data:

Request cimed out.
Request cimed out.

Reply from 152.1€5.1.1: byces=32 cime<lms TTL=128
Reply from 152.1€8.1.1: byces=32 cime<lms TTL=128

Ping scavisvics for 152.165.1.1
Packets: Sent = 3, Received = 2, Lost = 2 (50% loss),
Bpproximate round trip vimes in milli-seconds

Minimm = 0ms, Maximm = 0ms, Average = Oms

C:\>ping 152.165.1.1

Pinging 152.168.1.1 with 32 byres of data:

Reply from 152168 bytes=32 cime<lms
Reply from 152168 bytes=32 cime<lms
Reply from 152168 bytes=32 cime<lms
Reply from 152168 bytes=32 cime<lms

Ping scavisvics for 152.165.1.1
Packets: Sent = 3, Received = 4, Lost = 0 (0% loss),
Bpprosimate round trip vimes in milli-seconds
Minimm = 0ms, Maximm = 0ms, Average = Oms

e
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fcommana Prompt

Packet Tracer BC Command Line 1.0
C:\>ping 152.165.1.1

Pinging 152.168.1.1 with 32 byres of data:

Reply from 152168 bytes=32 cime<lms
Reply from 152168 bytes=32 cime<lms
Reply from 152168 bytes=32 cime<lms
Reply from 152168 bytes=32 cime<lms

Ping scavisvics for 152.165.1.1
Packets: Sent = 3, Received = 4, Lost = 0 (0% loss),
Bpprosimate round trip vimes in milli-seconds
Minimm = 0ms, Maximm = 0ms, Average = Oms

e





