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HN/BSc (Hons) Computer Networks 
Network Principles (M4X01126)
2014-2015
Lab based Practical Resit Exam 



Student Name	: ______________________
Student ID		: ______________________
Date			: ______________________


This is an individual practical lab-test, held under examination conditions. You will be assigned a Router, a Switch and two PCs; you should configure these devices based on the following specifications. 

This paper is marked out of 100.

You will have 2 hours to complete this task.








TOPOLOGY DIAGRAM
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IP addressing scheme 

	Device
	Interface
	IP Address
	Subnet Mask
	Default Gateway

	R1
	Fa0/0
	192.168.1.1
	255.255.255.0
	N/A

	
	Fa0/1
	192.168.2.1
	255.255.255.0
	N/A

	S1
	VLAN 1
	192.168.1.10
	255.255.255.0
	192.168.1.1

	PC1
	NIC
	192.168.2.254
	255.255.255.0
	192.168.2.1

	PC2
	NIC
	192.168.1.254
	255.255.255.0
	192.168.1.1

	PC3
	NIC
	192.168.1.253
	255.255.255.0
	192.168.1.1



	
	Task 1: Network Connection (15 Marks)
	Physically cable the network as shown in the topology diagram. 

	Task 2: Configure the Router (25 Marks)

Part 1: 
1) Assign a device name R1 to the router.
2) Disable DNS lookup to prevent the router from attempting to translate incorrectly entered commands as though they were host names.
3) Assign class as the privileged EXEC encrypted password.
4) Assign cisco as the console password and enable login.
5) Assign cisco as the VTY password and enable login.
6) Encrypt the clear text passwords.
7) Create a banner that warns anyone accessing the device that unauthorized access is prohibited.
8) Configure and activate both interfaces on the router.
9) Configure an interface description for each interface indicating which device is connected to it.
10) Save the running configuration to the startup configuration file.

Task 3: Configure the Switch (20 Marks)

11) Enter global configuration mode and assign the switch hostname.
12) Assign class as the privileged EXEC encrypted password.
13) Assign cisco as the console password and enable login.
14) Encrypt the clear text passwords.
Prevent unwanted Domain Name System (DNS) lookups.
Configure a login message-of-the-day (MOTD) banner.
Enter global configuration mode to set the SVI (VLAN 1) IP address to allow remote switch management.
Configure IP default gateway. 
Configure the virtual terminal (VTY) line for the switch to allow Telnet access. If you do not configure a VTY password, you will not be able to Telnet to the switch.
Save the running configuration to the startup configuration file.

Task 4: Configure host PCs (30 marks)
After configuring each host computer, record the host network settings with the ipconfig /all command. 

	Host PC1 Network Configuration

	Description
	

	Physical Address
	

	IP Address
	

	Subnet Mask
	

	Default Gateway
	



	Host PC2 Network Configuration

	Description
	

	Physical Address
	

	IP Address
	

	Subnet Mask
	

	Default Gateway
	



	Host PC3 Network Configuration

	Description
	

	Physical Address
	

	IP Address
	

	Subnet Mask
	

	Default Gateway
	





Task 5: Test Connectivity (10 Marks)

	Task
	Result

	PC1 to PC2 and vice versa
	

	PC1 to PC3 and vice versa
	




Submission Requirement 
	All documentation for your solution should be submitted. Your name should be clearly printed on the documents, and signed. 

At the end of the test a flash memory will be given to you, the configuration files for all routers should be copied to the media and handed in to your instructor.  

The file name should be studentname_ID_devicename.txt

Show running-configuration
Show ip interface brief
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