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Using ping command, verify end-to-end connectivity:
1.From PC-1, ping PC-2 – Yes.
[image: A screenshot of a computer

Description automatically generated]
2. From PC-1 to Laptop – No.
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3. From PC-1, default gateway – No.
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4. From PC-2, ping 172.16.0.1. Is it successful - No
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5. From PC-1, ping 172.16.0.254. Is it successful? No
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6. Verify HSRP
[image: A screenshot of a computer

Description automatically generated]
PC-2> ping 172.16.0.1 Ping should not be successful: no
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Description automatically generated]
PC-2> ping default gateway Ping should be successful to 172.16.0.3: no
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From PC-2, ping 209.165.200.225. Is it successful? No
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