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ANSWER ALL QUESTIONS
FROM MOODLE LINK ONLINE EXAM


1. To which address is a limited broadcast sent to ?
A.	255.255.255.255
B.	255.255.0.0
C.	172.16.1.0
D.        0.0.0.0

2. What are disadvantages of deploying a peer-to-peer network model? Choose two.
A.	all the above
B.	lack of high security
C.	lack of central administration
D.	lack of scalability

3. DHCP is a used to automatically assign IP address to hosts. 
A.	False
B.	True



4. The range of wireless technologies most frequently used in home networks are 
A.	unlicensed 902 to 929 Mhz frequency ranges
B.	unlicensed 2.4 GHz and 5 GHz frequency ranges
C.	licensed 902 to 929 Mhz frequency ranges
D.	licensed 2.4 GHz and 5 GHz frequency ranges



5. A consumer places his debit card close to a pay terminal at a shop and the shopping charge is successfully paid. Which type of wireless technology was used?
A.	Bluetooth
B.	4G
C.	Wi-Fi
D.	RFID


 
6. When two computers are directly connected to one another using either wired or wireless media, the resultant network is known as 
A.	Client Server Network
B.	Peer to Peer Network
C.	Interconnected Network
D.	Scalable Network


7. The data which individuals create and explicitly share in platforms like social media profiles is classified as 
A.	Volunteered Data
B.	Observed Data
C.	Inferred Data
D.	Big Data


8. Which type of network cable can be extended for several miles and could be immune for EMI and RFI? 
A.	coaxial cable
B.	twisted-pair cable
C.	Multipair cable
D.       fiber-optic cable


9. Which type of network cable is commonly used to connect office computers to the local network?
A.	twisted-pair cable
B.	coaxial cable
C.	glass fiber-optic cable
D.	plastic fiber-optic cable


10. The layer which describes how a device accesses and sends data over the network media in the TCP/IP model?
A.	application
B.	internet
C.        Network Access
D.	transport



11. What is the maximum size of a valid Ethernet frame?
A.	1522 bytes
B.	1518 bytes
C.	1400 bytes
D.	2048 bytes


12. A network design engineer has been asked to design the IP addressing scheme for a customer network which requires 255 hosts. The network design engineer decides to use IP addresses from the 192.168.20.0/24 network. Will this IP addressing scheme accommodate all the hosts in the customer network?

A. Yes, the network is having the required usable hosts
B. No, the network is not having required usable hosts


13. The network which is using 192.168.11.0/24 network allocates 254 IP addresses for the hosts on the network but excludes 192.168.11.0/24 and 192.168.11.255/24 IP addresses. Why?
A.	These two IP addresses are reserved for email and DNS Servers
B.	These two IP addresses are used for DHCP servers and default gateway
C.	These two IP addresses are reserved to route through the internet. 
D.        These two IP addresses are network IP Address and network broadcast address


14. Routers can eliminate excessive broadcast traffic by subdividing networks into separate broadcast domains. That means,

A.	Routers forward broadcast by default
B.	Routers do not forward broadcast by default


15. Private IP addresses are designed to be exclusively used for external networks and they can be used on the Internet 
A.	True
B.	False


16. The URL identifies the MAC address of the web server 
A.	True
B.	False


17. Hypertext Transfer Protocol is used by web servers to serve up a web page 
A.	True
B.	False


18. In Wireless networks, which wireless security initiative helps to secure sensitive information during data transit?
A.	Authentication
B.	Encryption
C.	IP Address filtering
D.	MAC Address filtering


19. What is the process of placing one message inside another message format called?  
A.	Encapsulation
B.	De-encapsulation
C.	Fragmentation
D.	De-fragmentation


20. Streaming audio and video applications require receipt of all packets regardless of delay. 
A.	True
B.	False

21. Which port can be used for the initial configuration of a Cisco router remotely through a dialup phone line and a modem connected
A.	AUX
B.	console
C.	flash slot
D.	LAN interface
E.	WAN interface


22. To remotely connect a switch or a router securely for management tasks, we shall use
A.	Telnet
B.	SSH
C.	None
D.	Both


23. Which protocol uses plaintext communications for all transmitted data between devices during remote connections?
A.	Telnet
B.	SSH
C.	None
D.	Both



24. While configuring Wireless access points/ wireless routers, which type of device filtering technique is used to enhance the security?
A.	Authentication
B.	Encryption
C.	IP Address
D.	MAC Address



25. Which address is reserved for experimental purposes?
A.	242.1.2.3
B.	239.1.2.3
C.	223.1.2.3
D.	127.1.2.3 


26. You receive an email posing to be a Human Resource Manager of a company and the email states about offering a job for which you have never applied. They have shared a link and ask you to complete a consent form to complete the process of employment. What possible type of attack it could be?
A.	Phishing
B.	Vishing
C.	DDoS
D.	Brute force


27. Which one of the following describes the User Datagram protocol best?
A.	Reliable
B.	Low latency
C.	Maximum bandwidth
D.	All the above


28. A network technician is statically assigning a class B IP address as 172.16.20.10 and Subnet Mask as 255.0.0.0 to a PC. What is wrong in this configuration?
A.	Wrong Subnet Mask. It should be 255.255.0.0 
B.	Wrong Subnet Mask. It should be 255.255.255.255 
C.	Wrong Subnet Mask. It should be 255.255.255.0 
D.	Wrong Subnet Mask. It should be 255.0.0.0


29. After troubleshooting a network problem, what should you do as a network administrator? 
A.	Refer to FAQ.
B.	Escalate the problem.
C.	Update the documentation.
D.	Run remote access software.



30. The Ping command is used to 
A.	test the end-to-end connectivity between hosts
B.	display the network connections 
C.	display the route information from source to destination
D.	none of the above


31. The attacker uses invented scenarios to gain the trust of victim is 
A.	Phishing
B.	Vishing
C.	Pretexting
D.	Tailgating 


32. The architecture that decouples the control and data plane is 
A. Software Defined Networking
B. Legacy Networking 
C. Traditional Networking
D. None of the above


33. One of the below commands communicates with the name server for details about the destination domain is
A.	Ping
B.	Tracert
C.	nslookup
D.	netstat


34. The function that provides secure remote access to servers
A.	DNS
B.	DHCP
C.	SSH
D.	Telnet


35. Why utility lists the protocol in use, the local address and port numbers, the foreign address and port numbers, and the state of the connection?
A.	Ping
B.	Tracert
C.	Ipconfig
D.	netstat



36. One of the main advantages of wireless network technology is
A.	Fairly easy to install
B.	Inexpensive
C.	Easy expansion
D.	All the above

37. All devices that wish to participate in the WLAN need not have the same SSID.
A. True
B. False


38. Applications and services offered for a specific organization or entity such as government institutions, enterprise organizations etc. are categorized under
A.	Private Cloud
B.	Public Cloud
C.	Hybrid Cloud
D.	Community Cloud

39. There are many advantages in virtualization. One major advantage is
A. Slow server provisioning
B. Decreased Server uptime 
C. Increased Server idle time
D. Increased Server uptime

40. The type of hypervisor which is installed directly on the server or networking hardware is 
A. Virtual Box Hypervisor
B. Type 2 Hypervisor
C. Bare Metal Hypervisor
D. Hosted Hypervisor
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