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interface Serial0o/L/o
bandwidch S12

ip address 152.163.35.1 255255255252
ipve address FE80::2 link-local

ipve address 2001:ABCD:EEEF:10

Clock rate €4000

incerface Serialo/l/l
no ip address

Clack rate 2000000
shucdown

incerface Vianl
no ip address
shucdoun

password 7 0822455DUALEDELSIC
logging synchronous

line vey 0 2
password 7 0822455DUALE130308
login local
cranspore inpuc ssh

line vey 3 4
no login

line vey 5 15
no login
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R3ven
Fassvoza:

R3gshow run

Building configuration...

Curzent configuravion : 1315 byves
version 15.4

no service vimestamps log davevime msec
no service vimestamps debug davecime msec

service password-encryprion

hostnsme 23

enable secrec § $13mERrsS.a€PATGBNAMKDLusTEkS/

ip cer
ipve cer
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ipve address FE80::1 link-local
ipve address 2001:CEED:DB3:205::225/64

ss/es

ipve address 2001:CEED:DBS:205:

inverface GigabicEthernesd/o/0
no ip address
duplex auco

speed auto
=hucdoun

inverface GigabicEthernecd/o/1
no ip address
duplex auco

speed auto
=hucdoun

inverface GigabitEthernesd/0/2
no ip address
duplex auco

speed auto
=hucdoun

inverface Serialo/2/o
no ip address

Clack rate 2000000
shucdown

incerface Serialo/2/1
bandwidch S12

ip address 152.163.35.5 255255255252
ipve address FE80::2 link-local

ipve address 2001:ABCD:EE:

ses

interface Visal
no ip address
shucdoun

ip classless

ip flow-expors version 5

cdp run

Te T

annes motd ~C Authorized Ussrs Only ~C
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clock rate 2000000
shucdown

interface Serialo/2/1
bandwidch S12
ip address 152.163.35.5 255255255252

no cdp run

banner metd ~C Authorized Users Only ~C

line con 0
password 7 0822455DUALEDELSIC

logging synchronous

line vey 0 2
password 7 0822455DUALE130308
login local
cranspore inpuc ssh

line vey 3 4
no login

line vey 5 15
no login

Rsz
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You did not complete the activity. Please close this window and try again.
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Rlzen
Passvord:

Rlfshow run

Building configuravion. ..

Current configuravion : 1417 byces
version 15.4

no service timestamps log davevime msec
no service vimestamps debug davevime msec

service password-encryprion

hostname R

enable secret § $13mER3S.acP4JgbNINKOLusTfka/

interface GigabitEctherneto/0/0
ip address 152.168.1.1 255.255.285.0
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interface GigabitEthernet0/0/0
ip address 152.163.1.1 255.255.255.0
aquplex auco
speed auto

interface GigabitZtherneso/o/1
no ip address
duplex auco

speed auto
=hucdoun

interface GigabitZthernetd/0/2
no ip address
duplex auco

speed auto
=hucdoun

interface Serialo/2/o
bandwidch S12

ip address 152.163.55.2 255255255252
ipve address FE80::1 link-local

interface Serialo/2/1

bandwidch S12

ip address 152 16335 ¢ 255255255252
ipve address FE80::1 link-local

ipve address 2001:ABCD:EEEF:20
Clock rate €4000

2/e8

snterface Vlaal
no ip address
shucdoun

ip classless
ip rouce 152.163.59.0 255.255.255 252 Serialo/2/o

ip route 172.16.1.0 255.255.255.0 Serials/2/o

ip flow-expors version 5

cdp run

cgTT

banner motd ~C Authorized Users Only ~C
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banner motd °C Authorized Users Only °C

line con 0
password 7 0822455DUALEDELSIC

logging synchronous

line vey 0 2
password 7 0822455DUALE130308
login local
cranspore inpuc ssh

line vey 3 4
no login

line vey 5 15
no login

21
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R2>en
Passvord

R2ssnow run

Building configuration...

Current configuration : 1581 byses
version 15.4

no service timestamps log datetime msec
no service timestamps debug datetime msec

service password-encryption

nostnsme 22

enable secret § §15mERESS.a€PATGENAMKDLusT SRS/

ip cer
ipve cer

ip domain-lookup

A A

spanning-tree mode pvst

snterface Loopbackl
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1p address 172.26.1.1 £95.255.255.0

interface Loopbacks
ip address 172.16.2.1 255.255.255.0

interface GigabitZtherneso/0/0
ip address 152 163.25 €5 255.255.255.224
aquplex auco

speed auto

ipve address FESD::1 link-local

ipve address 2001:1111:8De3:e4

interface GigabitZtherneso/o/1
no ip address
duplex auco

speed auto
=hucdoun

interface GigabitZthernetd/0/2
no ip address

duplex auco

speed auto

=hucdoun

interface Serialo/1/o
bandwidch S12

ip address 152.163.35.1 255255255252
ipve address FE80::2 link-local

ipve address 2001:ABCD:EEEF:10

Clock rate €4000

1768

interface Serialo/1/1
no ip address

Clack rate 2000000
shucdown

snterface Vlaal
no ip address





