Router:

Show Run:
Building configuration...


Current configuration : 3612 bytes
!
! Last configuration change at 12:11:35 UTC Mon Aug 19 2019
!
version 16.9
service timestamps debug datetime msec
service timestamps log datetime msec
service password-encryption
platform qfp utilization monitor load 80
no platform punt-keepalive disable-kernel-core
!
hostname R1
!
boot-start-marker
boot-end-marker
!
!
enable secret 5 $1$iVfW$aLEg3Kn3aBx3/x.pj/wRT0
!
no aaa new-model
!
no ip domain lookup
ip admission watch-list expiry-time 0
!
!
!
!
!
!
!
!
!
!
subscriber templating
multilink bundle-name authenticated
!
!
!
crypto pki trustpoint TP-self-signed-1562137005
 enrollment selfsigned
 subject-name cn=IOS-Self-Signed-Certificate-1562137005
 revocation-check none
 rsakeypair TP-self-signed-1562137005
!
!
crypto pki certificate chain TP-self-signed-1562137005
 certificate self-signed 01
  30820330 30820218 A0030201 02020101 300D0609 2A864886 F70D0101 05050030
  31312F30 2D060355 04031326 494F532D 53656C66 2D536967 6E65642D 43657274
  69666963 6174652D 31353632 31333730 3035301E 170D3139 30383139 31323034
  33385A17 0D333030 31303130 30303030 305A3031 312F302D 06035504 03132649
  4F532D53 656C662D 5369676E 65642D43 65727469 66696361 74652D31 35363231
  33373030 35308201 22300D06 092A8648 86F70D01 01010500 0382010F 00308201
  0A028201 0100CFB9 A6169538 2D465AB0 B26CBEF0 DE3976D6 A02F15AB 57056215
  A053F598 30609AD0 8A51C6DC CF7E0103 A94B3A24 F210E3E9 CD473F6B 9A983074
  41537E6A 0F3FC8F2 591D8B80 1D3DBCC8 5D425134 C16686AE 48AD9E60 28BAD331
  923673F9 BBC489AC 2C790E4D 608725FD 98C44528 56E83B8C E6CEC968 A1E816DA
  98259B4E 20546478 685000E6 BD96B432 5F923160 DF541518 82309B84 59F48519
  D7C97455 F0904FD8 3F704528 F210036B B76E4280 ABF5CA45 8D25340A F3A1A32B
  34FC1E16 FEE91EAA 40C0A241 BF482C85 B4F3B402 F1F0F465 ACC8976B 1E0F4E7E
  EBF04E48 F407E9F3 AA36AD28 DABC6499 44C443B4 B4DC8D23 D96FA1B5 93EB85EB
  75CC317E 32A10203 010001A3 53305130 0F060355 1D130101 FF040530 030101FF
  301F0603 551D2304 18301680 14573DA9 7D7BAB22 44700A3B 08419603 69EF5504
  B8301D06 03551D0E 04160414 573DA97D 7BAB2244 700A3B08 41960369 EF5504B8
  300D0609 2A864886 F70D0101 05050003 82010100 1A60839A C2663FDB 741B07AE
  338DD1F8 8A0D5B43 69A43DC4 CDEE516E 3058F603 AA6498EE 964C0499 D10A0375
  EA4FF59C 9B6D61D7 686EF9B0 5FE3FABF 4B8BA217 5AA6D678 0A62E53E 0BD5C983
  527A27CD 22B8D0E6 9F998514 0F374C88 9D5EC4E3 7E9AF923 60CDE659 E546A584
  21805555 4B8058FF 3064C22E D180C8CE 3210F904 04F09E35 349E655A D3C29DD6
  B2D6E32A D81792FD 51F25615 42AF4327 4E1F7C9C 32A7E0E5 CF19CB76 92B43F35
  9AA5EE35 986FD48A A0A2C1B4 E2E31615 CDA53E2D 09E4ED6B 25AA0189 57FEE470
  3B7A0E44 FBB9EE17 B08C87D8 0A0EF4DA 3F130227 32B461DC 4A3AB10F 98A0DDF7
  5311BFE0 16FC8489 2B99A5E8 C46B4B12 07D9091C
        quit
!
license udi pid ISR4221/K9 sn FGL224190DN
no license smart enable
diagnostic bootup level minimal
!
spanning-tree extend system-id
!
!
!
!
redundancy
 mode none
!
!
!
!
!
!
!
!
interface GigabitEthernet0/0/0
 description connection to PCB(13)
 ip address 172.16.10.1 255.255.255.0
 negotiation auto
!
interface GigabitEthernet0/0/1
 description connection to SW(13)
 ip address 172.16.11.1 255.255.255.0
 negotiation auto
!
interface Serial0/1/0
 no ip address
 shutdown
!
interface Serial0/1/1
 no ip address
 shutdown
!
ip forward-protocol nd
ip http server
ip http authentication local
ip http secure-server
!
!
!
!
!
!
control-plane
!
banner motd ^Cotd# Unauthorized access prohibited!!#


Unauthorized access prohibited#


^C
!
line con 0
 password 7 1511021F0725
 login
 transport input none
 stopbits 1
line vty 0 4
 password 7 060506324F41
 login
!
!
!
!
!
!
End



R1#show ip int brief
Interface              IP-Address      OK? Method Status                Protocol
GigabitEthernet0/0/0   172.16.10.1     YES manual up                    up
GigabitEthernet0/0/1   172.16.11.1     YES manual up                    up
Serial0/1/0            unassigned      YES unset  administratively down down
Serial0/1/1            unassigned      YES unset  administratively down down





Switch:
SW13#show run
Building configuration...

Current configuration : 2993 bytes
!
! Last configuration change at 00:08:22 UTC Mon Mar 1 1993
!
version 15.2
no service pad
service timestamps debug datetime msec
service timestamps log datetime msec
no service password-encryption
!
hostname SW13
!
boot-start-marker
boot-end-marker
!
!
no aaa new-model
system mtu routing 1500
!
!
!
!
!
!
!
no ip domain-lookup
!
!
crypto pki trustpoint TP-self-signed-425053184
 enrollment selfsigned
 subject-name cn=IOS-Self-Signed-Certificate-425053184
 revocation-check none
 rsakeypair TP-self-signed-425053184
!
!
crypto pki certificate chain TP-self-signed-425053184
 certificate self-signed 01
  30820229 30820192 A0030201 02020101 300D0609 2A864886 F70D0101 05050030
  30312E30 2C060355 04031325 494F532D 53656C66 2D536967 6E65642D 43657274
  69666963 6174652D 34323530 35333138 34301E17 0D393330 33303130 30303035
  385A170D 32303031 30313030 30303030 5A303031 2E302C06 03550403 1325494F
  532D5365 6C662D53 69676E65 642D4365 72746966 69636174 652D3432 35303533
  31383430 819F300D 06092A86 4886F70D 01010105 0003818D 00308189 02818100
  E445ED4E EF36A041 F4BCB3A8 6945D722 D77246DA AB650DED 3B013401 67008CB1
  7021A18D 0F645D2A 6523CF43 D2616FEA A8A19821 2C8A94C1 6E5A2EF8 FF67597F
  1E6C7F47 52BCE746 30E2BEB2 FD985A73 AFB26515 F701598D BD6F37D4 AB07297E
  AA02EAF7 3D4E0527 8290853A B4778EEA 238D4C58 F94ECEFD BF91C8BF 64F0A93D
  02030100 01A35330 51300F06 03551D13 0101FF04 05300301 01FF301F 0603551D
  23041830 16801431 8DBA0C60 DD4C558C A8C5229A 7DCF09C1 CE481C30 1D060355
  1D0E0416 0414318D BA0C60DD 4C558CA8 C5229A7D CF09C1CE 481C300D 06092A86
  4886F70D 01010505 00038181 00110116 2B46FDE3 3E927100 7513BC97 4DED2A99
  929ADDB6 FD66BC89 B748B767 9564ED71 CA5D00CC 7343701E 9D98DC9E 11F32575
  29B9F911 40FA0DC7 8A6A4450 0AA8F5FE 015BA2D5 FC15CD49 E49F8439 A9D19487
  39F54112 AB8B998B 0D06030E A033B78A A42B25EE 63E2F68B C787D0EE AB709A3E
  44AB342C BB1CEDCA 528CA0E6 C1
        quit
spanning-tree mode pvst
spanning-tree extend system-id
!
vlan internal allocation policy ascending
!
!
!
!
!
!
interface FastEthernet0/1
!
interface FastEthernet0/2
!
interface FastEthernet0/3
!
interface FastEthernet0/4
!
interface FastEthernet0/5
!
interface FastEthernet0/6
!
interface FastEthernet0/7
!
interface FastEthernet0/8
!
interface FastEthernet0/9
!
interface FastEthernet0/10
!
interface FastEthernet0/11
!
interface FastEthernet0/12
!
interface FastEthernet0/13
!
interface FastEthernet0/14
!
interface FastEthernet0/15
!
interface FastEthernet0/16
!
interface FastEthernet0/17
!
interface FastEthernet0/18
!
interface FastEthernet0/19
!
interface FastEthernet0/20
!
interface FastEthernet0/21
!
interface FastEthernet0/22
!
interface FastEthernet0/23
!
interface FastEthernet0/24
!
interface GigabitEthernet0/1
!
interface GigabitEthernet0/2
!
interface Vlan1
 ip address 172.16.11.10 255.255.255.0
!
ip default-gateway 172.16.11.1
ip http server
ip http secure-server
!
no vstack
!
line con 0
line vty 0 4
 password cisco
 login
line vty 5 15
 login
!
End




SW13#show ip int brief
Interface              IP-Address      OK? Method Status                Protocol
Vlan1                  172.16.11.10    YES NVRAM  up                    up
FastEthernet0/1        unassigned      YES unset  down                  down
FastEthernet0/2        unassigned      YES unset  down                  down
FastEthernet0/3        unassigned      YES unset  down                  down
FastEthernet0/4        unassigned      YES unset  down                  down
FastEthernet0/5        unassigned      YES unset  up                    up
FastEthernet0/6        unassigned      YES unset  up                    up
FastEthernet0/7        unassigned      YES unset  down                  down
FastEthernet0/8        unassigned      YES unset  down                  down
FastEthernet0/9        unassigned      YES unset  down                  down
FastEthernet0/10       unassigned      YES unset  down                  down
FastEthernet0/11       unassigned      YES unset  down                  down
FastEthernet0/12       unassigned      YES unset  down                  down
FastEthernet0/13       unassigned      YES unset  down                  down
FastEthernet0/14       unassigned      YES unset  down                  down
FastEthernet0/15       unassigned      YES unset  down                  down
FastEthernet0/16       unassigned      YES unset  down                  down
FastEthernet0/17       unassigned      YES unset  down                  down
FastEthernet0/18       unassigned      YES unset  down                  down
FastEthernet0/19       unassigned      YES unset  down                  down
FastEthernet0/20       unassigned      YES unset  down                  down
FastEthernet0/21       unassigned      YES unset  down                  down
FastEthernet0/22       unassigned      YES unset  down                  down
FastEthernet0/23       unassigned      YES unset  down                  down
FastEthernet0/24       unassigned      YES unset  down                  down
GigabitEthernet0/1     unassigned      YES unset  down                  down
GigabitEthernet0/2     unassigned      YES unset  down                  down
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Command Prompt

C:\Users\Admin>ipconfig /allll

Windows TP Configuration

Host Name . : LN271-NETLAB
Primary Dns Suffix’ R

Node Type . . . C ... .. Hybrid

Ip Routing Enabled. . . . . . . . : Mo

WINS Proxy Enabled. . . . . . . . : No

Ethernet adapter Ethernet:

Connection-specific DNS Suffix

Description . Intel(R) Ethernet Connection (2) I219-M
Physical Address. .~ .. ... :8C-9D-92-BF-BB-78
DHCP Enabled. . . . S ...l
Autoconfiguration Enabled . Yes
Link-local IPv6 Address . . . : fe80::41e5:356b: celc:9cod¥12(Preferred)
IPv4 Address. . . . . . . ... .: 172.16.16.254(Preferred)
Subnet Mask . 255.255.255.6
Default Gateway . . . . . . . . . : 172.16.16.1
DHCPV6 TAID . . . . . . . .. ..: 118267282
DHCPV6 Client DUID. . . . . . . . : @0-81-80-61-23-4F-C2-SE-0C-9D-92-BF-BB-78
DNS Servers . . . . . . . ... .: feco:8:0:FFFf::1%1
Fec0:0:0: FFFF::2%1
feco
NetBIOS over Tcpip. . . . . . . . : Enabled

C:\Users\Admin>
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Command Prompt

Fec0:0:0: FFFf::3%1
NetBIOS over Tcpip. . . . . . . . : Enabled

C:\Users\Admin>ping 172.16.16.254

Pinging 172.16.10.254 with 32 bytes of data:
Reply from 172.16.10.254: bytes=32 time<ims
Reply from 172.16.10.254: bytes=32 time<ims
Reply from 172.16.16.254 2 time<ins
Reply from 172.16.16.254:

Ping statistics for 172.16.16.254:
Packets: Sent = 4, Received = 4, Lost = © (8% loss),
Approximate round trip times in milli-seconds:
Minimum = @ms, Maximum - ems, Average = 6ms

C:\Users\Admin>ping 172.16.16.254

Pinging 172.16.16.254 with 32 bytes of data: 1
Reply from 172.16.10.254: bytes=32 timecims TTL-127

Reply from 172.16.10.254 2 timecins
Reply from 172.16.10.254 2 timecins
Reply from 172.16.10.254: bytes=32 time<ims TTL-127

Ping statistics for 172.16.16.254:
Packets: Sent = 4, Received = 4, Lost = © (8% loss),
Approximate round trip times in milli-seconds:
Minimum = @ms, Maximum - ems, Average = 6ms

C:\Users\Admin>




