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Lab – Understanding Ethernet Cable Standards 
Topology
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Addressing Table
	Device
	Interface
	IP Address
	Subnet Mask
	Default Gateway

	PC-A
	NIC
	192.168.10.1
	255.255.255.0
	N/A

	PC-B
	NIC
	192.168.10.2
	255.255.255.0
	N/A


Objectives
Part 1: Analyze Ethernet Cabling Standards and Pinouts
Part 2: Build an Ethernet Crossover Cable
Part 3: Test an Ethernet Crossover Cable
Background / Scenario
In this lab, you will build and terminate an Ethernet crossover cable and test it by connecting two PCs together and pinging between them. You will first analyze the Telecommunications Industry Association/Electronic Industries Association (TIA/EIA) 568-A and 568-B standards and how they apply to Ethernet cables. You will then construct an Ethernet crossover cable and test it. Finally, you will use the cable you just constructed to connect two PCs together and test it by pinging between them.
Note: With autosensing capabilities available on many devices, such as the Cisco 1941 Integrated Services Router (ISR) switch, you may see straight-through cables connecting like devices.
Required Resources
One length of cable, either Category 5 or 5e. Cable length should be 0.6 to 0.9m (2 to 3 ft.)
2 RJ-45 connectors
RJ-45 crimping tool
Wire cutter
Wire stripper
Ethernet cable tester (optional)
2 PCs (Windows 7 or 8)
Analyze Ethernet Cabling Standards and Pinouts
The TIA/EIA has specified unshielded twisted pair (UTP) cabling standards for use in LAN cabling environments. TIA/EIA 568-A and 568-B stipulates the commercial cabling standards for LAN installations; these are the standards most commonly used in LAN cabling for organizations and they determine which color wire is used on each pin.
With a crossover cable, the second and third pairs on the RJ-45 connector at one end of the cable are reversed at the other end, which reverses the send and receive pairs. The cable pinouts are the 568-A standard on one end and the 568-B standard on the other end. Crossover cables are normally used to connect hubs to hubs or switches to switches, but they can also be used to directly connect two hosts to create a simple network.
Reflection:  
Write a research report (Max word count 600) on Cat 5e and 6 Ethernet cable standards.  
Cat 5e and 6 Ethernet cable standards

Ethernet cables are grouped into sequentially numbered of categories ("CAT") based on various specifications. Often a category is updated with further clarifications or testing standards (e.g. 5e, 6a). These categories show how to find out what type of cable is needed for a particular device. As the number of categories increases, the wire speed and “Mhz” increases, each category introduces more stringent crosstalk elimination (XT), tests and added insulation between wires. [1] [2]

The category 5 cable was changed and replaced mainly by the category 5 extended cable (CAT-5e), which did not change anything physically in the cable, but instead used more stringent crosstalk testing standards. Category 6 was changed using the extended category 6 (CAT-6a), which provided testing of 500 MHz communication (compared to 250 MHz Cat-6). Higher communication frequency has eliminated foreign crosstalk (AXT), which allows for greater range at 10 Gb/s. [3] [4] [5]

Number of twists per cm in the wire, and sheath thickness are the two main physical differences between CAT-5 and CAT-6 cables. Cable twisting length is not standardized, but typically there are 1.5-2 turns per cm on CAT-5 (e) and 2+ turns per cm on CAT-6. For a single cable, each colored pair will have different twist lengths based on prime numbers, it means that they will never match. The number of twists per pair is usually unique for each cable manufacturer. [1] [2]

Many CAT-6 cables also include a nylon tongue that helps eliminate crosstalk. Although a spline is not required for a CAT-5 cable, some manufacturers include it anyway. For a CAT-6 cable, the spline is not required as long as the cable comply with the standards.
While the nylon spline helps reduce wire crosstalk, the thicker shield protects against near-end crosstalk (NEXT) and foreign crosstalk (AXT), which are more common as the frequency increases (Mhz). [6] [3]

Because all Ethernet cables are twisted, it produces shielding to further protection from interference. Unshielded twisted pair can be successfully used for cables between the computer and the wall, but in areas with high interference and cable routing outside or inside the walls, it is recommended to use shielded cable. There are different ways to protect an Ethernet cable, but this usually involves placing a shield around each pair of wires in the cable. This protects the vapor from crosstalk internally. [7] [8]

Solid and twisted Ethernet cables refer to a real copper conductor in pairs. A solid cable uses a single piece of copper for an electrical conductor, while the twisted cable uses a series of copper cables twisted together. The solid cable is not as flexible, but it is also more durable, which makes it ideal for fixed installations as well as outside and on the walls. Cable with ropes is more flexible and should be used at the desk or wherever the cable is often moved. [9] [2]

It is important to choose the right cable as there any many differences between CAT-5e and CAT-6, as stated above. The most important is the network speed and frequency of the cable required. If the wrong cable is used for a network with a large number of users, speed and data loss may occur. Copper quality should be also considered as low-quality copper used in cables can cause up to 70% of network downtime. [6] [10]
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Analyze diagrams and tables for the TIA/EIA 568-A standard Ethernet cable.
The following table and diagrams display the color scheme and pinouts, as well as the function of the four pairs of wires used for the 568-A standard. 
Note: In LAN installations using 100Base-T (100 Mb/s), only two pairs out of the four are used.
568-A 10/100/1000Base-TX Ethernet
	Pin Number
	Pair Number
	Wire Color
	10Base-T Signal
100Base-TX Signal
	1000Base-T Signal

	1
	2
	White/Green
	Transmit
	BI_DA+

	2
	2
	Green
	Transmit
	BI_DA-

	3
	3
	White/Orange
	Receive
	BI_DB+

	4
	1
	Blue
	Not Used
	BI_DC+

	5
	1
	White/Blue
	Not Used
	BI_DC-

	6
	3
	Orange
	Receive
	BI_DB-

	7
	4
	White/Brown
	Not Used
	BI_DD+

	8
	4
	Brown
	Not Used
	BI_DD-




The following diagrams display how the wire color and pinouts align with an RJ-45 jack for the 568-A standard.
[image: T-568A]
[image: RJ-45 Jack]
Analyze diagrams and tables for the TIA/EIA 568-B standard Ethernet cable.
The following table and diagram display the color scheme and pinouts for the 568-B standard.
568-B 10/100/1000-BaseTX Ethernet
	Pin Number
	Pair Number
	Wire Color
	10Base-T Signal
100Base-TX Signal
	1000Base-T Signal

	1
	2
	White/Orange
	Transmit
	BI_DA+

	2
	2
	Orange
	Transmit
	BI_DA-

	3
	3
	White/Green
	Receive
	BI_DB+

	4
	1
	Blue
	Not Used
	BI_DC+

	5
	1
	White/Blue
	Not Used
	BI_DC-

	6
	3
	Green
	Receive
	BI_DB-

	7
	4
	White/Brown
	Not Used
	BI_DD+

	8
	4
	Brown
	Not Used
	BI_DD-


[image: T568B_ColorPinout_AndRJ45Jack]


Build an Ethernet Crossover Cable
A crossover cable has the second and third pairs on the RJ-45 connector at one end, reversed at the other end (refer to the table in Part 1, Step 2). The cable pinouts are the 568-A standard on one end and the 568-B standard on the other end. The two following diagrams illustrate this concept.
[image: Cross_over_CableRJ45Connectors_1]
Build and terminate a TIA/EIA 568-A cable end.
Determine the cable length required. (Your instructor will let you know the cable length you should make.)
Note: If you were making a cable in a production environment, the general guideline is to add another 12 in. (30.48 cm) to the length.
Cut off a piece of cable to the desired length and using your wire stripper, remove 5.08 cm (2 in.) of the cable jacket from both ends.
Hold the four pairs of twisted cables tightly where the jacket was cut away. Reorganize the cable pairs into the order of the 568-A wiring standard. Refer to the diagrams, if necessary. Take as much care as possible to maintain the twists in the cable; this provides noise cancellation.
Flatten, straighten, and line up the wires using your thumb and forefinger.
Ensure that the cable wires are still in the correct order for the 568-A standard. Using your wire cutters, trim the four pairs in a straight line to within 1.25 to 1.9 cm (1/2 to 3/4 in.).
Place an RJ-45 connector on the end of your cable, with the prong on the underside pointing downward. Firmly insert the wires into the RJ-45 connector. All wires should be seen at the end of the connector in their proper positions. If the wires are not extending to the end of the connector, take the cable out, rearrange the wires as necessary, and reinsert the wires back into the RJ-45 connector.
If everything is correct, insert the RJ-45 connector with cable into the crimper. Crimp down hard enough to force the contacts on the RJ-45 connector through the insulation on the wires, thus completing the conducting path. See the following diagram for an example.
[image: crimp_Pic]
Build and terminate a TIA/EIA 568-B cable end.
Repeat steps 1a to 1g using the 568-B color wiring scheme for the other end.
Test an Ethernet Crossover Cable
Test the cable.
Many cable testers will test for length and mapping of wires. If the cable tester has a wire map feature, it verifies which pins on one end of the cable are connected to which pins on the other end.
If your instructor has a cable tester, test the crossover cable for functionality. If it fails, check with your instructor first as to whether you should re-cable the ends and re-test.
Connect two PCs together via NICs using your Ethernet crossover cable.
Working with a lab partner, set your PC to one of the IP addresses shown in the Addressing Table (see page 1). For example, if your PC is PC-A, your IP address should be set to 192.168.10.1 with a 24-bit subnet mask. You partner’s IP address should be 192.168.10.2. The default gateway address can be left empty.
Using the crossover cable you made, connect the two PCs together via their NICs.
On the PC-A command prompt, ping the PC-B IP address.
Note: The Windows firewall may have to be temporarily disabled for pings to be successful. If the firewall is disabled, make sure you re-enable it at the conclusion of this lab.
Repeat the process and ping from PC-B to PC-A.
Assuming IP addressing and firewall are not issues, your pings should be successful if the cables were properly made.
Reflection
Which part of making cables did you find the most difficult?
Most difficult part was to hold cables in the correct order while trying to push them in.
Why do you have to learn how to make a cable if you can easily buy pre-made cables?
To understand how ethernet cable works and what are the different standards.
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