
Packet Tracer PC Command Line 1.0
C:\>ping 185.95.2.3

Pinging 185.95.2.3 with 32 bytes of data:

Reply from 185.95.1.1: Destination host unreachable.
Reply from 185.95.1.1: Destination host unreachable.
Reply from 185.95.1.1: Destination host unreachable.
Reply from 185.95.1.1: Destination host unreachable.

Ping statistics for 185.95.2.3:
Packets: Sent = 4, Received = 0, Lost = 4 (100% loss),

C:\>

[image: ]

R1
Show run
R1#show run
Building configuration...

Current configuration : 975 bytes
!
version 15.1
no service timestamps log datetime msec
no service timestamps debug datetime msec
no service password-encryption
!
hostname R1
!
!
!
!
!
!
!
!
no ip cef
no ipv6 cef
!
!
!
!
license udi pid CISCO1941/K9 sn FTX15244QM7-
!
!
!
!
!
!
!
!
!
!
!
spanning-tree mode pvst
!
!
!
!
!
!
interface GigabitEthernet0/0
ip address 185.95.1.1 255.255.255.0
duplex auto
speed auto
!
interface GigabitEthernet0/1
no ip address
duplex auto
speed auto
shutdown
!
interface Serial0/0/0
ip address 185.95.12.1 255.255.255.252
!
interface Serial0/0/1
ip address 185.95.13.1 255.255.255.252
clock rate 2000000
!
interface Vlan1
no ip address
shutdown
!
router ospf 1
router-id 1.1.1.1
log-adjacency-changes
passive-interface GigabitEthernet0/0
auto-cost reference-bandwidth 1000
network 185.95.1.0 0.0.0.255 area 0
!
ip classless
!
ip flow-export version 9
!
!
!
banner motd ^CAuthorized Access only^C
!
!
!
!
!
line con 0
!
line aux 0
!
line vty 0 4
login
!
!
!
end
 show ip int brief
R1#show ip int brief
Interface IP-Address OK? Method Status Protocol 
GigabitEthernet0/0 185.95.1.1 YES manual up up 
GigabitEthernet0/1 unassigned YES unset administratively down down 
Serial0/0/0 185.95.12.1 YES manual up up 
Serial0/0/1 185.95.13.1 YES manual up up 
Vlan1 unassigned YES unset administratively down down
R1#
R1#
R1#
R1#show ip route
Codes: L - local, C - connected, S - static, R - RIP, M - mobile, B - BGP
D - EIGRP, EX - EIGRP external, O - OSPF, IA - OSPF inter area
N1 - OSPF NSSA external type 1, N2 - OSPF NSSA external type 2
E1 - OSPF external type 1, E2 - OSPF external type 2, E - EGP
i - IS-IS, L1 - IS-IS level-1, L2 - IS-IS level-2, ia - IS-IS inter area
* - candidate default, U - per-user static route, o - ODR
P - periodic downloaded static route

Gateway of last resort is not set

185.95.0.0/16 is variably subnetted, 6 subnets, 3 masks
C 185.95.1.0/24 is directly connected, GigabitEthernet0/0
L 185.95.1.1/32 is directly connected, GigabitEthernet0/0
C 185.95.12.0/30 is directly connected, Serial0/0/0
L 185.95.12.1/32 is directly connected, Serial0/0/0
C 185.95.13.0/30 is directly connected, Serial0/0/1
L 185.95.13.1/32 is directly connected, Serial0/0/1

R1#

R1#show ip ospf neighbor

R1#
R1#show ip ospf neighbor

R1#
R1#
R1#show ip ospf database
OSPF Router with ID (1.1.1.1) (Process ID 1)

Router Link States (Area 0)

Link ID ADV Router Age Seq# Checksum Link count
1.1.1.1 1.1.1.1 917 0x80000003 0x0065c1 1
R1#


R2>enable
R2#show run
Building configuration...

Current configuration : 933 bytes
!
version 15.1
no service timestamps log datetime msec
no service timestamps debug datetime msec
no service password-encryption
!
hostname R2
!
!
!
!
!
!
!
!
no ip cef
no ipv6 cef
!
!
!
!
license udi pid CISCO1941/K9 sn FTX1524L1K3-
!
!
!
!
!
!
!
!
!
!
!
spanning-tree mode pvst
!
!
!
!
!
!
interface GigabitEthernet0/0
ip address 185.95.2.1 255.255.255.0
duplex auto
speed auto
!
interface GigabitEthernet0/1
no ip address
duplex auto
speed auto
shutdown
!
interface Serial0/0/0
ip address 185.95.12.2 255.255.255.252
!
interface Serial0/0/1
ip address 185.95.23.1 255.255.255.252
clock rate 128000
!
interface Vlan1
no ip address
shutdown
!
router ospf 1
router-id 2.2.2.2
log-adjacency-changes
passive-interface GigabitEthernet0/0
auto-cost reference-bandwidth 1000
!
ip classless
!
ip flow-export version 9
!
!
!
banner motd ^C Authorized assess^C
!
!
!
!
!
line con 0
!
line aux 0
!
line vty 0 4
login
!
!
!
end


R2#
R2#
R2#
R2#
R2#
R2#show ip int brief
Interface IP-Address OK? Method Status Protocol 
GigabitEthernet0/0 185.95.2.1 YES manual up up 
GigabitEthernet0/1 unassigned YES unset administratively down down 
Serial0/0/0 185.95.12.2 YES manual up up 
Serial0/0/1 185.95.23.1 YES manual up up 
Vlan1 unassigned YES unset administratively down down
R2#
R2#
R2#show ip ospf neighbor

R2#
R2#
R2#show ip ospf database
R2#
R2#show ip route
Codes: L - local, C - connected, S - static, R - RIP, M - mobile, B - BGP
D - EIGRP, EX - EIGRP external, O - OSPF, IA - OSPF inter area
N1 - OSPF NSSA external type 1, N2 - OSPF NSSA external type 2
E1 - OSPF external type 1, E2 - OSPF external type 2, E - EGP
i - IS-IS, L1 - IS-IS level-1, L2 - IS-IS level-2, ia - IS-IS inter area
* - candidate default, U - per-user static route, o - ODR
P - periodic downloaded static route

Gateway of last resort is not set

185.95.0.0/16 is variably subnetted, 6 subnets, 3 masks
C 185.95.2.0/24 is directly connected, GigabitEthernet0/0
L 185.95.2.1/32 is directly connected, GigabitEthernet0/0
C 185.95.12.0/30 is directly connected, Serial0/0/0
L 185.95.12.2/32 is directly connected, Serial0/0/0
C 185.95.23.0/30 is directly connected, Serial0/0/1
L 185.95.23.1/32 is directly connected, Serial0/0/1

R2#

Authorized assess

R3>enable
R3#enable
R3#show run
Building configuration...

Current configuration : 932 bytes
!
version 15.1
no service timestamps log datetime msec
no service timestamps debug datetime msec
no service password-encryption
!
hostname R3
!
!
!
!
!
!
!
!
no ip cef
no ipv6 cef
!
!
!
!
license udi pid CISCO1941/K9 sn FTX1524F394-
!
!
!
!
!
!
!
!
!
!
!
spanning-tree mode pvst
!
!
!
!
!
!
interface GigabitEthernet0/0
ip address 185.95.3.1 255.255.255.0
duplex auto
speed auto
!
interface GigabitEthernet0/1
no ip address
duplex auto
speed auto
shutdown
!
interface Serial0/0/0
ip address 185.95.13.2 255.255.255.252
clock rate 128000
!
interface Serial0/0/1
ip address 185.95.23.2 255.255.255.252
!
interface Vlan1
no ip address
shutdown
!
router ospf 1
router-id 3.3.3.3
log-adjacency-changes
passive-interface GigabitEthernet0/0
auto-cost reference-bandwidth 1000
!
ip classless
!
ip flow-export version 9
!
!
!
banner motd ^CAuthorized assess^C
!
!
!
!
!
line con 0
!
line aux 0
!
line vty 0 4
login
!
!
!
end


R3#

R3#
R3#
R3#show ip int brief
Interface IP-Address OK? Method Status Protocol 
GigabitEthernet0/0 185.95.3.1 YES manual up up 
GigabitEthernet0/1 unassigned YES unset administratively down down 
Serial0/0/0 185.95.13.2 YES manual up up 
Serial0/0/1 185.95.23.2 YES manual up up 
Vlan1 unassigned YES unset administratively down down
R3#
R3#show ip route
Codes: L - local, C - connected, S - static, R - RIP, M - mobile, B - BGP
D - EIGRP, EX - EIGRP external, O - OSPF, IA - OSPF inter area
N1 - OSPF NSSA external type 1, N2 - OSPF NSSA external type 2
E1 - OSPF external type 1, E2 - OSPF external type 2, E - EGP
i - IS-IS, L1 - IS-IS level-1, L2 - IS-IS level-2, ia - IS-IS inter area
* - candidate default, U - per-user static route, o - ODR
P - periodic downloaded static route

Gateway of last resort is not set

185.95.0.0/16 is variably subnetted, 6 subnets, 3 masks
C 185.95.3.0/24 is directly connected, GigabitEthernet0/0
L 185.95.3.1/32 is directly connected, GigabitEthernet0/0
C 185.95.13.0/30 is directly connected, Serial0/0/0
L 185.95.13.2/32 is directly connected, Serial0/0/0
C 185.95.23.0/30 is directly connected, Serial0/0/1
L 185.95.23.2/32 is directly connected, Serial0/0/1

R3#show ip ospf neighbor

R3#
R3#
R3#show ip ospf database
R3#
R3#
R3#
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Programming  Aftrbu

Packet Tracer BC Command Line 1.0
C:\>ping 1855533

Pinging 185.55.3.3 with 32 byres of data:

Reply from 185.55
Reply from 18555
Reply from 18555
Reply from 185 55

Destination host unreachable
Destination host unreachable
Destination host unreachable

Destination host unreachable

Ping scavistics for 185.55.3.3
Packets: Sent = 4, Received = 0, Lost = 4 (100% loss),
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