R1#show run
Building configuration...

Current configuration : 959 bytes
!
version 15.1
no service timestamps log datetime msec
no service timestamps debug datetime msec
no service password-encryption
!
hostname R1
!
!
!
!
!
!
!
!
no ip cef
no ipv6 cef
!
!
!
!
license udi pid CISCO2911/K9 sn FTX152434C8-
!
!
!
!
!
!
!
!
!
!
!
spanning-tree mode pvst
!
!
!
!
!
!
interface GigabitEthernet0/0
description Link to PCA
ip address 185.95.1.1 255.255.255.0
duplex auto
speed auto
!
interface GigabitEthernet0/1
no ip address
duplex auto
speed auto
shutdown
!
interface GigabitEthernet0/2
no ip address
duplex auto
speed auto
shutdown
!
interface Serial0/3/0
description Link to R2
ip address 185.95.12.1 255.255.255.252
clock rate 9600
!
interface Serial0/3/1
description Link to R3
ip address 185.95.13.1 255.255.255.252
!
interface Vlan1
no ip address
shutdown
!
ip classless
!
ip flow-export version 9
!
!
!
banner motd ^CThis is a secure message^C
!
!
!
!
!
line con 0
!
line aux 0
!
line vty 0 4
login
!
!
!
end


R1#
R1#show run
Building configuration...

Current configuration : 959 bytes
!
version 15.1
no service timestamps log datetime msec
no service timestamps debug datetime msec
no service password-encryption
!
hostname R1
!
!
!
!
!
!
!
!
no ip cef
no ipv6 cef
!
!
!
!
license udi pid CISCO2911/K9 sn FTX152434C8-
!
!
!
!
!
!
!
!
!
!
!
spanning-tree mode pvst
!
!
!
!
!
!
interface GigabitEthernet0/0
description Link to PCA
ip address 185.95.1.1 255.255.255.0
duplex auto
speed auto
!
interface GigabitEthernet0/1
no ip address
duplex auto
speed auto
shutdown
!
interface GigabitEthernet0/2
no ip address
duplex auto
speed auto
shutdown
!
interface Serial0/3/0
description Link to R2
ip address 185.95.12.1 255.255.255.252
clock rate 9600
!
interface Serial0/3/1
description Link to R3
ip address 185.95.13.1 255.255.255.252
!
interface Vlan1
no ip address
shutdown
!
ip classless
!
ip flow-export version 9
!
!
!
banner motd ^CThis is a secure message^C
!
!
!
!
!
line con 0
!
line aux 0
!
line vty 0 4
login
!
!
!
end


R1#
R1#
R1#show run
Building configuration...

Current configuration : 959 bytes
!
version 15.1
no service timestamps log datetime msec
no service timestamps debug datetime msec
no service password-encryption
!
hostname R1
!
!
!
!
!
!
!
!
no ip cef
no ipv6 cef
!
!
!
!
license udi pid CISCO2911/K9 sn FTX152434C8-
!
!
!
!
!
!
!
!
!
!
!
spanning-tree mode pvst
!
!
!
!
!
!
interface GigabitEthernet0/0
description Link to PCA
ip address 185.95.1.1 255.255.255.0
duplex auto
speed auto
!
interface GigabitEthernet0/1
no ip address
duplex auto
speed auto
shutdown
!
interface GigabitEthernet0/2
no ip address
duplex auto
speed auto
shutdown
!
interface Serial0/3/0
description Link to R2
ip address 185.95.12.1 255.255.255.252
clock rate 9600
!
interface Serial0/3/1
description Link to R3
ip address 185.95.13.1 255.255.255.252
!
interface Vlan1
no ip address
shutdown
!
ip classless
!
ip flow-export version 9
!
!
!
banner motd ^CThis is a secure message^C
!
!
!
!
!
line con 0
!
line aux 0
!
line vty 0 4
login
!
!
!
end


R1#
R1#





R2#show run
Building configuration...

Current configuration : 959 bytes
!
version 15.1
no service timestamps log datetime msec
no service timestamps debug datetime msec
no service password-encryption
!
hostname R2
!
!
!
!
!
!
!
!
no ip cef
no ipv6 cef
!
!
!
!
license udi pid CISCO2911/K9 sn FTX15245IF2-
!
!
!
!
!
!
!
!
!
!
!
spanning-tree mode pvst
!
!
!
!
!
!
interface GigabitEthernet0/0
description Link to PCB
ip address 185.95.2.1 255.255.255.0
duplex auto
speed auto
!
interface GigabitEthernet0/1
no ip address
duplex auto
speed auto
shutdown
!
interface GigabitEthernet0/2
no ip address
duplex auto
speed auto
shutdown
!
interface Serial0/3/0
description Link to R1
ip address 185.95.12.2 255.255.255.252
!
interface Serial0/3/1
description Link to R3
ip address 185.95.23.1 255.255.255.252
clock rate 9600
!
interface Vlan1
no ip address
shutdown
!
ip classless
!
ip flow-export version 9
!
!
!
banner motd ^CThis is a secure message^C
!
!
!
!
!
line con 0
!
line aux 0
!
line vty 0 4
login
!
!
!
end


R2#
R2#
R2#
R2#
R2#show ip
R2#show ip in
R2#show ip interface br
R2#show ip interface brief 
Interface IP-Address OK? Method Status Protocol 
GigabitEthernet0/0 185.95.2.1 YES manual up up 
GigabitEthernet0/1 unassigned YES unset administratively down down 
GigabitEthernet0/2 unassigned YES unset administratively down down 
Serial0/3/0 185.95.12.2 YES manual up up 
Serial0/3/1 185.95.23.1 YES manual up up 
Vlan1 unassigned YES unset administratively down down
R2#
R2#
R2#
R2#
R2#show ip route 
Codes: L - local, C - connected, S - static, R - RIP, M - mobile, B - BGP
D - EIGRP, EX - EIGRP external, O - OSPF, IA - OSPF inter area
N1 - OSPF NSSA external type 1, N2 - OSPF NSSA external type 2
E1 - OSPF external type 1, E2 - OSPF external type 2, E - EGP
i - IS-IS, L1 - IS-IS level-1, L2 - IS-IS level-2, ia - IS-IS inter area
* - candidate default, U - per-user static route, o - ODR
P - periodic downloaded static route

Gateway of last resort is not set

185.95.0.0/16 is variably subnetted, 6 subnets, 3 masks
C 185.95.2.0/24 is directly connected, GigabitEthernet0/0
L 185.95.2.1/32 is directly connected, GigabitEthernet0/0
C 185.95.12.0/30 is directly connected, Serial0/3/0
L 185.95.12.2/32 is directly connected, Serial0/3/0
C 185.95.23.0/30 is directly connected, Serial0/3/1
L 185.95.23.1/32 is directly connected, Serial0/3/1

R2#
















R3#show run
Building configuration...

Current configuration : 959 bytes
!
version 15.1
no service timestamps log datetime msec
no service timestamps debug datetime msec
no service password-encryption
!
hostname R3
!
!
!
!
!
!
!
!
no ip cef
no ipv6 cef
!
!
!
!
license udi pid CISCO2911/K9 sn FTX1524K4PH-
!
!
!
!
!
!
!
!
!
!
!
spanning-tree mode pvst
!
!
!
!
!
!
interface GigabitEthernet0/0
description Link to PCC
ip address 185.95.3.1 255.255.255.0
duplex auto
speed auto
!
interface GigabitEthernet0/1
no ip address
duplex auto
speed auto
shutdown
!
interface GigabitEthernet0/2
no ip address
duplex auto
speed auto
shutdown
!
interface Serial0/3/0
description Link to R1
ip address 185.95.13.2 255.255.255.252
clock rate 9600
!
interface Serial0/3/1
description Link to R2
ip address 185.95.23.2 255.255.255.252
!
interface Vlan1
no ip address
shutdown
!
ip classless
!
ip flow-export version 9
!
!
!
banner motd ^CThis is a secure message^C
!
!
!
!
!
line con 0
!
line aux 0
!
line vty 0 4
login
!
!
!
end


R3#
R3#

R3#show ip interface b
R3#show ip interface brief 
Interface IP-Address OK? Method Status Protocol 
GigabitEthernet0/0 185.95.3.1 YES manual up up 
GigabitEthernet0/1 unassigned YES unset administratively down down 
GigabitEthernet0/2 unassigned YES unset administratively down down 
Serial0/3/0 185.95.13.2 YES manual up up 
Serial0/3/1 185.95.23.2 YES manual up up 
Vlan1 unassigned YES unset administratively down down
R3#

R3#show ip route 
Codes: L - local, C - connected, S - static, R - RIP, M - mobile, B - BGP
D - EIGRP, EX - EIGRP external, O - OSPF, IA - OSPF inter area
N1 - OSPF NSSA external type 1, N2 - OSPF NSSA external type 2
E1 - OSPF external type 1, E2 - OSPF external type 2, E - EGP
i - IS-IS, L1 - IS-IS level-1, L2 - IS-IS level-2, ia - IS-IS inter area
* - candidate default, U - per-user static route, o - ODR
P - periodic downloaded static route

Gateway of last resort is not set

185.95.0.0/16 is variably subnetted, 6 subnets, 3 masks
C 185.95.3.0/24 is directly connected, GigabitEthernet0/0
L 185.95.3.1/32 is directly connected, GigabitEthernet0/0
C 185.95.13.0/30 is directly connected, Serial0/3/0
L 185.95.13.2/32 is directly connected, Serial0/3/0
C 185.95.23.0/30 is directly connected, Serial0/3/1
L 185.95.23.2/32 is directly connected, Serial0/3/1

R3#
R3#
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