Method Statement
	Project title:
	Tai Tarian Office build

	Reference:
	TT052020

	Date:
	31.03.20



Description of Works
	Scope:
	Pad Foundation concrete casting

	Method of work:
	Following excavations. Prepare site.  Install rebar and concrete fill

	Duration:
	2 weeks

	Sequence:







	Reinforcement: 
· Cut and bend rebar on-site as per specification. 
· Support bars with concrete blocks.
·  Allow for inspection prior to casting.
Casting: 
· Clear areas of all debris
· Readymade concrete brought to site – hourly supply as per specification 
· Vibration plant in place at time of casting
· Site personal to check composition of concrete to confirm correct mix (delivery schedule) Temperature to be checked as per specification.
· Record all data on site – ensure local supply can reach site in the timescales required
· Concrete should undergo vibration at various intervals – follow spec – to ensure sufficient fill
· Apply water proofer according to spec.
· Inspection by Site Engineer on completion

	Location:
	Baglan Bay site



Resources required
	Personnel: 
	Site labour, Engineer and Site Manager

	Supervision:
	Site Manager

	Plant/Equipment 
	Crane, concrete mixer, vibrators, total station, trowel, level, shovel, wheelbarrow

	Materials:
	Rebars, conc block, concrete brought to site ready made



Assessment of Risks
	Access to site:
	

	Area of work:
	

	Staff at risk:
	

	Staff competence (sufficient training completed?)
	CSCS card for general labour, Site Engineer and Manager suitably qualified. 



Control Measures in place
	Permits:
	
n/a

	Security:
	On site

	Other:
	[bookmark: _GoBack]n/a



