Switch con0 is now available





Press RETURN to get started.


Switch>
Switch>
Switch>
Switch>enable
Switch#config t
Enter configuration commands, one per line.  End with CNTL/Z.
Switch(config)#hostname S1
S1(config)#enable password class
S1(config)#line console 0
S1(config-line)#password cisco
S1(config-line)#login
S1(config-line)#exit
S1(config)#enable secret class
The enable secret you have chosen is the same as your enable password.
This is not recommended.  Re-enter the enable secret.

S1(config)#service password-encryption
S1(config)#banner motd #Unathorized access is strictly prohibited#
S1(config)#no domain-lookup
                ^
% Invalid input detected at '^' marker.

S1(config)#no ip domain-lookup
S1(config)#
*Mar  1 04:20:33.143: %LINK-3-UPDOWN: Interface FastEthernet0/10, changed state to up
*Mar  1 04:20:34.150: %LINEPROTO-5-UPDOWN: Line protocol on Interface FastEthernet0/10, changed state to up
*Mar  1 04:21:01.169: %LINEPROTO-5-UPDOWN: Line protocol on Interface Vlan1, changed state to up
S1(config)#int vlan1
S1(config-if)#ip address 172.16.2.60 255.255.255.192
S1(config-if)#no shutdown
S1(config-if)#exit
S1(config)#ip default-gateway 172.16.2.1
S1(config)#exit
S1#
*Mar  1 04:36:10.235: %SYS-5-CONFIG_I: Configured from console by consoles
% Type "show ?" for a list of subcommands
S1#show run
Building configuration...

Current configuration : 1492 bytes
!
version 12.2
no service pad
service timestamps debug datetime msec
service timestamps log datetime msec
service password-encryption
!
hostname S1
!
boot-start-marker
boot-end-marker
!
enable secret 5 $1$cHPu$WVreAlKvtaQdIN3QUojlQ.
enable password 7 14141E0A1F17
!
!
!
no aaa new-model
system mtu routing 1500
no ip domain-lookup
!

S1#config t
Enter configuration commands, one per line.  End with CNTL/Z.
S1(config)#enable secret
% Incomplete command.

S1(config)#service password-encryption
S1(config)#line vty 0 15
S1(config-line)#password cisco
S1(config-line)#login
S1(config-line)#exit
S1(config)#
S1#
*Mar  1 04:39:34.321: %SYS-5-CONFIG_I: Configured from console by consoles
% Type "show ?" for a list of subcommands
S1#
S1#copy run startup
Destination filename [startup-config]?
Building configuration...
[OK]
0 bytes copied in 0.965 secs (0 bytes/sec)
S1#
S1#
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*Mar  1 04:50:38.355: %LINK-3-UPDOWN: Interface FastEthernet0/1, changed state to up
*Mar  1 04:50:39.361: %LINEPROTO-5-UPDOWN: Line protocol on Interface FastEthernet0/1, changed state to upUnathorized access is strictly prohibited

User Access Verification

Password:
S1>enable
Password:
Password:
S1#show run
Building configuration...

Current configuration : 1542 bytes
!
version 12.2
no service pad
service timestamps debug datetime msec
service timestamps log datetime msec
service password-encryption
!
hostname S1
!
boot-start-marker
boot-end-marker
!
enable secret 5 $1$cHPu$WVreAlKvtaQdIN3QUojlQ.
enable password 7 14141E0A1F17
!
!
!
no aaa new-model
system mtu routing 1500
no ip domain-lookup
!
!
!
!
!
!
!
!
spanning-tree mode pvst
spanning-tree extend system-id
!
vlan internal allocation policy ascending
!
!
!
interface FastEthernet0/1
!
interface FastEthernet0/2
!
interface FastEthernet0/3
!
interface FastEthernet0/4
!
interface FastEthernet0/5
!
interface FastEthernet0/6
!
interface FastEthernet0/7
!
interface FastEthernet0/8
!
interface FastEthernet0/9
!
interface FastEthernet0/10
!
interface FastEthernet0/11
!
interface FastEthernet0/12
!
interface FastEthernet0/13
!
interface FastEthernet0/14
!
interface FastEthernet0/15
!
interface FastEthernet0/16
!
interface FastEthernet0/17
!
interface FastEthernet0/18
!
interface FastEthernet0/19
!
interface FastEthernet0/20
!
interface FastEthernet0/21
!
interface FastEthernet0/22
!
interface FastEthernet0/23
!
interface FastEthernet0/24
!
interface GigabitEthernet0/1
!
interface GigabitEthernet0/2
!
interface Vlan1
 ip address 172.16.2.60 255.255.255.192
!
ip default-gateway 172.16.2.1
ip classless
ip http server
ip http secure-server
!
!
banner motd ^CUnathorized access is strictly prohibited^C
!
line con 0
 password 7 1511021F0725
 login
line vty 0 4
 password 7 094F471A1A0A
 login
line vty 5 15
 password 7 094F471A1A0A
 login
!
end
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