A). State the benefits of using Type 2 Hypervisor virtualisation software in your design.  Comment on the strengths and weaknesses of the VirtualBox platform used in your network.	Comment by John Rees: Needs more!
[1]One of the many advantages of type 2 hypervisor is that you don’t need to modify operating system or the function programme to run on the virtual environment
One of the disadvantages is that they only run on one operating system as a server and a client e.g. have to choose from Microsoft or Linux.

B). Explain, with use of diagrams, the significance of the following terms:  Active Directory Forests, Trees, Parent and Child Domains	Comment by John Rees: The diagram is fine, of itself, but it doesn’t answer all the question – forest and domain controller, parent and child domain, yes; trees, no.
Also, even though it shows decent research, it doesn’t demonstrate your understanding.  You get more marks for putting it in your own words/diagram.
[2][image:  ]



[3]
C ). Investigate [endnoteRef:1]and document the main roles and responsibilities of an Active Directory Domain Controller	Comment by John Rees: Again, this is partial, and needs to consider other aspects of the role [1: Installing client (windows 7) 


Pinging our client and server so can see if they are receiving each other 

Created the domain 


Image shows dhcp finalised.] 

Schema Master FSMO Role
Schema master is responsible for running the mater copy and performing updates. Only the schema master is allowed to do updates. Once the updates are complete then it gets passed to all the other domains. 
Domain Naming Master FSMO Role
The domain naming master is the only domain which can add and remove clients from the domain.
RID Master FSMO Role
Is responsible for removing and moving an object to another domain.
D). What actions could we take in the event of a Domain Controller becoming unavailable?
[bookmark: _GoBack]If the domain controller breaks or not functioning, you must search each domain controller one at a time on the server searching for backups from other domain controllers which will recover a older domain.  	Comment by John Rees: Normally nominate a secondary domain controller as part of the set up.
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[Ping statistics for 192.168.100
Packets: Sent = 4, Received

[poproxinate round trip times in milli-seconds:
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c:\Users\Adnint>
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Do

3

Microsoft Windows [Uersion 6.1.76811

Users\Adninistrator>ping 192.168.100.1
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Ping statistics for 192.168.100.1
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round trip times in milii
Bne, Maxinum = Ons, Average
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