Project 071
	Input
	Frequency
	Output

	0.2 p to p
	1.4 kHz
	300 mV peak

	
	10 kHz
	

	
	25 kHz
	

	
	50 kHz
	

	
	100 kHz
	

	
	150 kHz
	

	
	200 kHz
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Measurements
	Component
	Resistance
	Voltage
	Current(ma)

	R1
	1k
	2.64
	2.64

	R2
	500R
	0.43
	0.85

	R3
	10K5
	8.94
	0.85

	R4
	10K
	9.36
	0.94

	R5
	9K5
	8.08
	0.85

	R6
	500R
	0.43
	0.85

	R7
	1K
	0.85
	0.85
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project easy pc
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What was wrong with it?
The circuit was at fault for the lines not going to the correct positions also I had the resistors the wrong way round as you can see compared to the second picture. All I had to do was change one of the values from 12v to ground.
Results of this project easy pc (Front board)
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Results of this project easy pc (Back board)
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