6.0 Accommodation Requirements 
6.1 Space Requirements 
	The Client brief states to construct a state of the art Health Centre and requirements are:
· Reception/Welcome area 
· Library space 
· Culinary classroom 
· Gym with designated training areas
· Changing rooms
· Multifunction Room 
· Treatment Information Centre & Waiting Room
· Cryo Chambers 
· Massage Room 
· Sauna & Steam Room 
· Toilets 
· Rooftop Bar 
· Rooftop pool 
· Circulation space 
· Stores 
· Plant room 
· Supplement Bar 
· Offices 
· Wellness Garden 
· Coaching Parking 
· DDA Parking 
· Electric Charging 
6.2 Comparison with similar schemes previously undertaken
	Previous schemes reviewed and All requirements similar to previous schemes 
6.3 Services Requirements 
	New mains services & drainage will need to be installed when ground works being carried out to power/run then new leisure centre. New data will also be required to operate and use the building efficiently. The building will need an EMS which measures the below:
· Ground floor and first floor distribution board
· Air conditioning 
· MCC-02 Air Handling Units 
· Pool Plant room control Panel 
· Main Electricity incomer 
· Main Gas Meter 
· Main Water Meter 
· DHW Water Meter 
External Swimming Pool 
· Heat Pumps 
· Lighting 
Changing rooms HVAC  
· Heating via a dedicated ventilation system
· Plate heat exchanger 
· Openable high-level windows for natural ventilation in summer where possible. 
· Lighting 
· Corrosion resistant IP65+ 
· LED * bulkhead fittings or high efficiency fluorescent fittings.  
Fitness suite and studios HVAC  
· Heating and cooling provided via dedicated ventilation system 
· Comfort cooling provided by chilled water or VRF system. 
· Lighting 
· Recessed modular LED or high efficiency fluorescent fittings.  
Offices, staff room, Library and circulation HVAC  
· LST radiators
· Natural ventilation via manual openable windows where possible, mechanical ventilation for internal spaces. 
· Lighting 
· LED recessed downlighters or high efficiency fluorescent fittings 
Culinary Classroom 
· LST radiators 
· Mechanically ventilated canopy 
· Lighting 
Treatment Room
· Heating and cooling provided via dedicated ventilation system 
· Comfort cooling provided by chilled water or VRF system. 
· Lighting 
· Recessed modular LED or high efficiency fluorescent fittings.  
6.4 External Works 
	The Project has been proposed to have a wellness garden along with parking and road alterations. The wellness garden will consist of a mixture of hard & soft landscaping along with a variety of trees & plants. There is currently a roundabout in the middle of the site which needs to be removed at set up stage due to the location and masterplan design. There will also be alterations to the exiting car park to accommodate the new requirements, which will consist of coach parking, electric charging, DDA parking & standard parking. 
6.7 Customer supplied equipment/Furniture 
	As discussed, and agreed in previous meeting, No customer supplied equipment/furniture 
6.8 Alternative accommodation proposals/design 
	As discussed, and agreed in previous meeting, no alternative design/proposal accepted. Client has confirmed, only acceptance of proposed masterplan design & location 
6.9 Access for disabled persons 
	Building Regulation Part M must be reviewed and considered when designing and constructing the building. The following points/requirements must be complied with to get building regulation sign off:
· Access to and from the building and amenities.
· Car Park areas and sizes. 
· Access into the building for the general public and staff (Level Access, Ramps)
· Access through the Building – dimensions of hallways, doors, lifts. 
· The Design would also need to consider colour contrasting through the development to enable the visually impaired to navigate through the areas.
· Consideration must be made in installing Low Service Temperature (LST) heating devices through the buildings to prevent the young and persons with disabilities with burning. 
6.10 Security 
Site Security will consist of solid hoarding around the perimeter of the site with vehicle/pedestrian gate/turnstiles to access site. a designate gate man will be assigned to control access along with signing in & out operatives. Security cameras will be installed throughout site for security out of hours. 
6.11 Flexibility of use 
6.12 Phasing/Decanting 
	Due to the size of the site as a whole and the overall requirements for the client, phased handovers would not be a practical solution to the delivery of this scheme. The compound will be away from the main building and will be decanted to the end of the project. At PC stage the only remaining items will be site office/welfare & Hoarding. These will be stripped day before handover. 

	 

