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Lab - Building an Ethernet Crossover Cable

Lab – Understanding Ethernet Cable Standards 
Topology
[image: ]
Addressing Table
	Device
	Interface
	IP Address
	Subnet Mask
	Default Gateway

	PC-A
	NIC
	192.168.10.1
	255.255.255.0
	N/A

	PC-B
	NIC
	192.168.10.2
	255.255.255.0
	N/A


Objectives
Part 1: Analyze Ethernet Cabling Standards and Pinouts
Part 2: Build an Ethernet Crossover Cable
Part 3: Test an Ethernet Crossover Cable
Background / Scenario
In this lab, you will build and terminate an Ethernet crossover cable and test it by connecting two PCs together and pinging between them. You will first analyze the Telecommunications Industry Association/Electronic Industries Association (TIA/EIA) 568-A and 568-B standards and how they apply to Ethernet cables. You will then construct an Ethernet crossover cable and test it. Finally, you will use the cable you just constructed to connect two PCs together and test it by pinging between them.
Note: With autosensing capabilities available on many devices, such as the Cisco 1941 Integrated Services Router (ISR) switch, you may see straight-through cables connecting like devices.
Required Resources
One length of cable, either Category 5 or 5e. Cable length should be 0.6 to 0.9m (2 to 3 ft.)
2 RJ-45 connectors
RJ-45 crimping tool
Wire cutter
Wire stripper
Ethernet cable tester (optional)
2 PCs (Windows 7 or 8)
Analyze Ethernet Cabling Standards and Pinouts
The TIA/EIA has specified unshielded twisted pair (UTP) cabling standards for use in LAN cabling environments. TIA/EIA 568-A and 568-B stipulates the commercial cabling standards for LAN installations; these are the standards most commonly used in LAN cabling for organizations and they determine which color wire is used on each pin.
With a crossover cable, the second and third pairs on the RJ-45 connector at one end of the cable are reversed at the other end, which reverses the send and receive pairs. The cable pinouts are the 568-A standard on one end and the 568-B standard on the other end. Crossover cables are normally used to connect hubs to hubs or switches to switches, but they can also be used to directly connect two hosts to create a simple network.
Reflection: 
Write a research report (Max word count 600) on Cat 5e and 6 Ethernet cable standards. 

The IEEE which stands for electrical and electronic engineers institute stands for IEE. The most popular technology used today is LAN. Standard 802. The IEEE links up with the IOS model. IEEE 802  network are carried out to carry packets. It uses carrier sense. You have different types of cables you have coaxial cables, optical fiber cables, and multi-channel coaxial cable. Optical fiber is the most used because it is fastest and low interrupted. You also have copper inside a wire, a solid cable and a standard cable which has series of copper. Cables also have topology as well which goes with certain types of design. [1]
[bookmark: _GoBack]cat 5 and cat 6 are cables. It allows you to connect to the internet using ethernet. The difference between them physically that they look different. Cat 5 and cat 5 e is unshielded. They both have different speeds.  A shielded cable is more protective than a non-shielded. It is also much faster than a non-shielded one.  The cat 5//5e and cat 6/6a are different they have a plastic pipe in it. There are also different differences which are the cable length, etc. shielded are there to stop crosstalk. Cross talk is electric interference when signals affect another wire signal so the wire being shielded to stop that interference. It can cause loss of service and loss of data.  You have different networking cable which are U/TP, F/UTP, U/FTP, S/FTP. TP stands for twisted pair. U stands for unshielded. F stands for foil shielding and S stands for braided shielding.  The shielding is there to stop crosstalk because that affects the performance highly. [1]
There is also different type of wires. You have solid and standard. A solid use one single piece of copper. While stranded uses a series of copper cables twisted together.  A stranded is more flexible and a solid cable is not flexible.  When it comes to topology of networking, and wires. There different types and have IEEE standards.
[1]CAT 5 is not shielded and the maximum transmission speed is 10/100 Mbps and the maximum speed is 100 mhz which is slow comparing to cat 5e speeds, and cat 6.
While cat 5e speed is 1000mbps/1gbps and 100 mhz. CAT 5 cables are very slow comparing to cat 5e. CAT 5E is up to 10 times faster speeds and doesn’t get affected by crosstalk. CAT 5 would be slow if you used it today comparing cat 5e and cat6.  Cat5E stands for category 5 enhanced cable. Cat5E is the most common type of cabling used because it supports gigabit and it is reasonable price comparing to cat 6 which is used at high end networking.
[1]CAT 6 cable can be shielded or unshielded. It is the same speed as 5e and the maximum bandwidth is 250 mhz which is much better than cat 5e. It is also more expensive than 5e.  CAT 6a shielded and the maximum transmission is 1000 MBPS/1gbps and 250 maximum bandwidth is 500mhz. cat 6 cables support higher bandwidths than CAT5 or cat5e. They are built differently. There built to stop crosstalk and noise interference. When you have crosstalk and noise interference, they slow down the internet because of interruptions. Cat 6 is much faster than cat 5e it is more protected and can prevent crosstalk.  Cat 6 are used in for high end networking. There are many other different cables cat 7, cat 8.  
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Analyze diagrams and tables for the TIA/EIA 568-A standard Ethernet cable.
The following table and diagrams display the color scheme and pinouts, as well as the function of the four pairs of wires used for the 568-A standard. 
Note: In LAN installations using 100Base-T (100 Mb/s), only two pairs out of the four are used.
568-A 10/100/1000Base-TX Ethernet
	Pin Number
	Pair Number
	Wire Color
	10Base-T Signal
100Base-TX Signal
	1000Base-T Signal

	1
	2
	White/Green
	Transmit
	BI_DA+

	2
	2
	Green
	Transmit
	BI_DA-

	3
	3
	White/Orange
	Receive
	BI_DB+

	4
	1
	Blue
	Not Used
	BI_DC+

	5
	1
	White/Blue
	Not Used
	BI_DC-

	6
	3
	Orange
	Receive
	BI_DB-

	7
	4
	White/Brown
	Not Used
	BI_DD+

	8
	4
	Brown
	Not Used
	BI_DD-




The following diagrams display how the wire color and pinouts align with an RJ-45 jack for the 568-A standard.
[image: T-568A]
[image: RJ-45 Jack]
Analyze diagrams and tables for the TIA/EIA 568-B standard Ethernet cable.
The following table and diagram display the color scheme and pinouts for the 568-B standard.
568-B 10/100/1000-BaseTX Ethernet
	Pin Number
	Pair Number
	Wire Color
	10Base-T Signal
100Base-TX Signal
	1000Base-T Signal

	1
	2
	White/Orange
	Transmit
	BI_DA+

	2
	2
	Orange
	Transmit
	BI_DA-

	3
	3
	White/Green
	Receive
	BI_DB+

	4
	1
	Blue
	Not Used
	BI_DC+

	5
	1
	White/Blue
	Not Used
	BI_DC-

	6
	3
	Green
	Receive
	BI_DB-

	7
	4
	White/Brown
	Not Used
	BI_DD+

	8
	4
	Brown
	Not Used
	BI_DD-


[image: T568B_ColorPinout_AndRJ45Jack]


Build an Ethernet Crossover Cable
A crossover cable has the second and third pairs on the RJ-45 connector at one end, reversed at the other end (refer to the table in Part 1, Step 2). The cable pinouts are the 568-A standard on one end and the 568-B standard on the other end. The two following diagrams illustrate this concept.
[image: Cross_over_CableRJ45Connectors_1]
Build and terminate a TIA/EIA 568-A cable end.
Determine the cable length required. (Your instructor will let you know the cable length you should make.)
Note: If you were making a cable in a production environment, the general guideline is to add another 12 in. (30.48 cm) to the length.
Cut off a piece of cable to the desired length and using your wire stripper, remove 5.08 cm (2 in.) of the cable jacket from both ends.
Hold the four pairs of twisted cables tightly where the jacket was cut away. Reorganize the cable pairs into the order of the 568-A wiring standard. Refer to the diagrams, if necessary. Take as much care as possible to maintain the twists in the cable; this provides noise cancellation.
Flatten, straighten, and line up the wires using your thumb and forefinger.
Ensure that the cable wires are still in the correct order for the 568-A standard. Using your wire cutters, trim the four pairs in a straight line to within 1.25 to 1.9 cm (1/2 to 3/4 in.).
Place an RJ-45 connector on the end of your cable, with the prong on the underside pointing downward. Firmly insert the wires into the RJ-45 connector. All wires should be seen at the end of the connector in their proper positions. If the wires are not extending to the end of the connector, take the cable out, rearrange the wires as necessary, and reinsert the wires back into the RJ-45 connector.
If everything is correct, insert the RJ-45 connector with cable into the crimper. Crimp down hard enough to force the contacts on the RJ-45 connector through the insulation on the wires, thus completing the conducting path. See the following diagram for an example.
[image: crimp_Pic]
Build and terminate a TIA/EIA 568-B cable end.
Repeat steps 1a to 1g using the 568-B color wiring scheme for the other end.
Test an Ethernet Crossover Cable
Test the cable.
Many cable testers will test for length and mapping of wires. If the cable tester has a wire map feature, it verifies which pins on one end of the cable are connected to which pins on the other end.
If your instructor has a cable tester, test the crossover cable for functionality. If it fails, check with your instructor first as to whether you should re-cable the ends and re-test.
Connect two PCs together via NICs using your Ethernet crossover cable.
Working with a lab partner, set your PC to one of the IP addresses shown in the Addressing Table (see page 1). For example, if your PC is PC-A, your IP address should be set to 192.168.10.1 with a 24-bit subnet mask. You partner’s IP address should be 192.168.10.2. The default gateway address can be left empty.
Using the crossover cable you made, connect the two PCs together via their NICs.
On the PC-A command prompt, ping the PC-B IP address.
Note: The Windows firewall may have to be temporarily disabled for pings to be successful. If the firewall is disabled, make sure you re-enable it at the conclusion of this lab.
Repeat the process and ping from PC-B to PC-A.
Assuming IP addressing and firewall are not issues, your pings should be successful if the cables were properly made.
Reflection
Which part of making cables did you find the most difficult?
Lining up the wires and clipping it together
Why do you have to learn how to make a cable if you can easily buy pre-made cables?
A cable may not suit a topology. It also can be expensive to buy pre-made cables. 
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