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This is an individual practical test, held under examination conditions. You will be assigned three Switches and three Routers; you should configure these devices based on the given specifications. 

This paper is marked out of 100.
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Addressing Table
	Device
	Interface
	IP Address
	Subnet Mask
	Default Gateway

	R1
	G0/1
	192.168.0.1
	255.255.255.0
	N/A

	
	S0/0/0
	192.168.123.1
	255.255.255.252
	N/A

	
	Lo1
	192.168.1.1
	255.255.255.0
	N/A

	
	Lo2
	192.168.2.1
	255.255.255.0
	N/A

	
	Lo3
	192.168.3.1
	255.255.255.0
	N/A

	R2
	S0/0/0
	192.168.123.2
	255.255.255.252
	N/A

	
	S0/0/1
	192.168.123.5
	255.255.255.252
	N/A

	
	Lo0
	209.165.200.225
	255.255.255.248
	N/A

	R3
	G0/1
	192.168.0.3
	255.255.255.0
	N/A

	
	S0/0/1
	192.168.123.6
	255.255.255.252
	N/A

	
	Lo4
	192.168.4.1
	255.255.255.0
	N/A

	
	Lo5
	192.168.5.1
	255.255.255.0
	N/A

	
	Lo6
	192.168.6.1
	255.255.255.0
	N/A

	S1
	VLAN 6
	192.168.0.11
	255.255.255.0
	192.168.0.2

	S2
	VLAN 6
	192.168.0.12
	255.255.255.0
	192.168.0.2

	S3
	VLAN 6
	192.168.0.13
	255.255.255.0
	192.168.0.2

	PC-A
	NIC
	192.168.0.21
	255.255.255.0
	192.168.0.2

	PC-B
	NIC
	192.168.0.22
	255.255.255.0
	192.168.0.2

	PC-C
	NIC
	192.168.0.23
	255.255.255.0
	192.168.0.2


VLAN Table
	VLAN
	VLAN Name
	Ports

	2
	Sales
	Fa0/7 - 9

	3
	Finance
	Fa0/10 – 12

	4
	Guest
	Fa0/13 – 16

	5
	Warehouse
	Fa0/21– 24

	6
	Management & Native
	Fa0/6, Fa0/17 - 20



Task 1: - Topology Creation (5 marks)
Using Packet Tracer software create the topology shown above and complete all tasks below. 
· Configure hostnames on each device.
· Disable DNS lookup on all routers
· Configure all devices with IP address shown in the above tables and network topology.

Task 2: - Device Configuration (80 marks)
1. Configure RIPv2 on R1, R2 & R3. Advertise directly connected Networks. Disable automatic summarization. 
2. Set Router ID, 1.1.1.1 on R1, 2.2.2.2 on R2 and 3.3.3.3 on R3.
3. Set the bandwidth on serial links to 256kbps. 
4. On R2, configure default route using Lo0 as exit interface and propagate the default route to all other RIP routes.
5. Configure S1 as VTP Server and S2 and S3 as clients. Use soac.com as domain and set uwtsd as password. 
6. Configure VLANs as shown in the table.
7.  Force trunking on interfaces connected between switches. Use VLAN 6 as native VLAN.  
8. Configure PortFast and BPDU Guard on the interfaces connected to PCs. Shutdown all unused ports.  
9. On all switches, configure Rapid PVST as spanning tree mode. 
10. Configure S1 with root priority of 24576 and S3 with 28672.
11. Enable port security on ports connected to end devices. Set the maximum so that only one device can access the Fast Ethernet ports. 
12. Secure the ports so that the MAC address of a device is dynamically learned and added to the running configuration.   Set the violation mode so that the Fast Ethernet ports are not disabled when a violation occurs, but a notification of the security violation is generated and packets from the unknown source are dropped
13. On S1, configure an PAgP EtherChannel on interfaces connected to each other. Use group 1 and enable PAgP unconditionally.
14. On S3, configure an PAgP EtherChannel on interfaces connected to S1. Use group 1 and enable PAgP only if a PAgP device is detected.
15. Configure HSRP on R1 and R3. Group: 1, Virtual IP address: 192.168.0.2. Make R1 as the primary router. 

Task3: Network connectivity (10 marks) 
Using ping command, verify end-to-end connectivity:
From PC-A, ping PC-B & PC-C. Is it successful? ___no_____
From PC-A, ping default gateway. Is it successful? ___no_____
From PC-B, ping 192.168.0.1. Is it successful? __no_____
From PC-A, ping 209.165.200.225. Is it successful? ___no_____

Verify HSRP is working as expected
Issue the shutdown command on R1 G0/1, and then re-issue the following commands to verify that HSRP is working as expected:
From PC-B, ping 192.168.0.1. Ping should not be successful ___no___
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From PC-B, ping default gateway. Is it successful? ___no_____
From PC-B, ping 209.165.200.225. Is it successful? __no_____


Submission Requirement 
The packet tracer file should be saved as “studentname_id” and uploaded onto Moodle. In addition to packet tracer file, you must also submit 

· the output of show running-configuration command in a text file for all devices configured. 
· This document with Task 3 completed 

All documentation for your solution should be submitted electronically on Moodle.
It is your responsibility that you submit all the outputs and files correctly.
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