show running-config
ALS2#show running-config
Building configuration...

Current configuration : 1767 bytes
!
version 12.2
no service timestamps log datetime msec
no service timestamps debug datetime msec
no service password-encryption
!
hostname ALS2
!
enable secret 5 $1$mERr$9cTjUIEqNGurQiFU.ZeCi1
!
!
!
!
!
!
spanning-tree mode pvst
spanning-tree extend system-id
!
interface Port-channel1
 switchport mode trunk
!
interface FastEthernet0/1
 shutdown
!
interface FastEthernet0/2
 shutdown
!
interface FastEthernet0/3
 shutdown
!
interface FastEthernet0/4
 shutdown
!
interface FastEthernet0/5
 shutdown
!
interface FastEthernet0/6
 switchport access vlan 234
 switchport mode access
 shutdown
!
interface FastEthernet0/7
 switchport trunk native vlan 800
 switchport mode trunk
 channel-group 1 mode active
!
interface FastEthernet0/8
 switchport trunk native vlan 800
 switchport mode trunk
 channel-group 1 mode active
!
interface FastEthernet0/9
 switchport trunk native vlan 800
 switchport mode trunk
!
interface FastEthernet0/10
switchport trunk native vlan 800
switchport mode trunk
!
interface FastEthernet0/11
shutdown
!
interface FastEthernet0/12
shutdown
!
interface FastEthernet0/13
shutdown
!
interface FastEthernet0/14
shutdown
!
interface FastEthernet0/15
switchport access vlan 1111
switchport mode access
shutdown
!
interface FastEthernet0/16
shutdown
!
interface FastEthernet0/17
shutdown
!
interface FastEthernet0/18
shutdown
!
interface FastEthernet0/19
shutdown
!
interface FastEthernet0/20
shutdown
!
interface FastEthernet0/21
shutdown
!
interface FastEthernet0/22
shutdown
!
interface FastEthernet0/23
shutdown
!
interface FastEthernet0/24
shutdown
!
interface GigabitEthernet0/1
!
interface GigabitEthernet0/2
!
interface Vlan1
no ip address
shutdown
!
!
!
!
line con 0
!
line vty 0 4
login
line vty 5 15
login
!
!
!
!
end
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Show VLAN Brief
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Show VTP Status
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Show etherchannel
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Show spanning-tree Summary
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Show standby brief
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ALS2gshow vlan brief
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ALS2$show vtp status
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ALs2#shov etherchannel
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