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	Device
	Interface
	IP Address
	Subnet Mask
	Default Gateway

	Router1
	NIC
	192.168.2.2
	255.255.255.0
	192.168.2.0

	Router0
	NIC
	192.168.2.1
	255.255.255.0
	192.168.2.0

	PC0
	NIC
	192.168.0.254
	255.255.255.0
	192.168.0.1

	Server0
	NIC
	192.168.1.254
	255.255.255.0
	192.168.1.1

	Printer0
	NIC
	192.168.1.253
	255.255.255.0
	192.168.1.1

	Laptop1
	NIC
	192.168.1.252
	255.255.255.0
	192.168.1.1


Logical Topology 
PC1: NIC: 192.168.0.254 – 255.255.255.0 – 192.168.0.1
Server0: NIC: 192.168.1.254 – 255.255.255.0 – 192.168.1.1
Printer0: NIC: 192.168.1.253 – 255.255.255.0 – 192.168.1.1
Laptop1: NIC: 192.168.1.252 – 255.255.255.0 – 192.168.1.1
Router0: NIC: 192.168.2.1 – 255.255.255.0 
Router0: 
Gig0/0/0 192.168.0.1 – 255.255.255.0
Gig0/0/0 192.168.1.1 – 255.255.255.0
Se0/2/0 192.168.2.1 – 255.255.255.0
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C:\>ping 192.168.0.254
Pinging 192.168.0.254 with 32 bytes of data:

Reply from 192.168.
Reply from 192.168.
Reply from 192.168.
Reply from 192.168.

Ping statistics for 192.168.0.254
Packets: Sent = 4, Received = 4, Lost = 0 (0% loss),
Approximate round trip times in milli-seconds
Minimum = 20ms, Maximun = 47ms, Average

26ms
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C:\>ping 192.168.2.0
Pinging 192.168.2.0 with 32 bytes of data:

TTI=255
TTL=255
TTL=255
TTL=255

Reply from 192.168.
Reply from 192.168.
Reply from 192.168.
Reply from 192.168.

Ping statistics for 192.168.2.0
Packets: Sent = 4, Received = 4, Lost = 0 (0% loss),
Approximate round trip times in milli-seconds:
Minimum = léms, Maximun = 2lms, Average = 18ms
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C:\>ping 192.168.1.1

Pinging 192.168.1.1 with 32 bytes of data:

Reply from 192.168.
Reply from 192.168.
Reply from 192.168.
Reply from 192.168.

bytes=32 time=22ms TTL=255
bytes=32 time=15ms TTL=255
bytes=32 time=21ms TTL=255
byte TTL=255

Ping statistics for 192.168.1.1
Packets: Sent = 4, Received = 4, Lost = 0 (0% loss),
Approximate round trip times in milli-seconds:
Minimum = 15ms, Maximun = 22ms, Average = loms
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image10.png
>ping 192.168.0.1

Pinging 192.168.0.1 with 32 bytes of dat

Reply from 192.168.0.1: bytes=32 time=24ms TTL=255
Reply from 192.168.0.1: bytes=32 time=léms TTL=255
Reply from 192.168.0.1: bytes=32 time=léms TTL=255
Reply from 192.168.0.1: bytes=32 time=loms TTL=255

Ping statistics for 192.168.0.1:
Packets: Sent = 4, Received = 4, Lost = 0 (0% loss),
Approximate round trip times in milli-seconds:
Minimm = l4ms, Maximum = 24ms, Average = loms
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C:\>ping 192.168.2.2
Pinging 192.168.2.2 with 32 bytes of data:

Reply from 192.168.2.2:
Reply from 192.168.2.2: TTL=25¢
Reply from 192.168.2.2 TTL=25¢
Reply from 192.168.2.2: bytes=32 time=3oms TTL=254

TTL=25¢

Ping statistics for 192.168.2.2
Packets: Sent = 4, Received = 4, Lost = 0 (0% loss),
Approximate round trip times in milli-seconds
Minimm = 24ms, Maximum = 3%ms, Average = 28ms
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C:\> ping 192.168.1.254
Pinging 192.168.1.254 with 32 bytes of data:

Reply from 192.168.
Reply from 192.168.
Reply from 192.168.
Reply from 192.168.

bytes=32 time=46ms TTL=128
TII=128
TII=128
TII=128

Ping statistics for 192.168.1.254:
Packets: Sent = 4, Received = 4, Lost = 0 (0% loss),
Approximate round trip times in milli-seconds
Minimm = 15ms, Maximum = 4éms, Average = 25ms
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C:\>ping 192.168.2.1

Pinging 192.168.2.1 with 32 bytes of data:

TTI=255
TTL=255
TTL=255
TTL=255

Reply from 192.168.2.1
Reply from 192.168.2.1:
Reply from 192.168.2.1
Reply from 192.168.2.1:

Ping statistics for 192.168.2.1
Packets: Sent = 4, Received = 4, Lost = 0 (0% loss),
Approximate round trip times in milli-seconds
Minimm = 13ms, Maximum = 24ms, Average = léms
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C:\>ping 192.168.1.253
Pinging 192.168.1.253 with 32 bytes of data:

Reply from 192.168.
Reply from 192.168.
Reply from 192.168.
Reply from 192.168.

bytes=32 time=léms TTL=128

Ping statistics for 192.168.1.253
Packets: Sent = 4, Received = 4, Lost = 0 (0% loss),
Approximate round trip times in milli-seconds
Minimm = 13ms, Maximum = 4lms, Average = 22ms
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Packet Tracer BC Command Line 1.0

ping 192.168.1.252
Pinging 192.168.1.252 with 32 bytes of data:

Reply from 192.168.1.252: bytes=32 time<lms TTL=128
Reply from 192.168.1.252: TII=128
Reply from 192.168.1.252 TII=128
Reply from 192.168.1.252: TII=128

Ping statistics for 192.168.1.252:
Packets: Sent = 4, Received = 4, Lost = 0 (0% loss),
Approximate round trip times in milli-seconds:
Minimum = Oms, Maximum = 3ms, Average = lms





