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Configuration for R0
Router>
Router>
Router>enable
Router#config t
Enter configuration commands, one per line. End with CNTL/Z.
Router(config)#hostname R0
R0(config)#interface g0/0/0
R0(config-if)#ip address 192.168.2.0 255.255.248.0
R0(config-if)#no shutdown

R0(config-if)#
%LINK-5-CHANGED: Interface GigabitEthernet0/0/0, changed state to up

%LINEPROTO-5-UPDOWN: Line protocol on Interface GigabitEthernet0/0/0, changed state to up
exit
R0(config)#interface g0/0/1
R0(config-if)#ip address 192.168.3.0 255.255.248.0
% 192.168.0.0 overlaps with GigabitEthernet0/0/0
R0(config-if)#ip address 192.169.2.0 255.255.248.0
R0(config-if)#no shutdown

R0(config-if)#
%LINK-5-CHANGED: Interface GigabitEthernet0/0/1, changed state to up
exit
R0(config)#
%LINEPROTO-5-UPDOWN: Line protocol on Interface GigabitEthernet0/0/1, changed state to up

R0#
%SYS-5-CONFIG_I: Configured from console by console

Configuration for R1
Router>
Router>enable
Router#config t
Enter configuration commands, one per line. End with CNTL/Z.
Router(config)#hostname R1
R1(config)#interface
% Incomplete command.
R1(config)#interface g0/0
%Invalid interface type and number
R1(config)#interface g0/0/0
R1(config-if)#ip address 172.16.1.0 255.255.255.0
Bad mask /24 for address 172.16.1.0
R1(config-if)#ip address 172.16.1.0 255.255.248.0
R1(config-if)#no shutdown

R1(config-if)#
%LINK-5-CHANGED: Interface GigabitEthernet0/0/0, changed state to up

%LINEPROTO-5-UPDOWN: Line protocol on Interface GigabitEthernet0/0/0, changed state to up
exit
R1(config)#interface gg0/0/1
^
% Invalid input detected at '^' marker.
R1(config)#interface g0/0/1
R1(config-if)#ip address 192.168.24.0 255.255.255.0
Bad mask /24 for address 192.168.24.0
R1(config-if)#ip address 192.168.24.0 255.255.248.0
Bad mask /21 for address 192.168.24.0
R1(config-if)#exit
R1(config)#exit
R1#
%SYS-5-CONFIG_I: Configured from console by console

R1#
R1#
R1#
R1#exit
R1>enable
R1#config t
Enter configuration commands, one per line. End with CNTL/Z.
R1(config)#hostname R1
R1(config)#interface g0/0/0
R1(config-if)#ip address 172.16.1.0 255.255.248.0
R1(config-if)#no shutdown
R1(config-if)#exit
R1(config)#interface g0/0/1
R1(config-if)#ip address 192.168.1.0 255.255.248.0
R1(config-if)#no shutdown

R1(config-if)#
%LINK-5-CHANGED: Interface GigabitEthernet0/0/1, changed state to up
exit
R1(config)#exit
R1#
%SYS-5-CONFIG_I: Configured from console by console

R1#
%LINEPROTO-5-UPDOWN: Line protocol on Interface GigabitEthernet0/0/1, changed state to up

Configuration for R2
Router>
Router>
Router>enable
Router#config t
Enter configuration commands, one per line. End with CNTL/Z.
Router(config)#hostname R2
R2(config)#interface g0/0/1
R2(config-if)#ip address 192.169.1.0 255.255.248.0
R2(config-if)#no shutdown

R2(config-if)#
%LINK-5-CHANGED: Interface GigabitEthernet0/0/1, changed state to up

%LINEPROTO-5-UPDOWN: Line protocol on Interface GigabitEthernet0/0/1, changed state to up
exit
R2(config)#interface g0/0/0
R2(config-if)#ip address 10.10.1.0 255.255.248.0
R2(config-if)#no shutdown

R2(config-if)#
%LINK-5-CHANGED: Interface GigabitEthernet0/0/0, changed state to up

%LINEPROTO-5-UPDOWN: Line protocol on Interface GigabitEthernet0/0/0, changed state to up
exit
R2(config)#
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