
[image: A screenshot of a computer

Description automatically generated][image: A computer screen shot of a computer screen

Description automatically generated]
[image: A screenshot of a computer

Description automatically generated]

Tue Nov 14 12:16:01 2023   RA   Router>enable
Tue Nov 14 12:16:01 2023   RA   Router#configure terminal
Tue Nov 14 12:16:01 2023   RA   Router(config)#interface GigabitEthernet0/0
Tue Nov 14 12:16:05 2023   RA   Router(config-if)#no shutdown
Tue Nov 14 12:16:42 2023   RA   Router(config-if)#ip address 192.168.1.1 255.255.255.0
Tue Nov 14 12:16:45 2023   RA   Router(config-if)#ip address 192.168.1.1 255.255.255.0
Tue Nov 14 12:17:11 2023   RB   Router>enable
Tue Nov 14 12:17:11 2023   RB   Router#configure terminal
Tue Nov 14 12:17:11 2023   RB   Router(config)#interface GigabitEthernet0/0
Tue Nov 14 12:17:13 2023   RB   Router(config-if)#no shutdown
Tue Nov 14 12:17:19 2023   RB   Router(config-if)#exit
Tue Nov 14 12:17:19 2023   RB   Router(config)#interface GigabitEthernet0/1
Tue Nov 14 12:17:35 2023   RB   Router(config-if)#ip address 192.168.2.1 255.255.255.0
Tue Nov 14 12:17:39 2023   RB   Router(config-if)#ip address 192.168.2.1 255.255.255.0
Tue Nov 14 12:18:14 2023   RB   Router(config-if)#exit
Tue Nov 14 12:18:14 2023   RB   Router(config)#interface GigabitEthernet0/1
Tue Nov 14 12:18:23 2023   RB   Router(config-if)#ip address  
Tue Nov 14 12:18:35 2023   RB   Router(config-if)#ip address  
Tue Nov 14 12:18:35 2023   RB   Router(config-if)#no shutdown
Tue Nov 14 12:18:59 2023   RB   Router(config-if)#ip address 10.0.12.2 255.0.0.0
Tue Nov 14 12:19:06 2023   RB   Router(config-if)#ip address 10.0.12.2 255.0.0.0
Tue Nov 14 12:19:23 2023   RC   Router>enable
Tue Nov 14 12:19:23 2023   RC   Router#configure terminal
Tue Nov 14 12:19:23 2023   RC   Router(config)#interface GigabitEthernet0/0
Tue Nov 14 12:19:34 2023   RA   Router(config-if)#exit
Tue Nov 14 12:19:34 2023   RA   Router(config)#interface GigabitEthernet0/0
Tue Nov 14 12:19:36 2023   RA   Router(config-if)#exit
Tue Nov 14 12:19:36 2023   RA   Router(config)#interface GigabitEthernet0/1
Tue Nov 14 12:19:48 2023   RA   Router(config-if)#ip address 192.168.2.1 255.255.255.0
Tue Nov 14 12:19:51 2023   RA   Router(config-if)#ip address 192.168.2.1 255.255.255.0
Tue Nov 14 12:20:04 2023   RA   Router(config-if)#end
Tue Nov 14 12:20:04 2023   RA   Router#vlan database
Tue Nov 14 12:20:12 2023   RA   Router(vlan)#exit
Tue Nov 14 12:20:12 2023   RA   Router#configure terminal
Tue Nov 14 12:21:52 2023   SA   Switch>enable
Tue Nov 14 12:21:52 2023   SA   Switch#configure terminal
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