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 Figure 1: Client1 Virtual Machine – Windows Login Screen                                                                 
 Figure 2: Successful Ping Test Between Server1 and Client1 Virtual Machines
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Figure 3 X: Joining Client Machine to Domain via Server Manager
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Figure 4: Creating a New Computer Object in Active Directory Users and Computers
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Figure 5: Creating a New User Account in Active Directory Domain
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[image: ]Figure 6: Successful Ping Test Between Debian Client and Debian Server


Figure 7: Routing and Remote Access Service (RRAS) Configuration on London Server
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Figure 8: Server1 Local Server Properties in Server Manager
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Figure 9: Static IPv4 and DNS Configuration on Client1
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[image: ]Figure 10: Active Directory Users and Computers – New Object Creation Menu 
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