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[bookmark: _Hlk54105057]Project: Bridge Construction
Site address:
Central Ave, 
Neath,
Port Talbot
SA12 7AX
Date of works: 6th May 2021 - 4th Nov 2021
[bookmark: h.1kmozguib79q]Description of activity
· Working under high voltage overhead cables.

Involves:
· Use of plant and machinery under high voltage cables.
· Operatives working close to live unprotected power lines.
· Managers and supervisors being competent with safe distances.
· Site specific induction and onsite training.
· Site specific PPE issued by Principle Contractor.
.
[bookmark: h.ygmyk6vg3h9j]Supervision and personnel
· Site Manager - TBC
· Evan Pritchard Supervisor – TBC
· Health and Safety advisor - TBC
[bookmark: h.ocmnip9mxfv8]Training
· All operatives are adequately trained to carry out required tasks.
· All site operatives must hold the relevant CSCS certification.
· Additional health and safety training given if required.  
[bookmark: h.r46xzs9m3ioz]Legislation
· Health and Safety Work Act 1974
· The Management of Health and Safety at Work Regulations 2006
· Workplace (Health, Safety and Welfare) Regulations 1992
· The Personal Protective Equipment at Work Regulations 2002
· The Construction (Design and Management) Regulations 2015
· Avoiding danger from overhead power lines GS6 (Fourth edition)
· Electricity at Work Regulations 1989

[bookmark: h.2cpfsm4rqcx7]While working
Before any work commences, the site manager must be aware of the heights of all plant and machinery operating on the site. 
The height is to be measured by a competent person using a non-contact measuring device.
It is the responsibility of the Principle Contractor to find out the safe distances to these specific overhead power lines, this must happen before the site opens.
If any tall plant is required on site, the site manager is to ensure the site is safe. 
If equipment or machinery capable of breaching the safety clearance distance must pass underneath the overhead line, a passageway through will be clearly marked out.
Site operatives, including any contractors, understand the risks and are provided with instructions about the risk prevention measures.
Work is not to be conducted in poor lighting conditions or extreme bad weather, the lines must be clearly visible at all times.
[bookmark: h.ddte95cmjn8g]PPE requirements
· Hard hats
· Safety boots
· Hi-vis vest
· Safety gloves
· Safety glasses
[bookmark: h.jjom1h6ke549]Welfare
Welfare arrangements are supplied by the principal contractor.
These should be in line with Schedule 2 of the Construction Design & Management Regulations 2015 (CDM). All sites are to have a minimum amount of welfare facilities available for workers, which include the following:

· Toilets
· Washing facilities
· Drinking water
· Changing rooms and lockers
· Heating
· Rest facilities
[bookmark: h.zai7l19dxpwv]First aid
· Refer to the onsite safety notice board for all first aid information. 

· The first aid box Is adequate to the size of the site and will be checked regularly to ensure it is in the correct state.

· The principal contractor should nominate an appointed person to take care of first-aid arrangements. 

· The number of appointed first aiders shall be dependent on the number of employees but Is yet TBC.
[bookmark: h.ye0kne5onkgh]Emergency procedures
· The principal contractor will ensure that the existing site emergency procedures are followed and that relevant information is given to operatives during the site induction given by the assistant manager or when changes are made to procedures.

· The closest hospital is: Morriston Hospital, Heol Maes Eglwys, Cwmrhydyceirw, Morriston SA6 6NL
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