Celdwan Bandeira, ID 1812407



Packet Tracer PC Command Line 1.0
C:\>ping 185.95.2.3

Pinging 185.95.2.3 with 32 bytes of data:

Reply from 185.95.1.1: Destination host unreachable.
Reply from 185.95.1.1: Destination host unreachable.
Reply from 185.95.1.1: Destination host unreachable.
Reply from 185.95.1.1: Destination host unreachable.

Ping statistics for 185.95.2.3:
Packets: Sent = 4, Received = 0, Lost = 4 (100% loss),


Packet Tracer PC Command Line 1.0
C:\>ping 185.95.3.3

Pinging 185.95.3.3 with 32 bytes of data:

Reply from 185.95.2.1: Destination host unreachable.
Request timed out.
Reply from 185.95.2.1: Destination host unreachable.
Reply from 185.95.2.1: Destination host unreachable.

Ping statistics for 185.95.3.3:
Packets: Sent = 4, Received = 0, Lost = 4 (100% loss),


R1
!
!
!
license udi pid CISCO2911/K9 sn FTX1524D9TO-
!
!
!
!
!
!
!
!
!
!
!
spanning-tree mode pvst
!
!
!
!
!
!
interface GigabitEthernet0/0
ip address 185.95.1.1 255.255.255.0
duplex auto
speed auto
!
interface GigabitEthernet0/1
no ip address
duplex auto
speed auto
shutdown
!
interface GigabitEthernet0/2
no ip address
duplex auto
speed auto
shutdown
!
interface Serial0/0/0
ip address 185.95.12.1 255.255.255.252
!
interface Serial0/0/1
ip address 185.95.13.1 255.255.255.252
clock rate 2000000
!
interface Vlan1
no ip address
shutdown
!
router ospf 10
router-id 1.1.1.1
log-adjacency-changes
network 185.95.1.0 0.0.0.0 area 0
network 185.95.12.0 0.0.0.0 area 0
network 185.95.13.0 0.0.0.0 area 0
!
ip classless
!
ip flow-export version 9
!
!
!
banner motd ^CDanger^C
!
!
!
!
!
line con 0
!
line aux 0
!
line vty 0 4
login
!
!
!
end


R1#show running config
^
% Invalid input detected at '^' marker.
R1#show running-conf
Building configuration...

Current configuration : 1037 bytes
!
version 15.1
no service timestamps log datetime msec
no service timestamps debug datetime msec
no service password-encryption
!
hostname R1
!
!
!
!
!
!
!
!
no ip cef
no ipv6 cef
!
!
!
!
license udi pid CISCO2911/K9 sn FTX1524D9TO-
!
!
!
!
!
!
!
!
!
!
!
spanning-tree mode pvst
!
!
!
!
!
!
interface GigabitEthernet0/0
ip address 185.95.1.1 255.255.255.0
duplex auto
speed auto
!
interface GigabitEthernet0/1
no ip address
duplex auto
speed auto
shutdown
!
interface GigabitEthernet0/2
no ip address
duplex auto
speed auto
shutdown
!
interface Serial0/0/0
ip address 185.95.12.1 255.255.255.252
!
interface Serial0/0/1
ip address 185.95.13.1 255.255.255.252
clock rate 2000000
!
interface Vlan1
no ip address
shutdown
!
router ospf 10
router-id 1.1.1.1
log-adjacency-changes
network 185.95.1.0 0.0.0.0 area 0
network 185.95.12.0 0.0.0.0 area 0
network 185.95.13.0 0.0.0.0 area 0
!
ip classless
!
ip flow-export version 9
!
!
!
banner motd ^CDanger^C
!
!
!
!
!
line con 0
!
line aux 0
!
line vty 0 4
login
!
R1#show ip int brief
Interface IP-Address OK? Method Status Protocol 
GigabitEthernet0/0 185.95.1.1 YES manual up up 
GigabitEthernet0/1 unassigned YES unset administratively down down 
GigabitEthernet0/2 unassigned YES unset administratively down down 
Serial0/0/0 185.95.12.1 YES manual up up 
Serial0/0/1 185.95.13.1 YES manual up up 
Vlan1 unassigned YES unset administratively down down


R1#show ip route
Codes: L - local, C - connected, S - static, R - RIP, M - mobile, B - BGP
D - EIGRP, EX - EIGRP external, O - OSPF, IA - OSPF inter area
N1 - OSPF NSSA external type 1, N2 - OSPF NSSA external type 2
E1 - OSPF external type 1, E2 - OSPF external type 2, E - EGP
i - IS-IS, L1 - IS-IS level-1, L2 - IS-IS level-2, ia - IS-IS inter area
* - candidate default, U - per-user static route, o - ODR
P - periodic downloaded static route

Gateway of last resort is not set

185.95.0.0/16 is variably subnetted, 6 subnets, 3 masks
C 185.95.1.0/24 is directly connected, GigabitEthernet0/0
L 185.95.1.1/32 is directly connected, GigabitEthernet0/0
C 185.95.12.0/30 is directly connected, Serial0/0/0
L 185.95.12.1/32 is directly connected, Serial0/0/0
C 185.95.13.0/30 is directly connected, Serial0/0/1
L 185.95.13.1/32 is directly connected, Serial0/0/1

R1#show ip route
Codes: L - local, C - connected, S - static, R - RIP, M - mobile, B - BGP
D - EIGRP, EX - EIGRP external, O - OSPF, IA - OSPF inter area
N1 - OSPF NSSA external type 1, N2 - OSPF NSSA external type 2
E1 - OSPF external type 1, E2 - OSPF external type 2, E - EGP
i - IS-IS, L1 - IS-IS level-1, L2 - IS-IS level-2, ia - IS-IS inter area
* - candidate default, U - per-user static route, o - ODR
P - periodic downloaded static route

Gateway of last resort is not set

185.95.0.0/16 is variably subnetted, 6 subnets, 3 masks
C 185.95.1.0/24 is directly connected, GigabitEthernet0/0
L 185.95.1.1/32 is directly connected, GigabitEthernet0/0
C 185.95.12.0/30 is directly connected, Serial0/0/0
L 185.95.12.1/32 is directly connected, Serial0/0/0
C 185.95.13.0/30 is directly connected, Serial0/0/1
L 185.95.13.1/32 is directly connected, Serial0/0/1


R2#show ip ospf 
Routing Process "ospf 10" with ID 2.2.2.2
Supports only single TOS(TOS0) routes
Supports opaque LSA
SPF schedule delay 5 secs, Hold time between two SPFs 10 secs
Minimum LSA interval 5 secs. Minimum LSA arrival 1 secs
Number of external LSA 0. Checksum Sum 0x000000
Number of opaque AS LSA 0. Checksum Sum 0x000000
Number of DCbitless external and opaque AS LSA 0
Number of DoNotAge external and opaque AS LSA 0
Number of areas in this router is 1. 1 normal 0 stub 0 nssa
External flood list length 0
Area BACKBONE(0) (Inactive)
Number of interfaces in this area is 0
Area has no authentication
SPF algorithm executed 1 times
Area ranges are
Number of LSA 1. Checksum Sum 0x000550
Number of opaque link LSA 0. Checksum Sum 0x000000
Number of DCbitless LSA 0
Number of indication LSA 0
Number of DoNotAge LSA 0
Flood list length 0

Routing Process "ospf 109" with ID 185.95.23.1
Supports only single TOS(TOS0) routes
Supports opaque LSA
SPF schedule delay 5 secs, Hold time between two SPFs 10 secs
Minimum LSA interval 5 secs. Minimum LSA arrival 1 secs
Number of external LSA 0. Checksum Sum 0x000000
Number of opaque AS LSA 0. Checksum Sum 0x000000
Number of DCbitless external and opaque AS LSA 0
Number of DoNotAge external and opaque AS LSA 0
Number of areas in this router is 0. 0 normal 0 stub 0 nssa
External flood list length 0


R2#show ip int brief
Interface IP-Address OK? Method Status Protocol 
GigabitEthernet0/0 185.95.2.1 YES manual up up 
GigabitEthernet0/1 unassigned YES unset administratively down down 
GigabitEthernet0/2 unassigned YES unset administratively down down 
Serial0/0/0 185.95.12.2 YES manual up up 
Serial0/0/1 185.95.23.1 YES manual up up 
Vlan1 unassigned YES unset administratively down down


R2#show ip route
Codes: L - local, C - connected, S - static, R - RIP, M - mobile, B - BGP
D - EIGRP, EX - EIGRP external, O - OSPF, IA - OSPF inter area
N1 - OSPF NSSA external type 1, N2 - OSPF NSSA external type 2
E1 - OSPF external type 1, E2 - OSPF external type 2, E - EGP
i - IS-IS, L1 - IS-IS level-1, L2 - IS-IS level-2, ia - IS-IS inter area
* - candidate default, U - per-user static route, o - ODR
P - periodic downloaded static route

Gateway of last resort is not set

185.95.0.0/16 is variably subnetted, 6 subnets, 3 masks
C 185.95.2.0/24 is directly connected, GigabitEthernet0/0
L 185.95.2.1/32 is directly connected, GigabitEthernet0/0
C 185.95.12.0/30 is directly connected, Serial0/0/0
L 185.95.12.2/32 is directly connected, Serial0/0/0
C 185.95.23.0/30 is directly connected, Serial0/0/1
L 185.95.23.1/32 is directly connected, Serial0/0/1


R3

R3#show run
Building configuration...

Current configuration : 1037 bytes
!
version 15.1
no service timestamps log datetime msec
no service timestamps debug datetime msec
no service password-encryption
!
hostname R3
!
!
!
!
!
!
!
!
no ip cef
no ipv6 cef
!
!
!
!
license udi pid CISCO2911/K9 sn FTX1524XQ96-
!
!
!
!
!
!
!
!
!
!
!
spanning-tree mode pvst
!
!
!
!
!
!
interface GigabitEthernet0/0
ip address 185.95.3.1 255.255.255.0
duplex auto
speed auto
!
interface GigabitEthernet0/1
no ip address
duplex auto
speed auto
shutdown
!
interface GigabitEthernet0/2
no ip address
duplex auto
speed auto
shutdown
!
interface Serial0/0/0
ip address 185.95.13.2 255.255.255.252
!
interface Serial0/0/1
ip address 185.95.23.2 255.255.255.252
clock rate 2000000
!
interface Vlan1
no ip address
shutdown
!
router ospf 10
router-id 3.3.3.3
log-adjacency-changes
network 185.95.3.0 0.0.0.0 area 0
network 185.95.13.0 0.0.0.0 area 0
network 185.95.23.2 0.0.0.0 area 0
!
ip classless
!
ip flow-export version 9
!
!
!
banner motd ^CDanger^C
!
!
!
!
!
line con 0
!
line aux 0
!
line vty 0 4
login
!
!
!
End


R3#show ip int brief
Interface IP-Address OK? Method Status Protocol 
GigabitEthernet0/0 185.95.3.1 YES manual up up 
GigabitEthernet0/1 unassigned YES unset administratively down down 
GigabitEthernet0/2 unassigned YES unset administratively down down 
Serial0/0/0 185.95.13.2 YES manual up up 
Serial0/0/1 185.95.23.2 YES manual up up 
Vlan1 unassigned YES unset administratively down down

R3#show ip route
Codes: L - local, C - connected, S - static, R - RIP, M - mobile, B - BGP
D - EIGRP, EX - EIGRP external, O - OSPF, IA - OSPF inter area
N1 - OSPF NSSA external type 1, N2 - OSPF NSSA external type 2
E1 - OSPF external type 1, E2 - OSPF external type 2, E - EGP
i - IS-IS, L1 - IS-IS level-1, L2 - IS-IS level-2, ia - IS-IS inter area
* - candidate default, U - per-user static route, o - ODR
P - periodic downloaded static route

Gateway of last resort is not set

185.95.0.0/16 is variably subnetted, 6 subnets, 3 masks
C 185.95.3.0/24 is directly connected, GigabitEthernet0/0
L 185.95.3.1/32 is directly connected, GigabitEthernet0/0
C 185.95.13.0/30 is directly connected, Serial0/0/0
L 185.95.13.2/32 is directly connected, Serial0/0/0
C 185.95.23.0/30 is directly connected, Serial0/0/1
L 185.95.23.2/32 is directly connected, Serial0/0/1
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