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Foundation Piling Limited	Risk Assessment Piling Works
Job Name : Techniquest, Cardiff	Date : 22/05/2019
Client: G Oakley & Sons LtdRef No. : 0060.19
Prep. By : GCP



	ACTIVITY
	RISKS
	Degree of Risk
	CONTROL PROCEDURES
	Residual Risk

	
	
	L
	S
	R
	
	L
	S
	R

	Site Access / Egress
	Collision with Vehicles /
	3
	4
	12
	Principle Contractor to erect suitable
	1
	2
	3

	
	Persons
	
	
	
	barriers to reduce the interaction between plant / vehicles and any site operatives / general public. Operatives to supervise and direct plant and vehicles across public footpaths and access routes.
	
	
	

	Storage & Security
	Falling / Collapsing 
	3
	3
	9
	Operatives to stack piling equipment
	2
	1
	2

	
	Materials
	
	
	
	& materials in such a way as not to become unstable when moved / used.
	
	
	

	
	Unauthorised Access
	3
	3
	9
	Principal Contractor to provide site security as required; erect and maintain.
	2
	1
	2

	
	Loss / Theft
	4
	2
	8
	Boundary fencing to prevent unauthorised access at all times.
	1
	1
	1

	Site Electrics
	Electrocution
	3
	4
	12
	All electrical equipment to be a maximum of 110v DC. All portable electrical equipment to be checked before it is used and thoroughly inspected every day by a competent person.
Damaged / faulty equipment to be marked up as "DO NOT USE" and returned to plant department for repair.
	1
	2
	2

	
	Fire
	3
	4
	12
	Suitable fire extinguishers are to be available for dealing with electrical fires.
	1
	2
	2

	
	Tripping Hazards (cables)
	2
	4
	8
	Operatives to plan the route of cables so as not to present a tripping hazard to any other site personnel.
	1
	2
	2

	Lifting Operations
	Falling Plant and 
	4
	4
	16
	Only Banksman / Slingers are to 
	1
	1
	1

	
	Materials
	
	
	
	control lifting operations on site and ensure that the loads are properly slung prior to lift commencing.
	
	
	

	
	Collisions with Plant,
	3
	4
	12
	Banksman to also ensure that the lift
	1
	1
	1

	
	Persons and Overhead
	
	
	
	path / route is clear of other site
	
	
	

	
	Services
	
	
	
	operatives and overhead services, in particular HV cables and overhead pipe racks.
	
	
	

	
	Failure of Appliance
	3
	4
	12
	Foreman to ensure that all lifting equipment is inspected weekly and that the "Record of Inspection" has been completed.
	1
	2
	1

	ACTIVITY
	RISKS
	Degree of Risk
	CONTROL PROCEDURES
	Residual Risk

	
	
	L
	S
	R
	
	L
	S
	R

	Lifting Operations (cont.)
	
	
	
	
	Foreman is to also ensure that all lifting equipment has been given a thorough test / examination every six months.
Banksman / Slinger to assess all loads before they are lifted to ensure that the Safe Working Load of the lifting equipment is not exceeded at any point during the lift.
	
	
	

	Plant & Machinery
	Collisions with Plant &
	4
	4
	16
	Principal Contractor to erect suitable
	2
	1
	2

	
	Persons
	
	
	
	signage and barriers to prevent any unauthorised site operatives gaining access to the piling area.
All piling operations to cease if any unauthorised persons enter the piling area.
	
	
	

	
	Contact with Moving 
	2
	4
	8
	Foreman to check machinery / plant
	1
	1
	1

	
	Parts
	
	
	
	to ensure that guards are secured in place to prevent any physical contact with moving parts / machinery.
	
	
	

	
	Over-turning
	4
	4
	16
	Principal Contractor to design, install and maintain piling platforms to safely support the weight of the piling rig in its working mode.
In order to comply with the latest HSE
Legislation:- the Working Platform
Certificate is to be signed by the 
Principal Contractor and / or Planning Supervisor and returned prior to commencing any piling operations. All excavations to remove existing foundations / underground 
obstructions should be backfilled with suitable materials in 300mm layers and compacted with suitable compaction equipment.
	1
	4
	4

	Manual Handling
	Musculoskeletal Injuries
	5
	3
	15
	Manual Handling to be reduced to a minimum by using mechanical method (crane / HIAB). Should the above not be possible:- heavy loads to be split into smaller items of not more than 25kg each.
If this is still not possible:- the loads are to be lifted by multiple operatives, ensuring that the weight does not exceed 25kg per person.
	2
	1
	2


Degree of Risk = Likelihood          5 = Almost Certain,   4 = Very Likely,   3 = Likely,   2 = Unlikely,   1 = Very Unlikely
Severity          5 = Fatality,   4 = Specified Injury,   3 = 7 Day Injury,   2 = Minor Injury,   1 = No Injury Risk = Likelihood x Severity
Residual Risk not to be greater than 4

	ACTIVITY
	RISKS
	Degree of Risk
	CONTROL PROCEDURES
	Residual Risk

	
	
	L
	S
	R
	
	L
	S
	R

	Manual Handling (cont.)
	Falling / Tripping
	3
	3
	9
	Operatives to "walk the route" before they carry any loads to ensure that there are no obstacles that could impede the manual handling operation.
	1
	1
	1

	
	Trapping Toes / Fingers
	4
	2
	8
	Operatives to wear protective equipment provided; this includes steel toed boots / wellies and rigger type gloves.
When lowering the loads, care should be taken to ensure that fingers / toes are not trapped.
	1
	1
	1

	Existing Services
	Contact with Services
	4
	4
	16
	Principal Contractor to scan for, locate, expose, divert, protect as necessary all existing underground services prior to the start of any piling operations.
	1
	4
	4

	
	Damage to Services
	
	
	
	Principal Contractor to be notified of any pressure loss / anomalies whilst drilling / injecting piles.
	
	
	

	
	Electrocution
	
	
	
	All work to cease if cable strike occurs. Rig operator to stay in cab or jump well clear, not step down.
Call emergency services in fire seen.
	
	
	

	Smoking
	Fire & / OR Explosion
	4
	4
	16
	SMOKING to be confined to designated smoking areas only.
	2
	2
	4

	
	Fire
	
	
	
	All cigarettes / cigars / pipes to be properly extinguished and disposed.
	
	
	

	
	Explosion
	
	
	
	NO SMOKING near flammable liquids/ gases or by any other sources of fuel
e.g. paper / wood / cloth / plastics, etc.
	
	
	

	Working Above / 
	Drowning
	2
	4
	8
	Principal Contractor to install & 
	1
	1
	1

	Adjacent to Water
	
	
	
	
	maintain fencing and / or guard rails to prevent operatives from falling into adjacent bodies of water.
Principal Contractor to install & and maintain bunding to prevent spoil, slurry or concrete from running downhill into bodies of water / watercourses.
	
	
	

	Substances Hazardous
	Respiratory Distress
	4
	3
	12
	Principal Contractor to control dust
	2
	1
	2

	to Health
	Inhalation
	
	
	
	levels on the site by damping down the haul roads / piling platforms and reducing site traffic speeds.
	
	
	

	
	Skin Irritation
	4
	2
	12
	Wet concrete can cause cement burns to the skin
Should any operative come into 
	2
	1
	2

	ACTIVITY
	RISKS
	Degree of Risk
	CONTROL PROCEDURES
	Residual Risk

	
	
	L
	S
	R
	
	L
	S
	R

	Substances Hazardous
	
	
	
	
	contact with wet concrete, they should
	
	
	

	to Health (cont.)
	
	
	
	
	thoroughly wash the affected area to remove any traces. Any clothing made wet by concrete should be removed as soon as possible and the affected areas of the skin thoroughly washed / dried.
The clothing is to be washed before re-use or properly disposed of.
	
	
	

	
	Eye Injury
	3
	3
	9
	Should there be any eye contact with dust / concrete, the affected eye should be thoroughly irrigated with cold, clean water or a propriety eyewash solution.
	2
	1
	2

	Noise
	Industrial Deafness
	5
	3
	15
	Noise assessments have been carried out on piling rigs and equipment. Operatives are provided with hearing protection and instructed when / where it is to be used.
	2
	1
	2

	
	Noise Pollution
	5
	1
	5
	Piling rig / equipment is to be kept in good working order, however should exhaust silencers fail, these are to be replaced / repaired without delay.
	2
	1
	2

	
	Tinnitus
	
	
	
	Working hours for each individual site are to be adhered to without exception.
	
	
	

	
	Temporary Hearing Loss
	5
	2
	10
	Should operatives experience temporary hearing loss they should
stop work and report it to their foreman / manager immediately. When operative returns to work they should be provided with and instructed to wear ear protection at all times throughout the working day.
Remember:- if an operative continues to work at higher noise levels, they 
will suffer from PERMANENT NONREVERSIBLE HEARING LOSS.
	
	
	

	Members of the Public,
	Falling Materials
	4
	4
	16
	To prevent members of the public /
	2
	1
	2

	Visitors & Others
	
	
	
	
	site operatives being hit by falling materials:- operatives are to ensure that there is no spoil / concrete / debris flighted up the auger. Principal Contractor to erect and maintain polythene sheeting / debris netting to perimeter walls / fencing to prevent mud / concrete / slurry splashing members of the public.
	
	
	


Degree of Risk = Likelihood          5 = Almost Certain,   4 = Very Likely,   3 = Likely,   2 = Unlikely,   1 = Very Unlikely
Severity          5 = Fatality,   4 = Specified Injury,   3 = 7 Day Injury,   2 = Minor Injury,   1 = No Injury Risk = Likelihood x Severity
Residual Risk not to be greater than 4

	ACTIVITY
	RISKS
	Degree of Risk
	CONTROL PROCEDURES
	Residual Risk

	
	
	L
	S
	R
	
	L
	S
	R

	Members of the Public,
	Collision
	2
	4
	8
	Principal Contractor to provide and 
	2
	1
	2

	Visitors & Others (cont.)
	
	
	
	
	erect suitable signage to warn members of the public about the risk of vehicles entering and exiting site. All reversing vehicles are to be seen back by trained Banksman / Slingers to ensure that there are no crush hazards / zones.
	
	
	

	
	Tripping
	4
	4
	16
	Operatives are to ensure that our water and concrete hoses do not cross pedestrian access routes. Should this not be possible, the hoses are to be buried or the Principal Contractor is to build a suitable pedestrian crossover point. Should this not be possible, then the Principal Contractor is to provide a fulltime watchperson to escort pedestrians across the hoses or across the road to the other footpath.
	2
	1
	2

	Contaminated Ground
	Damage to Health 
	4
	4
	16
	Principal Contractor to provide a
	2
	1
	2

	
	through Ingestion / Skin
	
	
	
	complete report of all known
	
	
	

	
	Contact
	
	
	
	contaminates, including the analysis of chemical concentrations. Operatives to wear PPE provided and adopt a high standard of Health & Hygiene. Principal Contractor to prevent all arisings flowing into watercourses and remove contaminated material from site.
	
	
	

	Waste Management
	Environmental Damage
	4
	4
	16
	Foreman to ensure that all general rubbish is placed in the skips provided by the Principal Contractor.
	1
	1
	1

	
	Damage to Health 
	
	
	
	Principal Contractor to set up
	
	
	

	
	through Contact
	
	
	
	supervise and control all site waste management including movement on site and disposal to tips off site.
	
	
	

	
	Damage to the 
	4
	2
	8
	Principal Contractor to plan for,
	1
	1
	1

	
	Environment
	
	
	
	supervise and control measures to safeguard the environment.
	
	
	

	Emergency Procedures
	Burns
	4
	4
	16
	Foreman to notify site manager and
	2
	2
	4

	for Fire
	
	
	
	
	contact emergency services if smoke or fire is seen anywhere on site.
	
	
	

	
	Smoke Inhalation
	4
	2
	8
	Foreman to direct site operatives to the site rendezvous point as directed in Site Induction. Appointed Persons to attend to injured persons should this be required.
	2
	1
	2

	ACTIVITY
	RISKS
	Degree of Risk
	CONTROL PROCEDURES
	Residual Risk

	
	
	L
	S
	R
	
	L
	S
	R

	Fuel Storage
	Leakage / Pollution /
	5
	2
	10
	All gas oil to be stored in bunded
	1
	1
	1

	
	Contamination
	
	
	
	containers. All surface spillages / leakages are to be cleaned up and disposed of properly - not just left on site.
	
	
	

	
	Fire & / OR Explosion
	3
	3
	9
	NO SMOKING when working with or near any flammable liquids / gases.
	
	
	

	Vibrating Equipment
	Arm / Hand / Finger
	4
	3
	12
	Operatives use light pneumatic picks
	2
	1
	2

	
	Damage
	
	
	
	to remove the build up of concrete grout on our equipment. Operatives involved in this activity should limit themselves to 30 minutes work and a 30 minute break. Two operatives can job share to reduce their exposure to hand / arm vibration.
	
	
	

	Levels of Illumination
	Trips and Falls
	4
	3
	12
	Task lighting provided to allow our operatives to safely walk about the piling area and carry out their required tasks.
	1
	2
	2

	
	Collision with Plant /
	3
	4
	12
	Principal Contractor to provide, erect
	1
	2
	2

	
	Materials and People
	
	
	
	and maintain access lighting to allow plant / vehicles to access the site and our operatives to access the welfare facilities.
	
	
	

	Working at Height
	Falling
	2
	4
	8
	Operatives to wear full harness when working at height. Harness to be connected to the inertia fall-arrest device on the piling rig. Working platform on the agitator has a hand rail.
	2
	2
	4

	
	Falling Objects / Tools / 
	2
	3
	6
	Operatives on the ground are to be
	2
	1
	2

	
	Materials
	
	
	
	made aware of operatives working at height - Banksman to manage the area. Tools / equipment used at height to be carried in a tool belt.
	
	
	

	
	Unauthorised Access
	3
	4
	12
	Principal Contractor to provide site
	2
	1
	2

	
	(General Public)
	
	
	
	security as required and erect &
	
	
	

	
	(Children)
	
	
	
	maintain boundary fencing at all times.
	
	
	

	Working from MEWP
	Falling
	2
	4
	8
	Operatives to wear full harness when working at height or in a MEWP. Harness to be connected by restraint lanyard to designated anchor point.
	2
	2
	4

	
	Overturning
	3
	4
	12
	The MEWP will only be used on the designed piling platform. The MEWP will only be operated by FP operatives holding the relevant qualification.
	1
	4
	4


Degree of Risk = Likelihood          5 = Almost Certain,   4 = Very Likely,   3 = Likely,   2 = Unlikely,   1 = Very Unlikely
Severity          5 = Fatality,   4 = Specified Injury,   3 = 7 Day Injury,   2 = Minor Injury,   1 = No Injury Risk = Likelihood x Severity
Residual Risk not to be greater than 4
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Degree of Risk = Likelihood          5 = Almost Certain,   4 = Very Likely,   3 = Likely,   2 = Unlikely,   1 = Very Unlikely
Severity          5 = Fatality,   4 = Specified Injury,   3 = 7 Day Injury,   2 = Minor Injury,   1 = No Injury Risk = Likelihood x Severity
Residual Risk not to be greater than 4
Degree of Risk = Likelihood          5 = Almost Certain,   4 = Very Likely,   3 = Likely,   2 = Unlikely,   1 = Very Unlikely
Severity          5 = Fatality,   4 = Specified Injury,   3 = 7 Day Injury,   2 = Minor Injury,   1 = No Injury Risk = Likelihood x Severity
Residual Risk not to be greater than 4
	ACTIVITY
	RISKS
	Degree of Risk
	CONTROL PROCEDURES
	Residual Risk

	
	
	L
	S
	R
	
	L
	S
	R

	Working from MEWP
	Upper Control Failure /
	3
	3
	9
	A competent person will be at the base
	3
	1
	3

	(cont.)
	Immobilisation of 
	
	
	
	of the MEWP at all times and familiar
	
	
	

	
	Operator
	
	
	
	with the emergency lowering procedure.
	
	
	

	
	Malfunction at Height
	3
	3
	9
	Daily checks to be completed prior to use.
	1
	3
	3

	
	Falling Objects, Tools or
	2
	3
	6
	Operatives on the ground to be aware
	2
	1
	2

	
	Materials
	
	
	
	of operatives working at height, banksman to manage the area. Tools / equipment used at height to be carried in toolbelt and toe guard to be present on MEWP platform.
	
	
	

	
	Slips, Trips and Falls on
	4
	3
	12
	MEWP operator to ensure the platform
	1
	3
	3

	
	Platform
	
	
	
	is clear of debris at all times.
	
	
	

	Auger Cleaning
	Falling Materials
	2
	3
	6
	Mechanical auger cleaning devices to be activated during withdrawal phase to prevent loose spoil rising above head height.
	1
	1
	1

	NOTE - in certain circumstances, typically stiff / very stiff clay , the mechanical auger cleaning device may not clear all spoil from the auger. In this event, the spoil is to be loosened manually, either by an operative working at ground level using an appropriate tool or working on the rig ladder, wearing a full harness 
attached to the fall-arrest system.                                                               
In either event, the auger must NOT be rotated during manual cleaning.

	Concrete Ground-Line
	Concrete Spraying into
	2
	3
	6
	Concrete ground-line and rig hoses to
	2
	2
	4

	and Rig Hoses
	Eyes
	
	
	
	be inspected regularly by a competent person (piling Forman or supervisor) for broken & exposed braiding. Damaged lines to be clearly identified and taken out of service.
Bolted pipe connectors to be checked for tightness regularly.
Whip-checks to be secured and quickrelease couplers to have R-clips fitted.
Avoid trafficking hoses.
USE CROSSING POINTS.
	
	
	

	Drop Hose on Rig 
	Falling Objects/Materials
	2
	3
	6
	Banksman on the ground to be aware
	2
	1
	2

	Snagging
	Damage to Property
	
	
	
	of pumping operations and to watch concrete hose relative to rig structure. Rig operator to observe Banksman's' directions.
	
	
	


Degree of Risk = Likelihood          5 = Almost Certain,   4 = Very Likely,   3 = Likely,   2 = Unlikely,   1 = Very Unlikely
Severity          5 = Fatality,   4 = Specified Injury,   3 = 7 Day Injury,   2 = Minor Injury,   1 = No Injury Risk = Likelihood x Severity
Residual Risk not to be greater than 4
	ACTIVITY
	RISKS
	Degree of Risk
	CONTROL PROCEDURES
	Residual Risk

	
	
	L
	S
	R
	
	L
	S
	R

	Cleaning Out Hoses
	Grout Splashing / Stone Chippings
Persons Being Struck by
Hose
	3
2
	3
3
	9
6
	When blowing-out, always use boards or a blow-out bucket to contain the wash-out and loose aggregate.
Always restrain the end of the landline either by placing a digger bucket on it or leaving it connected to the rig.
	1
1
	1
1
	1
1

	Welding
	Electrocution
Arc eye 
Burns / Fire
	4
4
4
	4
4
4
	16
16
16
	Welders competent and trained in the use of equipment. All equipment checked and in good working order.
Correct PPE worn by welder. Welding screens erected to prevent risk to members of the public and other operatives.
Hot works permit to be issued by PC. Fire extinguishers located close by. Welders competent and issued with correct PPE.
	1
1
1
	4
4
4
	4
4
4

	
	
	
	RI
	SK
	

	Likelihood
	
	
	
	

	1
	5
	4
	3
	2
	

	2
	10
	8
	6
	4
	

	3
	15
	12
	9
	6
	

	4
	20
	16
	12
	8
	

	5
	25
	20
	15
	10
	

	
	5
	4
	3
	2
	

	
	
	
	Consequence
	

	N.B. AREAS HIGHLIGHTED IN RED ARE AN UNACCEPTABLE RISK LEVEL

	AREAS HIGHLIGHTED IN BLUE ARE ACCEPTABLE RISK LEVELS

	
	Likelihood
Almost Certain
	5

	Very Likely
	4

	Likely
	3

	Unlikely
	2

	Very Unlikely
	1



	
	Severity
Fatality
Specified Injury
7 Day Injury
Minor Injury
No Injury






	1
3
2
1
5
4

5
4
3
2
1


Degree of Risk = Likelihood          5 = Almost Certain,   4 = Very Likely,   3 = Likely,   2 = Unlikely,   1 = Very Unlikely
Severity          5 = Fatality,   4 = Specified Injury,   3 = 7 Day Injury,   2 = Minor Injury,   1 = No Injury Risk = Likelihood x Severity
Residual Risk not to be greater than 4
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