	RISK ASSESSMENT
	No:   009

	Project: Riverside Health & Wellbeing Centre
	PAGE NO: 1 of 1

	COMPLETED BY:  Anthony Lloyd
	DATE: 15.04.24
	REVIEW: 

	Personnel Involved:

Personnel in the immediate location.
	PPE: All personnel will wear hard hats, safety footwear, high visibility jackets/vest, gloves and eye protection.
	SUPERVISOR IN CHARGE: 
C Keys

	Operation: Steel Fixing 

	ACTIVITY AND HAZARDS

(Identify hazards associated with task)
	INITIAL RISK RATING
	CONTROL MEASURES

(Identify measures to eliminate, reduce or control hazard or those that are requested by others)
	RESIDUAL RISK RATING
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	Entanglement with reinforcement and tying wire.

Tripping and falling whilst fixing rebar.

Manual handling of the material (back injuries)

Cutting steel with disc cutter (eye injuries).
Lifting of retaining walls 
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	Keep work area free from loose wire and debris.

Unload reinforcement as close to work area as practical.

Keep work area free from loose wire and debris.

Split bundles/packs to reduce weight to be carried by operatives.

Pre fabrication to be in designated work area where possible.
T,I,L,E,

Task, Induvial, Load, Environment, should all be took into account before any lifting 

Gloves to be worn when carrying reinforcement.

Split bundles/packs to reduce weight to be carried by operatives.

Were possible heavy lifts will be by means of forklift / JCB or tracked excavator to reduce manual handling.

All lifting will be controlled by a banks man. 

Eye and ear protection to be worn when using disc cutters.

Abrasive wheels to be changed by trained operatives.

Lifting of wall should be carried out with the means of forklift/ JCB or tracked 
Excavator while using a lifting beam and under a control of a banksman 
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All persons undertaking activities indicated on this risk assessment form must be made fully aware of its contents
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