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This is an individual practical lab-test, held under examination conditions. You will be assigned three Switches and two Routers; you should configure these devices based on the given specifications. 

This paper is marked out of 100.
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ISP
	Interface
	IP Address  
	CIDR

	Loopback 10
	209.165.201.253
	/24

	G0/0
	PPPoE Enabled Global Group
	-

	G0/1
	Last Available Address (Refer to Topology)
	/26

	Virtual Template 1
	80.0.0.1
	/30

	S0/0/0
	First Available Address (Refer to Topology)
	/30

	s0/0/1
	First Available Address (Refer to Topology)
	/30


Cardiff
	Interface
	IP Address
	CIDR

	G0/0
	PPPoE Enabled – Dialer Pool 1
	-

	Dialer 1
	IP Address Negotiated – Last Available PPPoE Pool
	-

	Tunnel 10
	First Available Address (Refer to Topology)
	/29

	S0/0/0
	Last Available Address (Refer to Topology)
	/30


Swansea
	Interface
	IP Address
	CIDR

	G0/1
	Last Available Address (Refer to Topology)
	/26

	Tunnel 10
	Fifth Available Address (Refer to Topology)
	/29

	S0/0/1
	Last Available Address (Refer to Topology)
	/30


PC-A
	Interface
	IP Address
	Default Gateway 
	DNS Server

	NIC
	DHCP
	DHCP
	8.8.8.8


PC-B
	Interface
	IP Address
	Default Gateway 
	DNS Server

	NIC
	DHCP
	DHCP
	8.8.8.8



Task 1: - Topology Creation (5 marks)
Using Packet Tracer software create the topology shown above and complete all tasks below. 
Task 2: - Basic Device Configuration (10 marks)
1. Cable a network as per the topology diagram. 
2. Configure all devices with IP address shown in the above tables and network topology.
3. Configure hostnames on each device.
4. Disable DNS lookup on all routers.
5. Configure domain name on all routers = wanexam2020.com
6. Secure privilege executive login with level 5 encrypted password = class
7. Create local database of username and encrypted level 5 password for all routers; Username = admin Password = cisco
8. Secure all router console lines with local authentication and enable synchronous logging.
9. Secure all router virtual terminal lines with local authentication and disable telnet.  
10.  After enabling SSH; create cryptographic keys with 1024 bit modules.
  
Task 3: - Cardiff and Swansea DHCP configurations (8 marks)
1. Configure a DHCP pool on Cardiff router so PC-A receives its IP Address, Default Gateway and DNS Server configurations from the DHCP server. (4 Marks)
2. Configure a DHCP pool on Swansea router so PC-B receives its IP Address, Default Gateway and DNS Server configurations from the DHCP server. (4 Marks)
Note: Refer to Network Topology and IP Address table for IP addressing and DNS address.

Task 4: - Configure Exterior Gateway Routing with BGP (25 Marks)
1. Create a BGP instance on all routers utilizing the Autonomous System Numbers (ASN) that has been given within the network topology.
2. Configure all routers with the network statements pertaining to each of their interface subnet addresses.
3. Configure BGP neighbor addresses for each router where appropriate.

4. Configure a default static route on ISP router with Lo10 as outgoing interface.

5.  Redistribute the default route within BGP process by adding the network statement: network 0.0.0.0 to the ISP BGP process.
 
6. Verify all routes are on routing table. 


[bookmark: _GoBack]Task: 5 - Point to Point Protocol (PPP) (7 Marks)

1. Configure all serial links to utilize PPP encapsulation

2. Configure Challenge Handshake Authentication Protocol (CHAP) on all routers using the password = wanexam2020


Task: 6 - Generic Routing Encapsulation (GRE) Tunnel (10 Marks)

1. Configure a GRE tunnel link between Cardiff and Swansea routers using the IP address given within the IP table for the tunnel addresses. Use tunnel 10 as the GRE interface.

2. Use the serial interfaces as the source for each tunnel respectively.

3. Use the serial link IP address  for the destination of the tunnel on Cardiff and Swansea routers.

4. Use default tunnel mode for encapsulation.

Task: 7 - Network Address Translation (NAT) (5 Marks)

1. Allow PC-A and PC-B subnet to utilize PAT.

2. Configure Port Address Translation  (PAT) on the ISP router using the Loopback 10 interface as the translated address.

3. Configure NAT on the correct interfaces on the ISP router to start the NAT process. 
Task: 8 - Test connectivity Pre ACL				              	(15 marks)
From PC-A, ping PC-B and AWS Cloud Server and vice versa. Is it successful? ____________ 
From any PC - B, ping Cardiff router tunnel 10 IP address. Is it Successful? ______________

Task: 9 - Access Control Lists (ACL) (15 Marks)
Create an ACL to only allow the PC-B subnet to remote SSH into the Cardiff router. ( 3 Marks)
Create an ACL to prevent PC-B from ‘Pinging’ the AWS server and also prevent PC-B from using HTTP and DNS protocols within the AWS server.  (7 Marks)
Verify only PC-B is able to SSH to Cardiff router. Try SSH from PC-B and PC-A, screenshot the output here. (5 Marks)


Submission Requirement 
The packet tracer file should be saved as “studentname_id” and uploaded on Moodle. In addition to packet tracer file, you must also submit 

· the output of show running-configuration command in a text file for all devices configured. 
· This document with task 8 and task 9 completed 

All documentation for your solution should be submitted electronically on Moodle.
It is your responsibility that you submit all the outputs and files correctly.


2019/20                                                                                                                        Page 7 of 7

image1.jpeg
Prifysgol Cymru

Y Drindod Dewi Sant
University of Wales
Trinity Saint David





image2.png
Loopback - 10 = AWS Cloud Server
209.165.201.253/24

10.0.1.224/30

9011‘ ‘9011

| =~

PC-A PC-B

172.16.198.0/26 172.16.200.0/26

192.168.10.0/29





