Micros Assignment 


· 2 Capacitors - 22nF – Capacitors have many applications. Its primary use is energy storage – This means that capacitors have the capability have the ability to store energy and dissipate it throughout the circuit when required.  In addition, capacitors are used to block DC current while allowing AC current to flow through.    
· 7 Resistors – 220Ohms – Resistors are a two pinned component which are essential in the world of electronics. They provide resistance (Ω). In addition, they have the capability to lower the flow of current, divide voltages & block transmission signals. 
· 2 Resistors – 10kOhms
· 1 crystal oscillator – 4 Mhz Frequency – Arguably the most complex component in the circuit, an oscillator is implemented in many day-to-day electronic devices. An oscillator essentially converts DC signals to periodic AC signals then enabling users to set frequency – commonly used in any audio devices. 
· 1 PIC16F84A – The PIC16F84A, has 5 PORTA pins and 8 PORTB pins. One advantage when using this chip is its ability to set all PORTB pins to either Input or Output. This means all 8 pins can either sink or source current which is desirable for those who wish to fine tweak their circuits.
· 2 buttons 
· Power sources 
· These supplied power to the input pins 
· Ground sources
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	Above is the Common anode Hex value to make the 7-segment display shine a Zero 
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