Task3: Network connectivity (10 marks)

Using ping command, verify end-to-end connectivity:
From PC-1, ping PC-2 & LP-A. Is it successful? 			yes			 

From PC-1 ping default gateway. Is it successful? 			yes				 
Bellow screenshot for both above tasks
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From PC-2, ping 172.16.0.1. Is it successful? 	yes	 
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From PC-1, ping 172.16.0.254. Is it successful? 		yes		
[image: A screenshot of a computer

Description automatically generated]


Verify HSRP is working as expected
Issue the shutdown command on R1 G0/1, and then re-issue the following commands to verify that HSRP is working as expected:
From PC-2, ping 172.16.0.1. Ping should not be successful 	yes	 
From PC-2, ping default gateway. Is it successful? 	yes		  
From PC-2, ping 209.165.200.225. Is it successful? 		yes			
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Pinging 192.168.2.11 with 32 bytes of data:
Reply from 192.168.
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Ping statistics for 192.168.2.11:

Packets: Sent = 4, Received = 4, Lost = 0 (0% loss),
Approximate round trip times in milli-seconds:

Minimum = Oms, Maximum = lms, Average = Oms

C:\>ping 192.168.2.1

Pinging 192.168.2.1 with 32 bytes of data:
Reply from 192.168.
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Ping statistics for 192.168.2.1:

Packets: Sent = 4, Received = 4, Lost = 0 (0% loss),
Approximate round trip times in milli-seconds:

Minimum = Oms, Maximum = lms, Average = Oms
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[Command Prompt

Cisco Packet Tracer PC Command Line 1.0
C:\>ping 192.168.2.1

Pinging 192.168.2.1 with 32 bytes of data:

Request timed out.
Reply from 192.168.2.1: bytes=32 time=38ms TTL=254
Request timed out.
Reply from 192.168.2.1: bytes=32 time=39ms TTL=254

Ping statistics for 192.168.2.1:

Packets: Sent = 4, Received = 2, Lost = 2 (50% loss),
Approximate round trip times in milli-seconds:

Minimum = 38ms, Maximum = 39ms, Average = 38ms
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[Command Prompt

Cisco Packet Tracer PC Command Line 1.0
C:\>ping 172.16.0.1

Pinging 172.16.0.1 with 32 bytes of data:

Reply from 172.16.0.
Reply from 172.16.0.
Reply from 172.16.0.
Reply from 172.16.0.

bytes=32 time=2ms TTL=254
bytes=32 time=1lms TTL=254
bytes=32 time=24ms TTL=254
bytes=32 time=1lms TTL=254
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Ping statistics for 172.16.0.1:

Packets: Sent = 4, Received = 4, Lost = 0 (0% loss),
Approximate round trip times in milli-seconds:

Minimum = 1lms, Maximum = 24ms, Average = 7ms

C:\>
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Pinging 192.168.2.1 with 32 bytes of data:

Reply from 192.168.
Reply from 192.168.
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Ping statistics for 192.168.2.1:

Packets: Sent = 4, Received = 4, Lost = 0 (0% loss),
Approximate round trip times in milli-seconds:

Minimum = Oms, Maximum = lms, Average = Oms

C:\>ping 172.16.0.254
Pinging 172.16.0.254 with 32 bytes of data:

Request timed out.
Request timed out.
Reply from 172.16.0.254: bytes=32 time=13ms TTL=126
Reply from 172.16.0.254: bytes=32 time=1lms TTL=126

Ping statistics for 172.16.0.254:

Packets: Sent = 4, Received = 2, Lost = 2 (50% loss),
Approximate round trip times in milli-seconds:

Minimum = 1lms, Maximum = 13ms, Average = 7ms




