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	Activity being assessed: 
	  General site hazards                                   
	 
	
	Date: 
	April 2024 

	Location: 
	Bethany Square Car Park, Bethany Square, 87 Station Rd, Port Talbot SA13 1PQ
	Prepared by: 
	Elliott Lewis 
	
	 

	People at risk: 
	Employees ☒            Other contractors ☒               Site visitors ☒                  Others ☐ _______________________ 

	PPE Required: 
	 
[image: ][image: A blue circle with a white shirt

Description automatically generated][image: A blue circle with a white outline of a person's face

Description automatically generated][image: A blue circle with white headphones on it

Description automatically generated][image: A blue circle with white boots

Description automatically generated][image: A blue circle with white gloves

Description automatically generated][image: A blue circle with a white line on it with a face mask

Description automatically generated]	☒        	☒                         ☒                            ☐              ☐        	☐       	☐     
	[image: A blue circle with a white exclamation mark

Description automatically generated]

	 

	Hazard 
	Potential Harm 
	P 
	S 
	RR 
	How to make it safer….. 
	P 
	S 
	RRR 

	· Slips 
· Trips  - 	Falls 
 
	Injury to self and others if not suitably trained and unfamiliar with the site and control measures in place 
	4 
	4 
	16 
	a) All staff will be receiving a site specific induction by the site     manager and follow all project manager safety rules.    
b) All work will be carried out by trained and competent      staff, holding CSCS cards.
c) All staff will be appropriately dressed for with PPE,      including safety boots, long trouser, hard hats and high      visibility tabards, which must be worn at all times.         
d) Staff will liaise with site manager and other contractors on a      daily basis to ensure works across site are on schedule to      avoid activities clashing, increasing risk on site 
e) Apprentices will be supervised by an experienced member of  staff.                                   
f) Hand and power tools will not be left unattended. 
g) The site will be made safe at the end of each shift with tools     and materials securely stored to deter theft and accidents to     others. 


	2 
	2 
	4 

	Probability (P) 
	Severity (S) 
	Risk Rating (RR): Probability X Severity (PXS) 

	1. Improbable 
	1. No risk of injury or disease 
	  Residual Risk 
	Action 

	2. Remote 
	2. Minor injury 
	1-6 LOW 
	Reduce risk wherever possible. 

	3. Possible 
	3. RIDDOR > 3 day off work 
	7-14 MEDIUM 
	Only proceed with management authorisation 

	4. Probable 
	4. RIDDOR major injury 
	
	Consult with assessment personnel, re-define and reduce risk. 

	5. Likely 
	5. One or more fatalities 
	15–25   HIGH 
	Do NOT proceed.  Re-define, re-assess and reduce risk.   



	Activity being assessed: 
	Use of cartridge operated tools 
	
	 
	Date: 
	April 2024 

	Location: 
	Bethany Square Car Park, Bethany Square, 87 Station Rd, Port Talbot SA13 1PQ
	Prepared by: 
	Elliott Lewis 
	
	

	People at risk: 
	Employees ☒            Other contractors ☒               Site visitors ☐                  Others ☐ _______________________ 

	Hazard 
	Potential Harm 
	P 
	S 
	RR 
	How to make it safer….. 
	P 
	S 
	RRR 

	Wrong power setting for type of fixing and type of material. 
 
Soft material is punctured by nail/fastener when misfired. 
 
Use of incorrect cartridge/misfire. 
 
Ricochet of fastener or fixing device. 
 
Negligent discharge of projectile. 
 
Fragmentation of brittle materials during firing. 
 
Recoil throwing operative off balance. 
 
Exposure to noise. 
	Operatives and others sustaining 
fatal or severe puncture injuries 
 
Lacerations to eyes and exposed skin 
 
Serious injury or even fatal injury could occur if a worker falls. 
 
Hearing loss  
Tinnitus 
	4 
	4 
	16
	a) Operatives must be trained and competent, certificated and       authorised to use the cartridge tool - a record will be kept of      those authorised. 
b) Operatives shall wear impact eye protection and head      protection during loading, use and unloading. 
c) As cartridges are colour coded no person with defective      colour vision may operate the tool. 
d) Prior to work, test fixings shall be carried out especially in      concrete and masonry. 
f) Cartridge operated tools will be held firmly and flush with the     surface and fired at an angle of 90°. 
g) Brittle surfaces will be covered. 
h) Any new fixing must be 50mm away from an existing hole. 
l) Only fixing devices designed for use with the tool shall be     used. 
m) Guards to be in place and of sufficient size to check flying        pins and debris 
n) Other persons shall be cleared from the danger area. 
o) Tool to be unloaded and made safe when not in use, and      stored in a coal dry place. 
p) Tools and cartridges shall be held under lock and key in secure containers when not in use and issues suitably     controlled. 
q) Any unfired or misfired cartridges should be handed to the     site supervisor for safe disposal 
r) Cartridge operated tools will only be used from stable      position on secure and safe platforms. 

	2 
	3 
	6 

	Probability (P) 
	Severity (S) 
	Risk Rating (RR): Probability X Severity (PXS) 

	1. Improbable 
	1. No risk of injury or disease 
	  Residual Risk 
	Action 

	2. Remote 
	2. Minor injury 
	1-6 LOW 
	Reduce risk wherever possible. 

	3. Possible 
	3. RIDDOR > 3 day off work 
	7-14 MEDIUM 
	Only proceed with management authorisation 

	4. Probable 
	4. RIDDOR major injury 
	
	Consult with assessment personnel, re-define and reduce risk. 

	5. Likely 
	5. One or more fatalities 
	15–25   HIGH 
	Do NOT proceed.  Re-define, re-assess and reduce risk.   



	Activity being assessed: 
	  Use of nailing tool – Pneumatic/Gas 
	
	 
	Date: 
	April 2024 

	Location: 
	Bethany Square Car Park, Bethany Square, 87 Station Rd, Port Talbot SA13 1PQ
	Prepared by: 
	Elliott Lewis
	 
	 

	People at risk: 
	Employees ☒            Other contractors ☒               Site visitors ☒                  Others ☐ _______________________ 

	Hazard 
	Potential Harm 
	P 
	S 
	RR 
	How to make it safer….. 
	P 
	S 
	RRR 

	Puncture/piercing injury 
 
Misuse 
 
Injury to eyes 
 
Falls from height 
 
Malfunction 
 
Exposure to noise 
	Severe lacerations injuries to exposed eyes and skin Loss of sight 
Hearing loss/tinnitus 
Serious injury or death if worker falls. 
 
	4 
	4 
	16 
	a) The operator shall be competent, with certification to ensure      they have been fully instructed, in accordance with the      maker's recommendations, in the safe operation of the tool      and the safety precautions to be observed. 
b) Operators shall be authorised. 
c) Only to be used in accordance with makers instructions      
c) Tool shall be unloaded and made safe when not in use. 
d) The operator shall wear suitable eye protection during      loading, use and unloading. 
e) Operator and other persons affected shall wear suitable ear     protection. 
f) Nailing tools will only be used from stable position on secure      and safe platforms. 
g) Before driving fasteners, check that no one is present     immediately behind or below the working surface. 
h) Spent gas canisters shall be disposed of in a safe manner,  
    i.e. given to the site supervisor for safe disposal. 
 
	2 
	3 
	6 

	Probability (P) 
	Severity (S) 
	Risk Rating (RR): Probability X Severity (PXS) 

	1. Improbable 
	1. No risk of injury or disease 
	  Residual Risk 
	Action 

	2. Remote 
	2. Minor injury 
	1-6 LOW 
	Reduce risk wherever possible. 

	3. Possible 
	3. RIDDOR > 3 day off work 
	7-14 MEDIUM 
	Only proceed with management authorisation 

	4. Probable 
	4. RIDDOR major injury 
	
	Consult with assessment personnel, re-define and reduce risk. 

	Activity being assessed: 
	 Manual Handling 
	Assessment No: 
	
	Date: 
	April 2024 

	Location: 
	Bethany Square Car Park, Bethany Square, 87 Station Rd, Port Talbot SA13 1PQ
	Prepared by: 
	Elliott Lewis 
	Review Date: 
	

	People at risk: 
	Employees ☒            Other contractors ☐               Site visitors ☐                  Others ☐ _______________________ 

	Hazard 
	Potential Harm 
	P 
	S 
	RR 
	How to make it safer….. 
	P 
	S 
	RRR 

	· Heavy loads 
· Awkward shaped loads 
· Unstable contents 
· Loads at low level 
· Loads at high level 
· Sharp edges 
· Excessive distance 
· Obstructions on route 
 
	-Muscular skeletal injury 
 
-Strains 
-Sprains 
-Cuts/abrasions 
-Dropping of load injuring self    and/or others 
 
	3 
	3 
	9 
	a) Loads will be mechanically positioned as close as possible   to its final position. 
b) Lifting aids will be employed where practical. 
c) Staff have received training in safe lifting methods. 
 
 Implement TILE assessment principal: Task - what to where 
Individual(s) - Suitably fit, willing and able 
Load - Heavy, hot awkward or sharp 
Environment - free from obstruction and changes in height, level. 
 
d) Team lifting will be carried out under the direction of a     competent coordinator.  
 
e) Team members will be fully fit and of similar abilities.  
f) Area of lift and route along which it is to be carried must    be cleared of any slip, trip or fall hazards. 
 
	2 
	2 
	4 

	Probability (P) 
	Severity (S) 
	Risk Rating (RR): Probability X Severity (PXS) 

	1. Improbable 
	1. No risk of injury or disease 
	  Residual Risk 
	Action 

	2. Remote 
	2. Minor injury 
	1-6 LOW 
	Reduce risk wherever possible. 

	3. Possible 
	3. RIDDOR > 3 day off work 
	7-14 MEDIUM 
	Only proceed with management authorisation 

	4. Probable 
	4. RIDDOR major injury 
	
	Consult with assessment personnel, re-define and reduce risk. 

	5. Likely 
	5. One or more fatalities 
	15–25   HIGH 
	Do NOT proceed.  Re-define, re-assess and reduce risk.   




	Activity being assessed: 
	  Exposure to noise 
	Assessment No: 
	
	Date: 
	09/02/2024 

	Location: 
	Bethany Square Car Park, Bethany Square, 87 Station Rd, Port Talbot SA13 1PQ
	Prepared by: 
	Elliott Lewis 
	Review Date: 
	08/02/2025 

	People at risk: 
	Employees ☒            Other contractors ☒               Site visitors ☐                  Others ☐ _______________________ 

	Hazard 
	Potential Harm 
	P 
	S 
	RR 
	How to make it safer….. 
	P 
	S 
	RRR 

	 
1) Noise levels between  
    80 – 85dB 
 
2) Noise levels between     85 - 90dB 
 
	 
Hearing loss, tinnitus. 
 
	3 
	3 
	9 
	 
a) Low noise tools have been selected where possible and      appropriate 
b) Consideration will be given to the selection of appropriate     tools, and quieter methods of working selected where     appropriate (residential/built up areas) 
c) If noise exposure is between 80 - 85dB, personnel will be      provided with hearing protectors if requested. 
d) For noise exposure between 85 - 90dB, provide personnel      with hearing protectors and ensure their proper use. 
e) Areas where the use of hearing protection is compulsory,     will be identified and mark them with suitable signage. 
f) Provide personnel with training and information on how to     use and care for the hearing protectors. 
g) Make sure the protectors give enough protection - Select a       protector with an SNR of: 
· 85-90:  20 or less 
· 90-95:  20-30 
· 95-100:  25-35 
· 100-105:  30 or more.  
Aim at least to get below 85 dB at the ear. 
h) Make sure the protectors are compatible when worn with other protective equipment (e.g. hard hats, dust masks and eye protection). 
	1 
	1 
	2 


 
	Probability (P) 
	Severity (S) 
	Risk Rating (RR): Probability X Severity (PXS) 

	1. Improbable 
	1. No risk of injury or disease 
	  Residual Risk 
	Action 

	2. Remote 
	2. Minor injury 
	1-6 LOW 
	Reduce risk wherever possible. 

	3. Possible 
	3. RIDDOR > 3 day off work 
	7-14 MEDIUM 
	Only proceed with management authorisation 

	4. Probable 
	4. RIDDOR major injury 
	
	Consult with assessment personnel, re-define and reduce risk. 

	5. Likely 
	5. One or more fatalities 
	15–25   HIGH 
	Do NOT proceed.  Re-define, re-assess and reduce risk.   



	Activity being assessed: 
	   Use of hand tools 
	
	 
	Date: 
	April 2024

	Location: 
	Bethany Square Car Park, Bethany Square, 87 Station Rd, Port Talbot SA13 1PQ
	Prepared by: 
	Elliott Lewis 
	
	 

	People at risk: 
	Employees ☒            Other contractors ☒               Site visitors ☐                  Others ☐ _______________________ 

	Hazard 
	Potential Harm 
	P 
	S 
	RR 
	How to make it safer….. 
	P 
	S 
	RRR 

	 
Inappropriate application causing injury to self or others 
 
 
Damage to tools and/or works being undertaken 
 
 
 
 
	 
· Eye injuries caused by flying 
  Particles 
 
· Injury from contact with   tool or workpiece (bruising,   crushing, cuts, etc) 
 
· Strains and sprains from   incorrect use 
 
· Injury caused by tripping over   tools (due to poor housekeeping) 
	 
	 
	 
	 
a) Tools must not be used for anything other than intended      purpose. do not use a screwdriver as a chisel. 
b) Staff to carry out visual checks each day before use, and       remove and report any damaged tools. 
c) Eye protection must be worn when using tools (i.e.     chisels, hand saw) where there is a risk of flying     particles. 
d) Open-bladed knives, screwdrivers and other sharp tools     must not be carried in pockets or in a manner which     could cause injury to self for other. 
e) When using Knife: cut away from the body, secure the      piece and wear approved gloves to present lacerations. 
f) Sharpening is a skilled task and must only be caried out by     trained and authorised persons. 
g) Tools must not be left lying around, but returned to     storage after use. 
h) Hearing protection must be worn if carrying out       sustained hammering or other noisy tasks. 
	 
	 
	 

	Probability (P) 
	Severity (S) 
	Risk Rating (RR): Probability X Severity (PXS) 

	1. Improbable 
	1. No risk of injury or disease 
	  Residual Risk 
	Action 

	2. Remote 
	2. Minor injury 
	1-6 LOW 
	Reduce risk wherever possible. 

	3. Possible 
	3. RIDDOR > 3 day off work 
	7-14 MEDIUM 
	Only proceed with management authorisation 

	4. Probable 
	4. RIDDOR major injury 
	
	Consult with assessment personnel, re-define and reduce risk. 

	5. Likely 
	5. One or more fatalities 
	15–25   HIGH 
	Do NOT proceed.  Re-define, re-assess and reduce risk.   


 
	Activity being assessed: 
	   Circular Saw 110v 
	Assessment No: 
	
	Date: 
	09/02/2024 

	Location: 
	Bethany Square Car Park, Bethany Square, 87 Station Rd, Port Talbot SA13 1PQ
	Prepared by: 
	Elliott Lewis 
	Review Date: 
	08/02/2025 

	People at risk: 
	Employees ☒            Other contractors ☒               Site visitors ☐                  Others ☐ _______________________ 

	Hazard 
	Potential Harm 
	P 
	S 
	RR 
	How to make it safer….. 
	P 
	S 
	RRR 

	Wood Dust 
 
Noise 
 
Poorly maintained equipment 
 
 
	Eye injury from wood dust or splinter 
Personal injury - 
laceration/amputation from saw blade 
Electric shock (110 volt), personal injury, burns 
II-health from inhalation of wood dust (soft wood) 
Noise induced hearing loss 
II-health from effect of vibration 
(Hand/Arm Vibration (HAY) 
	 
	 
	 
	a) Eye protection recommended to be worn. 
 
b) Equipment to be maintained in good working order, with all      fitted guards being operational (spring loaded and self       returning). 
 
c) Hands/arms and loose clothing to be kept clear of working      area. 
d) Daily inspection required by user prior to use. 
 
e) Where possible, equipment should be used externally to allow dust to disperse. 
 
f) Disposable respirator should be worn if used in an enclosed space or if dust is excessive. 
 
g) Hearing protection must be worn if noise levels are in excess of85 dB(A). 
 
h) Timber being cut should be adequately supported.
	 
	 
	 

	Probability (P) 
	Severity (S) 
	Risk Rating (RR): Probability X Severity (PXS) 

	1. Improbable 
	1. No risk of injury or disease 
	  Residual Risk 
	Action 

	2. Remote 
	2. Minor injury 
	1-6 LOW 
	Reduce risk wherever possible. 

	3. Possible 
	3. RIDDOR > 3 day off work 
	7-14 MEDIUM 
	Only proceed with management authorisation 

	4. Probable 
	4. RIDDOR major injury 
	
	Consult with assessment personnel, re-define and reduce risk. 

	5. Likely 
	5. One or more fatalities 
	15–25   HIGH 
	Do NOT proceed.  Re-define, re-assess and reduce risk.   




	Activity being assessed: 
	  Young Persons 
	
	 
	Date: 
	09/02/2024 

	Location: 
	Bethany Square Car Park, Bethany Square, 87 Station Rd, Port Talbot SA13 1PQ
	Prepared by: 
	Elliott Lewis 
	Review Date: 
	08/02/2025 

	People at risk: 
	Employees ☒            Other contractors ☒               Site visitors ☐                  Others ☐ _______________________ 

	Hazard 
	Potential Harm 
	P 
	S 
	RR 
	How to make it safer….. 
	P 
	S 
	RRR 

	Inexperienced 
 
Overly confident 
 
 

	Minor, major or fatal injuries from lack of experience and understanding of the workplace. 





















	 
	 













	
	
a) Young persons shall receive specific site induction training. 
b) Consideration of the work to be carried out, and the 
     subject's capability to do so, will cover the following points: - 
· Their inexperience, lack of awareness of risks, and        maturity. 
· Their place of work will be assessed to ensure it is safe          and the young person shall be advised to leave area if         they feel it has become unsafe and report this to their          supervisor. 
c) The use of work equipment will be controlled - they will be     trained to ensure they are aware of the safe working     practices and the dangers posed by the equipment. 
d) Young persons shall be prevented from using work      equipment or plant which is high risk, i.e. equipment     producing high levels of noise and/or vibration;        (assess all plant and work equipment prior to work). 
e) Young person's work activities shall be organised to ensure     they are not put in unsafe or unfamiliar situations. 
f) Young persons shall be prevented from using, or exposed to      substances hazardous to health. 
g) A competent person shall supervise young persons. 
h) Supervisors shall monitor regularly the extent of the health      and safe training provided. 


	 
	 
	 

	Probability (P) 
	Severity (S) 
	Risk Rating (RR): Probability X Severity (PXS) 

	1. Improbable 
	1. No risk of injury or disease 
	  Residual Risk 
	Action 

	2. Remote 
	2. Minor injury 
	1-6 LOW 
	Reduce risk wherever possible. 

	3. Possible 
	3. RIDDOR > 3 day off work 
	7-14 MEDIUM 
	Only proceed with management authorisation 

	4. Probable 
	4. RIDDOR major injury 
	
	Consult with assessment personnel, re-define and reduce risk. 

	5. Likely 
	5. One or more fatalities 
	15–25   HIGH 
	Do NOT proceed.  Re-define, re-assess and reduce risk.   


 
 
 
 
















































	Activity being assessed: 
	   Crane lifting operations 
	Assessment No: 
	
	Date: 
	09/02/2024 

	Location: 
	Bethany Square Car Park, Bethany Square, 87 Station Rd, Port Talbot SA13 1PQ
	Prepared by: 
	Elliott Lewis 
	Review Date: 
	08/02/2025 

	People at risk: 
	Employees ☒            Other contractors ☐               Site visitors ☐                  Others ☐ _______________________ 

	Hazard 
	Potential Harm 
	P 
	S 
	RR 
	How to make it safer….. 
	P 
	S 
	RRR 

	Machine over-turning 
 
 
Materials or equipment during lifting operation 
 
 
Failure of lifting gear or equipment 
 
 
 
	Operatives and others sustaining fatal or severe crush injuries Death or loss of limbs 
Operatives and persons nearby suffering serious or fatal burns 
 
Severe injury or death by electric shock 

	
	4 



























	16 
	a) Craning operations will be organised and controlled by an     'Appointed Person', and will be carried out in accordance      with the Lifting Operations and Lifting Equipment Regulations     (LOLER) and BS 7121- a Lifting Plan will be prepared. 
b) The Appointed Person will be responsible to ensure that       inspections and maintenance of all lifting gear has been       carried out. 
c) The crane operator will be trained and competent, and be      responsible for safe operation, daily maintenance and      completion of records relating to the crane and lifting gear. 
d) Slingers/signallers will be adequately trained and competent,      able to communicate clearly and be aware of their duties –      certificates of training will be retained on site. They will be     required to know the weight of materials to be raised before      commencing a lift, and to ensure stability and security of        loads. 
e) The surface from which mobile crane is to operate will be      prepared and checked to ensure stability. 
f) Machinery and accessories used for lifting loads must be    clearly marked with its safe working load (SWL)- this must not    be exceeded.
g) If the crane operator cannot see the load during the whole of      the lifting operation, an additional slinger/signaller or radio     communication will be used. 
Where overhead power lines are likely to cause danger, the      electricity distributor who owns the lines should always be    contacted to calculate the safe working distances - these will depend on voltage, maximum sag and lateral swing (also see    HSEGuidanceNote GS6).


	2 
	2 
















	4 


















	
	
	
	
	
	
	
	
i) A 600mm wide clearance should be provided whenever     practicable belween travelling and slewing cranes and any     fixture (e.g. adjacent buildings, guardrails, access, etc.). If the    clearance is not practicable, then access should be barred    off. 
 
j) Where reasonably practicable, the area covered by the crane    operation should be kept clear of other work operations,     pedestrian access etc. 
 
k) When working over pavements or access ways, the operator     must ensure that no loads are lifted over persons at any time. 
 
         
	
	
	

	Probability (P) 
	Severity (S) 
	Risk Rating (RR): Probability X Severity (PXS) 

	1. Improbable 
	1. No risk of injury or disease 
	  Residual Risk 
	Action 

	2. Remote 
	2. Minor injury 
	1-6 LOW 
	Reduce risk wherever possible. 

	3. Possible 
	3. RIDDOR > 3 day off work 
	7-14 MEDIUM 
	Only proceed with management authorisation 

	4. Probable 
	4. RIDDOR major injury 
	
	Consult with assessment personnel, re-define and reduce risk. 

	5. Likely 
	5. One or more fatalities 
	15–25   HIGH 
	Do NOT proceed.  Re-define, re-assess and reduce risk.   


 
 
 
 
 
 
 
	Activity being assessed: 
	  Extreme Weather conditions 
	Assessment No: 
	
	Date: 
	09/02/2024 

	Location: 
	Bethany Square Car Park, Bethany Square, 87 Station Rd, Port Talbot SA13 1PQ
	Prepared by: 
	Elliott Lewis
	Review Date: 
	08/02/2025 

	People at risk: 
	Employees ☒            Other contractors ☒               Site visitors ☐                  Others ☐ _______________________ 

	Hazard 
	Potential Harm 
	P 
	S 
	RR 
	How to make it safer….. 
	P 
	S 
	RRR 

	Exposure to hot 
temperatures and sunlight 
 
Exposure to excessively cold temperatures 
 
Slippery surfaces 
 
 
 
 
	· Heat exhaustion/sun stroke 
· Sun burn 
 
· Hypothermia 
 
· Increased fatigue 
 
· Slips and strains due to icy conditions 
 
	3 
	3 
	9 
	a) Consideration will be taken when working outdoors/in exposed areas for the current weather conditions. 
b) Where weather warnings have been issued, Alpha Construction will assess the risk to employees in terms of travel to site and working conditions, making alternative arrangements where possible, to ensure staff safety is not compromised. 
c) Alpha Construction staff are provided with uniform including warm high vis trousers and Jackets, cap and hat and waterproofs to help protect against the elements. Staff must select the correct clothing for the conditions. 
d) Welfare facilities providing shade or warmth must be provided by the main contractor. 
e) Frequent breaks may be required in extreme hot or cold conditions. This will be agreed with Alpha Construction  team leader on the day.
	2 
	1 
	2 

	Probability (P) 
	Severity (S) 
	Risk Rating (RR): Probability X Severity (PXS) 

	1. Improbable 
	1. No risk of injury or disease 
	  Residual Risk 
	Action 

	2. Remote 
	2. Minor injury 
	1-6 LOW 
	Reduce risk wherever possible. 

	3. Possible 
	3. RIDDOR > 3 day off work 
	7-14 MEDIUM 
	Only proceed with management authorisation 

	4. Probable 
	4. RIDDOR major injury 
	
	Consult with assessment personnel, re-define and reduce risk. 

	5. Likely 
	5. One or more fatalities 
	15–25   HIGH 
	Do NOT proceed.  Re-define, re-assess and reduce risk.   


 
 	 































	Activity being assessed: 
	  Slinging of loads 
	Assessment No: 
	
	Date: 
	09/02/2024 

	Location: 
	Bethany Square Car Park, Bethany Square, 87 Station Rd, Port Talbot SA13 1PQ
	Prepared by: 
	Elliott Lewis 
	Review Date: 
	08/02/2025 

	People at risk: 
	Employees ☒            Other contractors ☒               Site visitors ☐                  Others ☐ _______________________ 

	Hazard 
	Potential Harm 
	P 
	S 
	RR 
	How to make it safer….. 
	P 
	S 
	RRR 

	Unintentional release of load  
 
Unplanned movement of load  
 
Damage to equipment and load  
 
 
 
	Crush injuries to personnel  
 
Trap injuries - fingers being caught between sling/chain and load 
 
	3 
	4 
	12 
	a) Check certification or lifting equipment and slingers before      allowing work to commence. 
b) When selecting lifting equipment, consideration must be     given to the weight, size, shape and center or gravity of the     load. 
c) All lifting gear should be individually identifiable and stored     so as to prevent damage or deterioration. 
d) The safe working load of the lifting equipment and all lifting      gear must be clearly marked on the item and never      exceeded. 
e) All lifting gear must be visually inspected before each use. 
f) Lifting gear (chains, slings etc.) must be protected from     damage during lifting by the use of packing on sharp edges. 
g) Before fully raising the load, checks must be made to ensure     that it is being lifted evenly and is not likely to swing or sway      when raised. 
h) Tail ropes must be used for larger loads to assist in      maneuvering operations. 
i) No persons are allowed to stand or work within the operating     radius of the lifting appliance without the operators express     permission. 
 
j) Loads must not be transported over persons. 
 
k) A banksman must be used at all times when the operator's      vision is impeded or whilst operating in a congested area. 

	2 
	2 
	4 

	
	
	
	
	
	
	
	l) Work must cease if weather conditions are likely to prevent     safe operations. 
 
j) The area within the arc of the operation must be cleared of    personnel before the load is lifted. 
 
k) No person may be permitted to stand below a suspended      load. 
         
 
	
	
	

	Probability (P) 
	Severity (S) 
	Risk Rating (RR): Probability X Severity (PXS) 

	1. Improbable 
	1. No risk of injury or disease 
	  Residual Risk 
	Action 

	2. Remote 
	2. Minor injury 
	1-6 LOW 
	Reduce risk wherever possible. 

	3. Possible 
	3. RIDDOR > 3 day off work 
	7-14 MEDIUM 
	Only proceed with management authorisation 

	4. Probable 
	4. RIDDOR major injury 
	
	Consult with assessment personnel, re-define and reduce risk. 

	5. Likely 
	5. One or more fatalities 
	15–25   HIGH 
	Do NOT proceed.  Re-define, re-assess and reduce risk.   
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