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Lack of time prevented me from answering question 2 completely. Although local power factor correction has more advantages as the correction unit would be significantly smaller and provide faster response times rather than a centralised unit depending on size of application. Switching current would also be dramatically decreased 
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